Project Name:	NSF
	Project Code:	NSF	Site ID:	VP26	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (VIC)
	Site Information
	Desc. By:	Locality:
	Date Desc.:	//	Elevation:	 140 metres
	Map Ref.:	Rainfall:	590
	Northing/Long.:	146.283333333333	Runoff:	No Data
	Easting/Lat.:	-36.1333333333333	Drainage:	No Data
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	No Data	Pattern Type:	No Data
	Morph. Type:	No Data	Relief:	No Data
	Elem. Type:	No Data	Slope Category:	No Data
	Slope:	0 % 	Aspect:	No Data
	Surface Soil Condition (dry):	N/A
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	 N/A    	Principal Profile Form:	Dr2.22
	ASC Confidence:	Great Soil Group:	Non-calcic brown 
	Confidence level not specified	soil
	Site Disturbance:
	Vegetation:
	Surface Coarse Fragments:
	Profile Morphology
	A	0 - 0.1 m	Reddish brown (5YR4/4-Moist); ; Loam; 
	A2	0.1 - 0.2 m	Yellowish red (5YR4/6-Moist); ; Sandy clay loam; 
	B21	0.2 - 0.4 m	Red (2.5YR4/6-Moist); ; Light clay; 
	B22	0.4 - 1 m	Red (2.5YR4/6-Moist); ; Medium clay; 
	B22	1 - 1.1 m	Red (2.5YR4/6-Moist); ; Medium clay; Few (2 - 10 %), Manganiferous, Medium (2 -6 mm), 
	Nodules; 
	1.1 - 1.4 m	; 
	Morphological Notes
	Observation Notes
	V70/P30                                                                                                                 
	Site Notes
	PEECHELBA EAST

	Project Name:	NSF
	Project Code:	NSF	Site ID:	VP26	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (VIC)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.1	5.8I	 0.11D	 1.9K	 0.36	 0.92	 0.1
	0.1 - 0.2	6.1I	 0.06D	 2.6K	 0.4	 0.52	 0.43
	0.2 - 0.3	6.6I	 0.06D	 4.1K	 1	 0.51	 0.25
	0.3 - 0.4	6.8I	 0.06D	 5.3K	 1.6	 0.53	 0.1
	0.4 - 0.5	6.8I	 0.06D	 5.9K	 2.3	 0.69	 0.22
	0.5 - 0.6	6.9I	 5.7K	 2.7	 0.84	 0.18
	0.6 - 0.7	7.1I	 5.2K	 3	 0.9	 0.25
	0.7 - 0.8	7.2I	 4.9K	 3	 0.9	 0.07
	0.8 - 0.9	7.1I	 4.8K	 3.2	 0.8	 0.9
	0.9 - 1	7.2I	 4.8K	 3.5	 0.88	 0.19
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.1	 0.99A	 10.3A
	0.1 - 0.2	 0.41A	 2.9A
	0.2 - 0.3	 0.3A	 2.5A
	0.3 - 0.4	 0.29A	 2.5A
	0.4 - 0.5	 0.24A	 2.9A
	0.5 - 0.6	 0.23A	 4.2A
	0.6 - 0.7	 0.17A	 4.5A
	0.7 - 0.8	 0.15A	 4.4A
	0.8 - 0.9	 0.19A	 3.9A
	0.9 - 1	 0.2A	 3.4A
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.1
	0.1 - 0.2
	0.2 - 0.3
	0.3 - 0.4
	0.4 - 0.5
	0.5 - 0.6
	0.6 - 0.7
	0.7 - 0.8
	0.8 - 0.9
	0.9 - 1

	Project Name:	NSF
	Project Code:	NSF	Site ID:	VP26	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (VIC)
	Laboratory Analyses Completed for this profile
	15_NR_CA	Exch. basic cations (Ca++) - meq per 100g of soil - Not recorded
	15_NR_K	Exch. basic cations (K++) - meq per 100g of soil - Not recorded
	15_NR_MG	Exch. basic cations (Mg++) - meq per 100g of soil - Not recorded
	15_NR_NA	Exch. basic cations (Na++) - meq per 100g of soil - Not recorded
	3_C_B	Electrical conductivity or soluble salts - Total soluble salts %
	4A_C_2.5	pH of soil - pH of 1:2.5 soil/water suspension
	5_C_B	Water soluble Chloride - Method recorded as B
	6A1	Organic carbon - Walkley and Black
	9B_9C	Available P (mg/kg) - Bicarbonate P - 0.5M NaHCO3 extractable