Project Name:	NSF
	Project Code:	NSF	Site ID:	VP50	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (VIC)
	Site Information
	Desc. By:	Locality:
	Date Desc.:	//	Elevation:	 166 metres
	Map Ref.:	Rainfall:	598
	Northing/Long.:	146.583333333333	Runoff:	No Data
	Easting/Lat.:	-36.0833333333334	Drainage:	No Data
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	No Data	Pattern Type:	No Data
	Morph. Type:	No Data	Relief:	No Data
	Elem. Type:	No Data	Slope Category:	No Data
	Slope:	0 % 	Aspect:	No Data
	Surface Soil Condition (dry):	N/A
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	 N/A    	Principal Profile Form:	Dy3.42
	ASC Confidence:	Great Soil Group:	Soloth
	Confidence level not specified
	Site Disturbance:
	Vegetation:
	Surface Coarse Fragments:
	Profile Morphology
	A	0 - 0.1 m	Brown (7.5YR4/4-Moist); ; Sandy clay loam; Massive grade of structure; 
	A2cb	0.1 - 0.3 m	Brown (7.5YR5/4-Moist); ; Sandy clay loam; Massive grade of structure; Few (2 - 10 %), 
	Ferruginous, Medium (2 -6 mm), ; 
	B21	0.3 - 0.6 m	Brownish yellow (10YR6/6-Moist); , 2.5YR46; Light clay; Moderate grade of structure; 
	B22	0.6 - 1 m	Yellow (2.5Y7/6-Moist); , 2.5YR46; Medium clay; Moderate grade of structure; 
	B22	1 - 1.1 m	Yellow (2.5Y7/6-Moist); , 2.5YR46; Medium clay; Moderate grade of structure; 
	1.1 - 1.4 m	; 
	Morphological Notes
	Observation Notes
	VP71/P28                                                                                                                
	Site Notes
	RUTHERGLEN R.S

	Project Name:	NSF
	Project Code:	NSF	Site ID:	VP50	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (VIC)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.1	5.2I	 0.19D	 3.8K	 0.88	 0.63	 0.1
	0.1 - 0.2	5.8I	 4.2K	 1.1	 0.38	 0.08
	0.2 - 0.3	6.3I	 0D	 5.2K	 1.7	 0.31	 0.25
	0.3 - 0.4	6.5I	 0D	 4.9K	 2.6	 0.3	 0.3
	0.4 - 0.5	6.6I	 0.06D	 5.1K	 3	 0.41	 0.44
	0.5 - 0.6	6.5I	 0.12D	 5.4K	 3.9	 0.56	 0.72
	0.6 - 0.7	6.6I	 0.12D	 5.3K	 4.7	 0.69	 0.88
	0.7 - 0.8	6.6I	 0.1D	 5.2K	 5.1	 0.72	 1.1
	0.8 - 0.9	6.8I	 0.1D	 5K	 5.5	 0.7	 1.3
	0.9 - 1	6.9I	 0.06D	 5K	 5.9	 0.67	 1.6
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.1	 1.2A	 14.1A
	0.1 - 0.2	 0.54A	 5.1A
	0.2 - 0.3	 0.39A	 3.2A
	0.3 - 0.4	 0.34A	 3.8A
	0.4 - 0.5	 0.24A	 4.3A
	0.5 - 0.6	 0.27A	 5.5A
	0.6 - 0.7	 0.24A	 6.1A
	0.7 - 0.8	 0.19A	 6A
	0.8 - 0.9	 0.19A	 3.6A
	0.9 - 1	 0.19A	 2.3A
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.1
	0.1 - 0.2
	0.2 - 0.3
	0.3 - 0.4
	0.4 - 0.5
	0.5 - 0.6
	0.6 - 0.7
	0.7 - 0.8
	0.8 - 0.9
	0.9 - 1

	Project Name:	NSF
	Project Code:	NSF	Site ID:	VP50	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (VIC)
	Laboratory Analyses Completed for this profile
	15_NR_CA	Exch. basic cations (Ca++) - meq per 100g of soil - Not recorded
	15_NR_K	Exch. basic cations (K++) - meq per 100g of soil - Not recorded
	15_NR_MG	Exch. basic cations (Mg++) - meq per 100g of soil - Not recorded
	15_NR_NA	Exch. basic cations (Na++) - meq per 100g of soil - Not recorded
	3_C_B	Electrical conductivity or soluble salts - Total soluble salts %
	4A_C_2.5	pH of soil - pH of 1:2.5 soil/water suspension
	5_C_B	Water soluble Chloride - Method recorded as B
	6A1	Organic carbon - Walkley and Black
	9B_9C	Available P (mg/kg) - Bicarbonate P - 0.5M NaHCO3 extractable