Project Name:	NSF
	Project Code:	NSF	Site ID:	VP52	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (VIC)
	Site Information
	Desc. By:	Locality:
	Date Desc.:	//	Elevation:	 166 metres
	Map Ref.:	Rainfall:	598
	Northing/Long.:	146.466666666667	Runoff:	No Data
	Easting/Lat.:	-36.05	Drainage:	No Data
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	No Data	Pattern Type:	No Data
	Morph. Type:	No Data	Relief:	No Data
	Elem. Type:	No Data	Slope Category:	No Data
	Slope:	0 % 	Aspect:	No Data
	Surface Soil Condition (dry):	N/A
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	 N/A    	Principal Profile Form:	Dr2.22
	ASC Confidence:	Great Soil Group:	Non-calcic brown 
	Confidence level not specified	soil
	Site Disturbance:
	Vegetation:
	Surface Coarse Fragments:
	Profile Morphology
	A	0 - 0.2 m	Reddish brown (5YR4/3-Moist); ; Clay loam; Massive grade of structure; Few (2 - 10 %), 
	Manganiferous, Medium (2 -6 mm), ; 
	A2	0.2 - 0.3 m	Yellowish red (5YR4/6-Moist); ; Light clay; Massive grade of structure; Few (2 - 10 %), 
	Manganiferous, Medium (2 -6 mm), ; 
	B1	0.3 - 0.6 m	Reddish yellow (7.5YR6/8-Moist); ; Medium clay; Moderate grade of structure; Few (2 - 10 %), 
	Manganiferous, Medium (2 -6 mm), ; 
	B2	0.6 - 1 m	Light reddish brown (2.5YR7/4-Moist); , 5YR46; Medium clay; Moderate grade of structure; Few 
	(2 - 10 %), Manganiferous, Medium (2 -6 mm), ; 
	B2	1 - 1.1 m	Light reddish brown (2.5YR7/4-Moist); , 5YR46; Medium clay; Moderate grade of structure; Few 
	(2 - 10 %), Manganiferous, Medium (2 -6 mm), ; 
	1.1 - 1.4 m	; 
	Morphological Notes
	Observation Notes
	VP71/P30                                                                                                                
	Site Notes
	RUTHERGLEN

	Project Name:	NSF
	Project Code:	NSF	Site ID:	VP52	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (VIC)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.1	5.4I	 0.22D	 3.7K	 1.2	 1	 0.26
	0.1 - 0.2	5.8I	 3.4K	 1.4	 0.58	 0.16
	0.2 - 0.3	6.6I	 0D	 2.9K	 1.9	 0.4	 0.33
	0.3 - 0.4	6.6I	 0D	 2.9K	 3.2	 0.41	 0.62
	0.4 - 0.5	6.6I	 0.06D	 3.8K	 5.3	 0.58	 1.3
	0.5 - 0.6	6.9I	 0.06D	 3.2K	 5	 0.57	 1.6
	0.6 - 0.7	7.5I	 0.09D	 3.4K	 6	 0.74	 2
	0.7 - 0.8	7.8I	 0.1D	 4.2K	 7	 0.89	 2.5
	0.8 - 0.9	8.2I	 0.11D	 4.2K	 7.2	 0.9	 2.7
	0.9 - 1	8.5I	 0.18D	 4.3K	 7.2	 0.84	 2.7
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.1	 1.4A	 10.5A
	0.1 - 0.2	 0.55A	 4A
	0.2 - 0.3	 0.26A	 2.4A
	0.3 - 0.4	 0.24A	 2.5A
	0.4 - 0.5	 0.2A	 4.2A
	0.5 - 0.6	 0.18A	 4.8A
	0.6 - 0.7	 0.19A	 3A
	0.7 - 0.8	 0.2A	 1.4A
	0.8 - 0.9	 0.11A	 1.1A
	0.9 - 1	 0.16A	 1A
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.1
	0.1 - 0.2
	0.2 - 0.3
	0.3 - 0.4
	0.4 - 0.5
	0.5 - 0.6
	0.6 - 0.7
	0.7 - 0.8
	0.8 - 0.9
	0.9 - 1

	Project Name:	NSF
	Project Code:	NSF	Site ID:	VP52	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (VIC)
	Laboratory Analyses Completed for this profile
	15_NR_CA	Exch. basic cations (Ca++) - meq per 100g of soil - Not recorded
	15_NR_K	Exch. basic cations (K++) - meq per 100g of soil - Not recorded
	15_NR_MG	Exch. basic cations (Mg++) - meq per 100g of soil - Not recorded
	15_NR_NA	Exch. basic cations (Na++) - meq per 100g of soil - Not recorded
	3_C_B	Electrical conductivity or soluble salts - Total soluble salts %
	4A_C_2.5	pH of soil - pH of 1:2.5 soil/water suspension
	5_C_B	Water soluble Chloride - Method recorded as B
	6A1	Organic carbon - Walkley and Black
	9B_9C	Available P (mg/kg) - Bicarbonate P - 0.5M NaHCO3 extractable