Project Name:	NSF
	Project Code:	NSF	Site ID:	VP7	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (VIC)
	Site Information
	Desc. By:	Locality:
	Date Desc.:	//	Elevation:	No Data
	Map Ref.:	Rainfall:	740
	Northing/Long.:	142.416666666667	Runoff:	No Data
	Easting/Lat.:	-38.1	Drainage:	No Data
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	No Data	Pattern Type:	No Data
	Morph. Type:	No Data	Relief:	No Data
	Elem. Type:	No Data	Slope Category:	No Data
	Slope:	0 % 	Aspect:	No Data
	Surface Soil Condition (dry):	N/A
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	 N/A    	Principal Profile Form:	Dy3.61
	ASC Confidence:	Great Soil Group:	Lateritic podzolic 
	Confidence level not specified	soil
	Site Disturbance:
	Vegetation:
	Surface Coarse Fragments:
	Profile Morphology
	A	0 - 0.1 m	Dark reddish brown (5YR3/2-Moist); ; Loam; Massive grade of structure; Few (2 - 10 %), 
	Ferruginous, Medium (2 -6 mm), ; 
	A2	0.1 - 0.2 m	Dark reddish brown (5YR3/4-Moist); ; Loam; Massive grade of structure; Many (20 - 50 %), 
	Ferruginous, Medium (2 -6 mm), ; 
	B2s	0.2 - 0.8 m	Yellowish brown (10YR5/4-Moist); , 2.5YR46; Medium clay; Massive grade of structure; Many (20
	 - 50 %), Ferruginous, Medium (2 -6 mm), ; 
	B2s	0.8 - 0.9 m	Yellowish brown (10YR5/4-Moist); , 2.5YR46; Medium clay; Massive grade of structure; Many (20
	 - 50 %), Ferruginous, Medium (2 -6 mm), ; 
	0.9 - 1.2 m	; 
	Morphological Notes
	Observation Notes
	VP70/P7                                                                                                                 
	Site Notes
	WOOLSTHORPE

	Project Name:	NSF
	Project Code:	NSF	Site ID:	VP7	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (VIC)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.1	5.2I	 0.27D	 3.1K	 1.5	 0.55	 0.5
	0.1 - 0.2	5.8I	 0.11D
	0.2 - 0.3	6.6I	 0.08D
	0.3 - 0.4	6.7I	 0.12D	 4.2K	 5.1	 0.2	 1.1
	0.4 - 0.5	6.5I	 0.13D
	0.5 - 0.6	6.4I	 0.16D
	0.6 - 0.7	6.3I	 0.18D
	0.7 - 0.8	6.2I	 0.18D
	0.8 - 0.9	6.2I	 0.18D
	0.9 - 1	6.2I	 0.18D	 3.4K	 5.8	 0.1	 1.4
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.1	 0.371A	 2C	 23	 20	 32
	0.1 - 0.2	 0.222A
	0.2 - 0.3	 0.121A
	0.3 - 0.4	 8C	 10	 5	 72
	0.4 - 0.5
	0.5 - 0.6	 0.033A
	0.6 - 0.7
	0.7 - 0.8
	0.8 - 0.9
	0.9 - 1	 0.016A	 5C	 13	 8	 70
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.1
	0.1 - 0.2
	0.2 - 0.3
	0.3 - 0.4
	0.4 - 0.5
	0.5 - 0.6
	0.6 - 0.7
	0.7 - 0.8
	0.8 - 0.9
	0.9 - 1

	Project Name:	NSF
	Project Code:	NSF	Site ID:	VP7	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (VIC)
	Laboratory Analyses Completed for this profile
	15_NR_CA	Exch. basic cations (Ca++) - meq per 100g of soil - Not recorded
	15_NR_K	Exch. basic cations (K++) - meq per 100g of soil - Not recorded
	15_NR_MG	Exch. basic cations (Mg++) - meq per 100g of soil - Not recorded
	15_NR_NA	Exch. basic cations (Na++) - meq per 100g of soil - Not recorded
	3_C_B	Electrical conductivity or soluble salts - Total soluble salts %
	4A_C_2.5	pH of soil - pH of 1:2.5 soil/water suspension
	5_C_B	Water soluble Chloride - Method recorded as B
	7A2	Total nitrogen - semimicro Kjeldahl , automated colour
	MIN_EC	Exchange Capacity - Minerology
	P10_NR_C	Clay (%) - Not recorded
	P10_NR_CS	Coarse sand (%) - Not recorded
	P10_NR_FS	Fine sand (%) - Not recorded
	P10_NR_Z	Silt (%) - Not recorded
	XRD_C_Gt	Geothite - X-Ray Diffraction
	XRD_C_Is	Interstratified clay minerals - X-Ray Diffraction
	XRD_C_Ka	Kaolin - X-Ray Diffraction
	XRD_C_Qz	Quartz - X-Ray Diffraction
	XRD_C_Vm	Vermiculte - X-Ray Diffraction