Project Name:	NSF
	Project Code:	NSF	Site ID:	VP92	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (VIC)
	Site Information
	Desc. By:	Locality:
	Date Desc.:	//	Elevation:	No Data
	Map Ref.:	Sheet No. : 7623   1:100000	Rainfall:	690
	Northing/Long.:	143.516666666667	Runoff:	No Data
	Easting/Lat.:	-37.4833333333333	Drainage:	Imperfectly drained
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	Basalt 
	Land Form
	Rel/Slope Class: 	No Data	Pattern Type:	No Data
	Morph. Type:	No Data	Relief:	No Data
	Elem. Type:	No Data	Slope Category:	No Data
	Slope:	3 % 	Aspect:	No Data
	Surface Soil Condition (dry):
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	 N/A    	Principal Profile Form:	Dy3.42
	ASC Confidence:	Great Soil Group:	Solodic soil
	Confidence level not specified
	Site Disturbance:
	Vegetation:
	Surface Coarse Fragments:
	Profile Morphology
	0 - 0.1 m	Dark reddish grey (5YR4/2-Moist); ; Loam; Weak grade of structure, 2-5 mm; Firm consistence; 
	0-2%, Quartz, coarse fragments; 
	0.1 - 0.2 m	Reddish grey (5YR5/2-Moist); ; Loam; Weak grade of structure, 2-5 mm; Firm consistence; 0-2%,
	 Quartz, coarse fragments; 
	0.2 - 0.3 m	Reddish grey (5YR5/2-Moist); ; Clay loam; Weak grade of structure, 2-5 mm; Firm consistence; 
	0-2%, Quartz, coarse fragments; 
	0.3 - 0.4 m	Pinkish grey (7.5YR6/2-Moist); ; Clay loam; Weak grade of structure, 2-5 mm; Firm consistence; 
	0-2%, Quartz, coarse fragments; 
	0.4 - 0.5 m	Light brownish grey (10YR6/2-Moist); ; Clay loam; Weak grade of structure, 2-5 mm; Firm 
	consistence; 0-2%, Quartz, coarse fragments; 
	0.5 - 0.6 m	Light brownish grey (10YR6/2-Moist); , 10YR68, 2-10% ; , 2-10% ; Light clay; Weak grade of 
	structure, 2-5 mm; Very strong consistence; 0-2%, Quartz, coarse fragments; 
	0.6 - 0.7 m	Dark greyish brown (10YR4/2-Moist); , 10YR68, 2-10% ; , 2-10% ; Light clay; Massive grade of 
	structure; Strong consistence; 0-2%, Quartz, coarse fragments; Very few (0 - 2 %), 
	Manganiferous, , Nodules; 
	0.7 - 0.8 m	Dark greyish brown (10YR4/2-Moist); , 10YR68, 2-10% ; , 2-10% ; Light clay; Massive grade of 
	structure; Strong consistence; 0-2%, Quartz, coarse fragments; Very few (0 - 2 %), 
	Manganiferous, , Nodules; 
	0.8 - 0.9 m	Dark greyish brown (10YR4/2-Moist); , 10YR68, 2-10% ; , 2-10% ; Light clay; Massive grade of 
	structure; Strong consistence; 0-2%, Quartz, coarse fragments; Few (2 - 10 %), Manganiferous, , 
	Nodules; 
	0.9 - 1 m	Grey (10YR6/1-Moist); , 10YR68, 2-10% ; , 2-10% ; Light clay; Weak grade of structure, 2-5 mm; 
	Very strong consistence; , Manganiferous, , Nodules; 
	Morphological Notes
	Observation Notes
	ORIGINALLY VP70/P11; DATA IS FROM BULK OF 8 CORES;                                                                      
	Site Notes

	Project Name:	NSF
	Project Code:	NSF	Site ID:	VP92	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (VIC)
	BEUUFORT

	Project Name:	NSF
	Project Code:	NSF	Site ID:	VP92	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (VIC)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.1	5.2I	 0.22D	 3.4K	 1.5	 0.75	 0.3
	0.1 - 0.2	5.6I	 0.1D
	0.2 - 0.3	6.1I	 0.08D
	0.3 - 0.4	6.6I	 0.07D
	0.4 - 0.5	7I	 0.1D
	0.5 - 0.6	7I	 0.11D	 4K	 6.4	 0.7	 1.7
	0.6 - 0.7	7.2I	 0.12D
	0.7 - 0.8	7.3I	 0.2D
	0.8 - 0.9	7.3I	 0.22D
	0.9 - 1	7.6I	 0.29D	 5.9K	 10	 0.65	 3.8
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.1	 0.273A	 4C	 37	 25	 24
	0.1 - 0.2	 0.096A
	0.2 - 0.3	 0.066A
	0.3 - 0.4
	0.4 - 0.5
	0.5 - 0.6	 0.045A	 5C	 31	 18	 46
	0.6 - 0.7
	0.7 - 0.8
	0.8 - 0.9
	0.9 - 1	 0.036A	 2C	 18	 14	 62
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.1
	0.1 - 0.2
	0.2 - 0.3
	0.3 - 0.4
	0.4 - 0.5
	0.5 - 0.6
	0.6 - 0.7
	0.7 - 0.8
	0.8 - 0.9
	0.9 - 1

	Project Name:	NSF
	Project Code:	NSF	Site ID:	VP92	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (VIC)
	Laboratory Analyses Completed for this profile
	15_NR_CA	Exch. basic cations (Ca++) - meq per 100g of soil - Not recorded
	15_NR_K	Exch. basic cations (K++) - meq per 100g of soil - Not recorded
	15_NR_MG	Exch. basic cations (Mg++) - meq per 100g of soil - Not recorded
	15_NR_NA	Exch. basic cations (Na++) - meq per 100g of soil - Not recorded
	2A1	Air-dry moisture content
	3_C_B	Electrical conductivity or soluble salts - Total soluble salts %
	4A_C_2.5	pH of soil - pH of 1:2.5 soil/water suspension
	5_C_B	Water soluble Chloride - Method recorded as B
	7A2	Total nitrogen - semimicro Kjeldahl , automated colour
	MIN_EC	Exchange Capacity - Minerology
	P10_NR_C	Clay (%) - Not recorded
	P10_NR_CS	Coarse sand (%) - Not recorded
	P10_NR_FS	Fine sand (%) - Not recorded
	P10_NR_Z	Silt (%) - Not recorded
	XRD_C_Il	Illite - X-Ray Diffraction
	XRD_C_Is	Interstratified clay minerals - X-Ray Diffraction
	XRD_C_Ka	Kaolin - X-Ray Diffraction
	XRD_C_Qz	Quartz - X-Ray Diffraction