Project Name:	NSF
	Project Code:	NSF	Site ID:	VP95	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (VIC)
	Site Information
	Desc. By:	Locality:
	Date Desc.:	//	Elevation:	No Data
	Map Ref.:	Sheet No. : 8124   1:100000	Rainfall:	665
	Northing/Long.:	146.1	Runoff:	No Data
	Easting/Lat.:	-36.5166666666667	Drainage:	Imperfectly drained
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	No Data	Pattern Type:	No Data
	Morph. Type:	No Data	Relief:	No Data
	Elem. Type:	No Data	Slope Category:	No Data
	Slope:	2 % 	Aspect:	No Data
	Surface Soil Condition (dry):
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	 N/A    	Principal Profile Form:	Db2.22
	ASC Confidence:	Great Soil Group:	Solodic soil
	Confidence level not specified
	Site Disturbance:	Complete clearing. Pasture, native or improved, cultivated at some stage
	Vegetation:
	Surface Coarse Fragments:
	Profile Morphology
	0 - 0.05 m	Very dark brown (10YR2/2-Moist); ; Silty loam; Massive grade of structure; Very weak 
	consistence; 
	0.05 - 0.1 m	Dark brown (10YR3/3-Moist); ; Silty loam; Moderate grade of structure, 2-5 mm; Very weak 
	consistence; Very few (0 - 2 %), Ferruginous, , Nodules; 
	0.1 - 0.2 m	Dark greyish brown (10YR4/2-Moist); ; Silty loam; Moderate grade of structure, 2-5 mm; Very 
	weak consistence; Very few (0 - 2 %), Ferruginous, , Nodules; 
	0.2 - 0.3 m	Dark greyish brown (10YR4/2-Moist); ; Silty loam; Moderate grade of structure, 5-10 mm; Very 
	weak consistence; Very few (0 - 2 %), Ferruginous, , Nodules; 
	0.3 - 0.4 m	Greyish brown (2.5Y5/2-Moist); , 2.5YR36, 2-10% ; , 2-10% ; Light clay; Strong grade of structure,
	 10-20 mm; Strong consistence; 
	0.4 - 0.5 m	Olive brown (2.5Y4/5-Moist); , 2.5YR36, 2-10% ; , 2-10% ; Light clay; Moderate grade of structure,
	 10-20 mm; Very strong consistence; 
	0.5 - 0.6 m	Olive brown (2.5Y4/4-Moist); ; Light clay; Moderate grade of structure, 10-20 mm; Very strong 
	consistence; 
	0.6 - 0.7 m	Olive brown (2.5Y4/4-Moist); , 2.5YR36, 10-20% ; , 10-20% ; Heavy clay; Moderate grade of 
	structure, 10-20 mm; Very strong consistence; 
	0.7 - 0.8 m	Dark greyish brown (2.5Y4/2-Moist); , 2.5YR36, 10-20% ; , 10-20% ; Heavy clay; Moderate grade 
	of structure, 10-20 mm; Very strong consistence; 
	0.8 - 0.9 m	Dark greyish brown (2.5Y4/2-Moist); , 10YR44, 10-20% ; , 2.5YR36, 10-20% ; Light clay; Weak 
	grade of structure, 10-20 mm; Very strong consistence; 
	0.9 - 1 m	Olive brown (2.5Y4/5-Moist); , 2.5Y52, 10-20% ; , 10-20% ; Light clay; Weak grade of structure, 
	10-20 mm; Very strong consistence; 
	Morphological Notes
	Observation Notes
	ORIGINALLY VP69/P3;MORPHOLOGY FROM SINGLE CORE No1;CHEM DATA FROM BULK OF 9 CORES:                                 
	     
	Site Notes

	Project Name:	NSF
	Project Code:	NSF	Site ID:	VP95	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (VIC)
	BENALLA

	Project Name:	NSF
	Project Code:	NSF	Site ID:	VP95	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (VIC)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.05	5.1I	 0.1D	 1.4K	 0.35	 0.1
	0.05 - 0.1	5.3I	 0D
	0.1 - 0.2	5.7I	 0D
	0.2 - 0.3	6I	 0D
	0.3 - 0.4	5.9I	 0.09D	 2.2K	 5.9	 1.6
	0.4 - 0.5	6I	 0.1D
	0.5 - 0.6	6.1I	 0.12D
	0.6 - 0.7	6.1I	 0.17D
	0.7 - 0.8	6.4I	 0.19D
	0.8 - 0.9	6.8I	 0.2D	 1.3K	 7.4	 3.1
	0.9 - 1
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.05	 0.175A	 5C	 52	 30	 10
	0.05 - 0.1	 0.027A
	0.1 - 0.2	 0.022A
	0.2 - 0.3
	0.3 - 0.4	 2C	 33	 25	 36
	0.4 - 0.5	 0.024A
	0.5 - 0.6
	0.6 - 0.7
	0.7 - 0.8
	0.8 - 0.9	 0.015A	 45	 25	 25
	0.9 - 1	 4C
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.05
	0.05 - 0.1
	0.1 - 0.2
	0.2 - 0.3
	0.3 - 0.4
	0.4 - 0.5
	0.5 - 0.6
	0.6 - 0.7
	0.7 - 0.8
	0.8 - 0.9
	0.9 - 1

	Project Name:	NSF
	Project Code:	NSF	Site ID:	VP95	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (VIC)
	Laboratory Analyses Completed for this profile
	15_NR_CA	Exch. basic cations (Ca++) - meq per 100g of soil - Not recorded
	15_NR_MG	Exch. basic cations (Mg++) - meq per 100g of soil - Not recorded
	15_NR_NA	Exch. basic cations (Na++) - meq per 100g of soil - Not recorded
	2A1	Air-dry moisture content
	3_C_B	Electrical conductivity or soluble salts - Total soluble salts %
	4A_C_2.5	pH of soil - pH of 1:2.5 soil/water suspension
	5_C_B	Water soluble Chloride - Method recorded as B
	7A2	Total nitrogen - semimicro Kjeldahl , automated colour
	MIN_EC	Exchange Capacity - Minerology
	P10_NR_C	Clay (%) - Not recorded
	P10_NR_CS	Coarse sand (%) - Not recorded
	P10_NR_FS	Fine sand (%) - Not recorded
	P10_NR_Z	Silt (%) - Not recorded
	XRD_C_Hm	Hematite - X-Ray Diffraction
	XRD_C_Il	Illite - X-Ray Diffraction
	XRD_C_Is	Interstratified clay minerals - X-Ray Diffraction
	XRD_C_Ka	Kaolin - X-Ray Diffraction
	XRD_C_Qz	Quartz - X-Ray Diffraction