Project Name:	NSF
	Project Code:	NSF	Site ID:	VW105	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (VIC)
	Site Information
	Desc. By:	Locality:
	Date Desc.:	//	Elevation:	No Data
	Map Ref.:	Rainfall:	0
	Northing/Long.:	145.9	Runoff:	No Data
	Easting/Lat.:	-36.1166666666667	Drainage:	No Data
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	No Data	Pattern Type:	No Data
	Morph. Type:	No Data	Relief:	No Data
	Elem. Type:	No Data	Slope Category:	No Data
	Slope:	0 % 	Aspect:	No Data
	Surface Soil Condition (dry):	Hardsetting
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	 N/A    	Principal Profile Form:	Dr2.13
	ASC Confidence:	Great Soil Group:	Red-brown earth
	Confidence level not specified
	Site Disturbance:
	Vegetation:
	Surface Coarse Fragments:
	Profile Morphology
	0 - 0.16 m	Dark reddish brown (5YR3/3-Moist); ; Loam; Massive grade of structure; 
	0.16 - 0.4 m	Olive (5Y4/4-Moist); ; Light clay; Moderate grade of structure; Very few (0 - 2 %), Manganiferous, 
	Fine (0 - 2 mm), Soft segregations; 
	0.4 - 1 m	Yellowish red (5YR5/6-Moist); ; Medium clay; Moderate grade of structure; Very few (0 - 2 %), 
	Manganiferous, Fine (0 - 2 mm), Soft segregations; Very few (0 - 2 %), Calcareous, , Soft 
	segregations; 
	1 - 1.1 m	Yellowish red (5YR5/6-Moist); ; Medium clay; Moderate grade of structure; Very few (0 - 2 %), 
	Calcareous, , Soft segregations; 
	1.1 - 1.4 m	; 
	Morphological Notes
	Observation Notes
	VW72/W22                                                                                                                
	Site Notes
	TUNGAMAH

	Project Name:	NSF
	Project Code:	NSF	Site ID:	VW105	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (VIC)
	Laboratory Test Results:
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.1	5.8I	 0.13D
	0.1 - 0.2	6.5I	 0.13D
	0.2 - 0.3	7.3I	 0.27D
	0.3 - 0.4	8.1I	 0.42D
	0.4 - 0.5	8.3I	 0.62D
	0.5 - 0.6	8.4I	 0.88D
	0.6 - 0.7	8.5I	 1.1D
	0.7 - 0.8	8.6I	 1.2D
	0.8 - 0.9	8.7I	 1.3D
	0.9 - 1	8.7I	 1.3D
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.1	 1.55A
	0.1 - 0.2	 0.73A
	0.2 - 0.3	 0.5A
	0.3 - 0.4	 0.27A
	0.4 - 0.5	 0.25A
	0.5 - 0.6	 0.19A
	0.6 - 0.7	 0.16A
	0.7 - 0.8	 0.11A
	0.8 - 0.9	 0.1A
	0.9 - 1	 0.09A
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.1
	0.1 - 0.2
	0.2 - 0.3
	0.3 - 0.4
	0.4 - 0.5
	0.5 - 0.6
	0.6 - 0.7
	0.7 - 0.8
	0.8 - 0.9
	0.9 - 1

	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Project Name:	NSF
	Project Code:	NSF	Site ID:	VW105	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (VIC)
	Laboratory Analyses Completed for this profile
	3_C_B	Electrical conductivity or soluble salts - Total soluble salts %
	4A_C_2.5	pH of soil - pH of 1:2.5 soil/water suspension
	5_C_B	Water soluble Chloride - Method recorded as B
	6A1	Organic carbon - Walkley and Black