Project Name:	NSF
	Project Code:	NSF	Site ID:	VW117	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (VIC)
	Site Information
	Desc. By:	K.H. Northcote	Locality:	Walpeup
	Date Desc.:	07/04/70	Elevation:	No Data
	Map Ref.:	1:10000	Rainfall:	No Data
	Northing/Long.:	142.01666666	Runoff:	No Data
	Easting/Lat.:	-35.15  Datum: AGD66	Drainage:	No Data
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	No Data	Pattern Type:	No Data
	Morph. Type:	No Data	Relief:	No Data
	Elem. Type:	No Data	Slope Category:	No Data
	Slope:	 % 	Aspect:	No Data
	Surface Soil Condition 
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	 N/A    	Principal Profile Form:	Gc1.12
	ASC Confidence:	Great Soil Group:	Solonized brown 
	Confidence level not specified	soil
	Site 
	Vegetation:
	Surface Coarse 
	Profile 
	A	0 - 0.1 m	Brown (7.5YR5/4-Moist); ; Loamy sand; Massive grade of structure; 2-10%, coarse fragments; 
	A	0.1 - 0.2 m	Brown (7.5YR5/4-Moist); ; Sandy loam; Massive grade of structure; 10-20%, coarse fragments; Gradual 
	change to - 
	B	0.2 - 0.3 m	Brown (7.5YR5/4-Moist); ; Loam; Massive grade of structure; 20-50%, coarse fragments; 
	0.3 - 0.4 m	Reddish yellow (5YR6/6-Moist); ; Clay loam; Massive grade of structure; 20-50%, coarse fragments; 
	0.4 - 0.5 m	Reddish yellow (5YR7/6-Moist); ; Clay loam; Massive grade of structure; 20-50%, coarse fragments; 
	0.5 - 0.6 m	Reddish yellow (5YR7/8-Moist); Yellowish red (5YR5/6-Moist); ; Light clay; Massive grade of structure; 
	2-10%, coarse fragments; 
	0.6 - 0.7 m	Strong brown (7.5YR5/6-Moist); Reddish yellow (7.5YR7/6-Moist); ; Light clay; Massive grade of 
	structure; 2-10%, coarse fragments; 
	0.7 - 0.8 m	Reddish yellow (5YR6/8-Moist); Yellowish red (5YR4/8-Moist); ; Medium heavy clay; Massive grade of 
	structure; 2-10%, coarse fragments; 
	0.8 - 0.9 m	Reddish yellow (5YR6/6-Moist); Red (2.5YR5/8-Moist); ; Medium heavy clay; Massive grade of 
	structure; 10-20%, coarse fragments; 
	0.9 - 1 m	Reddish yellow (5YR6/6-Moist); ; Sandy clay loam; Massive grade of structure; 10-20%, coarse 
	fragments; 
	Morphological Notes
	Observation Notes
	unpublished; previously VW70/W19; chemistry mean and bulk of 8 cores
	Site Notes

	Project Name:	NSF
	Project Code:	NSF	Site ID:	VW117	Observation 	1
	Agency Name:	CSIRO Division of Soils (VIC)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.1	8.4I	0.3D	14K	2.2	1.9	0.7	16J	4.38
	0.1 - 0.2	8.6I	0.38D
	0.2 - 0.3	9.1I	0.68D
	0.3 - 0.4	9.5I	1.07D	5.3K	5.5	1.4	4.2	12J	35.00
	0.4 - 0.5	9.7I	1.37D
	0.5 - 0.6	9.7I	1.72D
	0.6 - 0.7	9.7I	1.63D
	0.7 - 0.8	9.6I	1.76D
	0.8 - 0.9	9.6I	1.74D
	0.9 - 1	9.5I	1.93D	2.3K	5.1	1.8	6.5	13J	50.00
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.1	8.9C	1.1A	0.088A	43C	25	3	16
	0.1 - 0.2	15.9C	0.78A	0.06A
	0.2 - 0.3	31.7C	0.47A	0.043A
	0.3 - 0.4	40.9C	0.3A	23C	14	2	15
	0.4 - 0.5	47.3C	0.21A
	0.5 - 0.6	48C	0.17A
	0.6 - 0.7	46C	0.17A
	0.7 - 0.8	37C	0.14A
	0.8 - 0.9	38.6C	0.12A
	0.9 - 1	33.4C	0.12A	0.008A	24C	18	1	21
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.1
	0.1 - 0.2
	0.2 - 0.3
	0.3 - 0.4
	0.4 - 0.5
	0.5 - 0.6
	0.6 - 0.7
	0.7 - 0.8
	0.8 - 0.9
	0.9 - 1
	Laboratory Analyses Completed for this profile
	15_NR_CA	Exch. basic cations (Ca++) - meq per 100g of soil - Not recorded
	15_NR_CEC	CEC - meq per 100g of soil - Not recorded
	15_NR_K	Exch. basic cations (K++) - meq per 100g of soil - Not recorded
	15_NR_MG	Exch. basic cations (Mg++) - meq per 100g of soil - Not recorded
	15_NR_NA	Exch. basic cations (Na++) - meq per 100g of soil - Not recorded
	19B_NR	Calcium Carbonate (CaCO3) - Not recorded
	2A1	Air-dry moisture content
	3_C_B	Electrical conductivity or soluble salts - Total soluble salts %
	4A_C_2.5	pH of soil - pH of 1:2.5 soil/water suspension

	5_C_B	Water soluble Chloride - Method recorded as B
	6A1	Organic carbon - Walkley and Black
	7A2	Total nitrogen - semimicro Kjeldahl , automated colour
	MIN_EC	Exchange Capacity - Minerology
	P10_NR_C	Clay (%) - Not recorded
	P10_NR_CS	Coarse sand (%) - Not recorded
	P10_NR_FS	Fine sand (%) - Not recorded
	P10_NR_Z	Silt (%) - Not recorded