Project Name:	NSF
	Project Code:	NSF	Site ID:	VW45	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (VIC)
	Site Information
	Desc. By:	Locality:
	Date Desc.:	//	Elevation:	No Data
	Map Ref.:	Rainfall:	0
	Northing/Long.:	142.75	Runoff:	No Data
	Easting/Lat.:	-36.55	Drainage:	No Data
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	No Data	Pattern Type:	No Data
	Morph. Type:	No Data	Relief:	No Data
	Elem. Type:	No Data	Slope Category:	No Data
	Slope:	0 % 	Aspect:	No Data
	Surface Soil Condition (dry):	Self-mulching
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	 N/A    	Principal Profile Form:	Ug5.24
	ASC Confidence:	Great Soil Group:	Grey clay
	Confidence level not specified
	Site Disturbance:
	Vegetation:
	Surface Coarse Fragments:
	Profile Morphology
	A	0 - 0.2 m	Dark greyish brown (10YR4/2-Moist); ; Light medium clay; Moderate grade of structure; 
	B21	0.2 - 0.5 m	Yellowish brown (10YR5/4-Moist); ; Medium clay; Moderate grade of structure; 
	B22	0.5 - 0.8 m	Light yellowish brown (10YR6/4-Moist); ; Medium clay; Moderate grade of structure; 
	B23	0.8 - 1 m	Brown (10YR5/3-Moist); ; Medium clay; Moderate grade of structure; 
	1 - 1.1 m	Brown (10YR5/3-Moist); ; Medium clay; Moderate grade of structure; 
	1.1 - 1.4 m	; 
	Morphological Notes
	Observation Notes
	VW70/W3                                                                                                                 
	Site Notes
	BURREREO

	Project Name:	NSF
	Project Code:	NSF	Site ID:	VW45	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (VIC)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.1	 30K	 5.9	 2	 1.5
	0.1 - 0.2	8.8I	 0.28D
	0.2 - 0.3	8.9I	 0.36D
	0.3 - 0.4	 26K	 12	 2.1	 5.3
	0.4 - 0.5	9I	 0.55D
	0.5 - 0.6	9I	 0.77D
	0.6 - 0.7	9I	 1.02D
	0.7 - 0.8	8.9I	 1.3D
	0.8 - 0.9	8.8I	 1.73D
	0.9 - 1	 12K	 12	 2	 12
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.1	 14C	 17	 8	 48
	0.1 - 0.2	 0.51A	 0.061A
	0.2 - 0.3	 0.49A	 0.061A
	0.3 - 0.4	 13C	 13	 6	 49
	0.4 - 0.5	 0.41A
	0.5 - 0.6	 0.34A	 0.04A
	0.6 - 0.7	 0.29A
	0.7 - 0.8	 0.25A
	0.8 - 0.9	 0.2A
	0.9 - 1	 13C	 12	 8	 50
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.1
	0.1 - 0.2
	0.2 - 0.3
	0.3 - 0.4
	0.4 - 0.5
	0.5 - 0.6
	0.6 - 0.7
	0.7 - 0.8
	0.8 - 0.9
	0.9 - 1

	Project Name:	NSF
	Project Code:	NSF	Site ID:	VW45	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (VIC)
	Laboratory Analyses Completed for this profile
	15_NR_CA	Exch. basic cations (Ca++) - meq per 100g of soil - Not recorded
	15_NR_K	Exch. basic cations (K++) - meq per 100g of soil - Not recorded
	15_NR_MG	Exch. basic cations (Mg++) - meq per 100g of soil - Not recorded
	15_NR_NA	Exch. basic cations (Na++) - meq per 100g of soil - Not recorded
	3_C_B	Electrical conductivity or soluble salts - Total soluble salts %
	4A_C_2.5	pH of soil - pH of 1:2.5 soil/water suspension
	5_C_B	Water soluble Chloride - Method recorded as B
	6A1	Organic carbon - Walkley and Black
	7A2	Total nitrogen - semimicro Kjeldahl , automated colour
	MIN_EC	Exchange Capacity - Minerology
	P10_NR_C	Clay (%) - Not recorded
	P10_NR_CS	Coarse sand (%) - Not recorded
	P10_NR_FS	Fine sand (%) - Not recorded
	P10_NR_Z	Silt (%) - Not recorded
	XRD_C_Il	Illite - X-Ray Diffraction
	XRD_C_Is	Interstratified clay minerals - X-Ray Diffraction
	XRD_C_Ka	Kaolin - X-Ray Diffraction
	XRD_C_Qz	Quartz - X-Ray Diffraction