Project Name:	Shire of Kowree, Vic
	Project Code:	SK	Site ID:	A10	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (VIC)
	Site Information
	Desc. By:	G. Blackburn	Locality:
	Date Desc.:	19/11/53	Elevation:	 180 metres
	Map Ref.:	1:250000	Rainfall:	540
	Northing/Long.:	141.238611111111	Runoff:	No runoff
	Easting/Lat.:	-36.8211111111111	Drainage:	Very poorly drained
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	Rolling plains <9m 10-32%	Pattern Type:	Plain
	Morph. Type:	Flat	Relief:	9 metres
	Elem. Type:	Plain	Slope Category:	No Data
	Slope:	0 % 	Aspect:	No Data
	Surface Soil Condition (dry):
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Hypercalcic Mottled-Subnatric Yellow Sodosol     	Principal Profile Form:	Dy3.43
	ASC Confidence:	Great Soil Group:	Solodized solonetz
	No analytical data are available but confidence is fair.
	Site Disturbance:	No effective disturbance. Natural
	Vegetation:
	Mid Strata - Shrub, , . *Species includes - None recorded
	Tall Strata - Tree, 6.01-12m, . *Species includes - None Recorded
	Surface Coarse Fragments:
	Profile Morphology
	0 - 0.08 m	Light brownish grey (10YR6/2-Moist); ; Sand; Loose consistence; 
	0.08 - 0.3 m	; 10-20%, Gravel, coarse fragments; 
	0.3 - 0.38 m	Pale brown (10YR6/3-Moist); ; Sand; , Columnar; Strong consistence; 
	0.38 - 0.6 m	Brownish yellow (10YR6/6-Moist); , 10R56; Sandy medium clay; 
	1 - 1.06 m	Brownish yellow (10YR6/6-Moist); ; Medium clay; Many (20 - 50 %), Calcareous, , Soft 
	segregations; 
	Morphological Notes
	Observation Notes
	LAYERS RENUMBERED 10/11/92                                                                                              
	Site Notes
	LOWAN S & L.U. No 17. Map Site 10

	Project Name:	Shire of Kowree, Vic
	Project Code:	SK	Site ID:	A10	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (VIC)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.08	6.9A	 0.009C
	0.08 - 0.3
	0.3 - 0.38	6.8A	 0.018C
	0.38 - 0.6
	1 - 1.05	9.2A	 0.258C
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.08	 58C	 37	 2	 3
	0.08 - 0.3
	0.3 - 0.38
	0.38 - 0.6
	1 - 1.05
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.08
	0.08 - 0.3
	0.3 - 0.38
	0.38 - 0.6
	1 - 1.05

	Project Name:	Shire of Kowree, Vic
	Project Code:	SK	Site ID:	A10	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (VIC)
	Laboratory Analyses Completed for this profile
	2_LOI	Loss on Ignition (%)
	2A1	Air-dry moisture content
	3A_TSS	Electrical conductivity or soluble salts - Total soluble salts %
	4A1	pH of 1:5 soil/water suspension
	5A2	Chloride - 1:5 soil/water extract, automated colour
	P10_NR_C	Clay (%) - Not recorded
	P10_NR_CS	Coarse sand (%) - Not recorded
	P10_NR_FS	Fine sand (%) - Not recorded
	P10_NR_Z	Silt (%) - Not recorded