Project Name:	Shire of Kowree, Vic
	Project Code:	SK	Site ID:	A13	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (VIC)
	Site Information
	Desc. By:	G. Blackburn	Locality:
	Date Desc.:	20/11/53	Elevation:	 152 metres
	Map Ref.:	1:250000	Rainfall:	520
	Northing/Long.:	141.099444444445	Runoff:	Moderately rapid
	Easting/Lat.:	-36.7711111111111	Drainage:	Imperfectly drained
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	Rolling plains <9m 10-32%	Pattern Type:	Plain
	Morph. Type:	Closed Depression	Relief:	9 metres
	Elem. Type:	Swamp	Slope Category:	No Data
	Slope:	0 % 	Aspect:	No Data
	Surface Soil Condition (dry):
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Calcic Subnatric Grey Sodosol     	Principal Profile Form:	Dy3.43
	ASC Confidence:	Great Soil Group:	Solodized solonetz
	No analytical data are available but confidence is fair.
	Site Disturbance:
	Vegetation:	Low Strata - Shrub, , . *Species includes - None recorded
	Tall Strata - Tree, 12.01-20m, Sparse. *Species includes - Casuarina leuhmannii
	Surface Coarse Fragments:
	Profile Morphology
	0 - 0.05 m	Grey (10YR5/1-Moist); ; Sandy loam; Loose consistence; 
	0.05 - 0.2 m	Light grey (10YR7/2-Moist); ; Sand; Very firm consistence; 
	0.2 - 0.28 m	White (10YR8/2-Moist); ; Medium clay; 100-200 mm, Columnar; Firm consistence; 
	0.45 - 0.75 m	Brownish yellow (10YR6/6-Moist); ; Clay loam; Few (2 - 10 %), Calcareous, , Soft segregations; 
	0.5 - 0.55 m	Brownish yellow (10YR6/6-Moist); ; Medium clay; Common (10 - 20 %), Calcareous, , Soft 
	segregations; 
	Morphological Notes
	Observation Notes
	LAYER 2 - BLEACHED TOP 1CM THICK: LAYERS RENUMBERED 10/11/92                                                            
	Site Notes
	LOWAN S & L.U. No 17. Map Site 13

	Project Name:	Shire of Kowree, Vic
	Project Code:	SK	Site ID:	A13	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (VIC)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.05	6.7A	 0.023C
	0.05 - 0.2
	0.2 - 0.28	7.6A	 0.037C
	0.45 - 0.75
	0.5 - 0.55	9.3A	 0.171C
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.05
	0.05 - 0.2
	0.2 - 0.28
	0.45 - 0.75
	0.5 - 0.55
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.05
	0.05 - 0.2
	0.2 - 0.28
	0.45 - 0.75
	0.5 - 0.55

	Project Name:	Shire of Kowree, Vic
	Project Code:	SK	Site ID:	A13	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (VIC)
	Laboratory Analyses Completed for this profile
	2_LOI	Loss on Ignition (%)
	2A1	Air-dry moisture content
	3A_TSS	Electrical conductivity or soluble salts - Total soluble salts %
	4A1	pH of 1:5 soil/water suspension
	5A2	Chloride - 1:5 soil/water extract, automated colour