Project Name:	Victorian Beach Ridge Studies
	Project Code:	VBR	Site ID:	A1067	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (VIC)
	Site Information
	Desc. By:	G. Blackburn	Locality:
	Date Desc.:	14/03/67	Elevation:	 61 metres
	Map Ref.:	Rainfall:	280
	Northing/Long.:	141.651666666667	Runoff:	Slow
	Easting/Lat.:	-34.8944444444445	Drainage:	Imperfectly drained
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	Undulating plains <9m 3-10%	Pattern Type:	Plain
	Morph. Type:	Flat	Relief:	6 metres
	Elem. Type:	Plain	Slope Category:	No Data
	Slope:	0 % 	Aspect:	No Data
	Surface Soil Condition (dry):
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Epicalcareous Epipedal Grey Vertosol     	Principal Profile Form:	N/A
	ASC Confidence:	Great Soil Group:	Grey clay
	No analytical data are available but confidence is fair.
	Site Disturbance:	No effective disturbance other than grazing by hoofed animals
	Vegetation:
	Tall Strata - Tree mallee, , . *Species includes - Eucalyptus species
	Surface Coarse Fragments:
	Profile Morphology
	0 - 0.15 m	Light brownish grey (2.5Y6/2-Moist); ; Light clay; , Angular blocky; Strong consistence; Very few 
	(0 - 2 %), Calcareous, , Soft segregations; Field pH 9 (pH meter); Diffuse change to - 
	0.15 - 0.25 m	Light brownish grey (2.5Y6/2-Moist); ; Medium clay; , Angular blocky; Strong consistence; 
	0.25 - 0.45 m	Greyish brown (2.5Y5/2-Moist); ; Medium clay; , Angular blocky; Strong consistence; Few (2 - 10 
	%), Calcareous, Medium (2 -6 mm), Concretions; Field pH 9 (pH meter); 
	0.45 - 0.65 m	Greyish brown (2.5Y5/3-Moist); ; Medium clay; , Angular blocky; Strong consistence; Few (2 - 10 
	%), Calcareous, Coarse (6 - 20 mm), Concretions; 
	0.65 - 0.75 m	Greyish brown (2.5Y5/3-Moist); ; Medium clay; , Angular blocky; Very strong consistence; Few (2 
	- 10 %), Calcareous, , Soft segregations; Field pH 9 (pH meter); 
	0.75 - 0.92 m	Greyish brown (2.5Y5/3-Moist); ; Medium heavy clay; , Angular blocky; Very strong consistence; 
	Very few (0 - 2 %), Calcareous, , Soft segregations; Field pH 9 (pH meter); 
	Morphological Notes
	Observation Notes
	CLAY SKINS INCREASING IN THICKNESS WITH DEPTH LAYER 3 - SLIGHT GYPSUM:                                                  
	Site Notes
	MILLEWA

	Project Name:	Victorian Beach Ridge Studies
	Project Code:	VBR	Site ID:	A1067	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (VIC)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.15
	0.15 - 0.25
	0.25 - 0.45
	0.45 - 0.65
	0.65 - 0.75
	0.75 - 0.92
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.15
	0.15 - 0.25
	0.25 - 0.45
	0.45 - 0.65
	0.65 - 0.75
	0.75 - 0.92
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.15
	0.15 - 0.25
	0.25 - 0.45
	0.45 - 0.65
	0.65 - 0.75
	0.75 - 0.92

	Project Name:	Victorian Beach Ridge Studies
	Project Code:	VBR	Site ID:	A1067	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (VIC)
	Laboratory Analyses Completed for this profile