Project Name:	Wimmera Rec. & Little Desert, Vic.
	Project Code:	WR	Site ID:	A832	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (VIC)
	Site Information
	Desc. By:	G. Blackburn	Locality:	CLEARED ARABLE LAND IN USE FOR CEREAL & 
	LIVESTOCK PRODUCTION
	Date Desc.:	26/07/62	Elevation:	 171 metres
	Map Ref.:	Rainfall:	0
	Northing/Long.:	141.55	Runoff:	Slow
	Easting/Lat.:	-36.73333333	Drainage:	Imperfectly drained
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	Gently undulating plains <9m  	Pattern Type:	Plain
	1-3%
	Morph. Type:	Flat	Relief:	3 metres
	Elem. Type:	Plain	Slope Category:	Very gently sloped
	Slope:	0 % 	Aspect:	No Data
	Surface Soil Condition (dry):
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Haplic Epihypersodic Class Undetermined Vertosol     	Principal Profile Form:	N/A
	ASC Confidence:	Great Soil Group:	N/A
	No analytical data are available but confidence is fair.
	Site Disturbance:	Complete clearing. Pasture, native or improved, cultivated at some stage
	Vegetation:
	Tall Strata - , , . *Species includes - Casuarina leuhmannii
	Surface Coarse Fragments:
	Profile Morphology
	0 - 0.08 m	; Medium clay; 
	0.08 - 0.15 m	; Medium clay; Common (10 - 20 %), Calcareous, , Soft segregations; 
	0.15 - 0.3 m	; Medium clay; Common (10 - 20 %), Calcareous, , Soft segregations; 
	0.3 - 0.53 m	; Medium clay; Common (10 - 20 %), Calcareous, , Soft segregations; 
	0.53 - 0.79 m	; Medium clay; Common (10 - 20 %), Calcareous, , Soft segregations; 
	0.79 - 0.91 m	; Medium clay; Common (10 - 20 %), Calcareous, , Soft segregations; 
	0.91 - 1.14 m	; Medium clay; Common (10 - 20 %), Calcareous, , Soft segregations; 
	1.14 - 1.32 m	; Medium clay; Common (10 - 20 %), Calcareous, , Soft segregations; 
	1.32 - 1.52 m	; Medium clay; Common (10 - 20 %), Calcareous, , Soft segregations; 
	1.52 - 1.73 m	; Medium clay; Common (10 - 20 %), Calcareous, , Soft segregations; 
	1.73 - 1.85 m	; Medium clay; Common (10 - 20 %), Calcareous, , Soft segregations; 
	Morphological Notes
	Observation Notes
	Site Notes
	BORUNG

	Project Name:	Wimmera Rec. & Little Desert, Vic.
	Project Code:	WR	Site ID:	A832	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (VIC)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.08	8.3H	 0.065C
	0.08 - 0.15	8.5H	 0.06C
	0.15 - 0.3	9H	 0.069C
	0.3 - 0.53	9.3H	 0.1C
	0.53 - 0.79	9.3H	 0.19C
	0.79 - 0.91	9.2H	 0.29C
	0.91 - 1.14	9.2H	 0.38C
	1.14 - 1.32	9H	 0.46C
	1.32 - 1.52	9H	 0.49C
	1.52 - 1.73	9H	 0.46C
	1.73 - 1.85	8.8H	 0.45C
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.08	 1.4C	 0.15B	 16C	 21	 9	 48
	0.08 - 0.15	 1.8C	 0.095B	 14C	 16	 5	 58
	0.15 - 0.3	 4.9C	 0.054B	 11C	 15	 3	 63
	0.3 - 0.53	 2.5C
	0.53 - 0.79	 1.7C	 0.038B	 12C	 16	 2	 64
	0.79 - 0.91	 1.1C
	0.91 - 1.14	 9C	 0.021B	 1	 13C	 14	 5	 58
	1.14 - 1.32	 4.9C
	1.32 - 1.52	 1.3C	 0.014B	 15C	 16	 6	 58
	1.52 - 1.73	 0.21C
	1.73 - 1.85	 0.76C	 0.012B	 19C	 18	 5	 56
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.08
	0.08 - 0.15
	0.15 - 0.3
	0.3 - 0.53
	0.53 - 0.79
	0.79 - 0.91
	0.91 - 1.14
	1.14 - 1.32
	1.32 - 1.52
	1.52 - 1.73
	1.73 - 1.85

	Project Name:	Wimmera Rec. & Little Desert, Vic.
	Project Code:	WR	Site ID:	A832	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (VIC)
	Laboratory Analyses Completed for this profile
	19B_NR	Calcium Carbonate (CaCO3) - Not recorded
	2_LOI	Loss on Ignition (%)
	2A1	Air-dry moisture content
	3A_TSS	Electrical conductivity or soluble salts - Total soluble salts %
	4_NR	pH of soil - Not recorded
	5_NR	Water soluble Chloride - Cl(%) - Not recordede
	7_NR	Total nitrogen (%) - Not recorded
	P10_GRAV	Gravel (%)
	P10_NR_C	Clay (%) - Not recorded
	P10_NR_CS	Coarse sand (%) - Not recorded
	P10_NR_FS	Fine sand (%) - Not recorded
	P10_NR_Z	Silt (%) - Not recorded
	XRD_C_Hm	Hematite - X-Ray Diffraction
	XRD_C_Il	Illite - X-Ray Diffraction
	XRD_C_Ka	Kaolin - X-Ray Diffraction
	XRD_C_Qz	Quartz - X-Ray Diffraction
	XRD_C_St	Smectite - X-Ray Diffraction