Project Name:	Wimmera Rec. & Little Desert, Vic.
	Project Code:	WR	Site ID:	A838	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (VIC)
	Site Information
	Desc. By:	G. Blackburn	Locality:	CEREAL CULTIVATION
	Date Desc.:	06/09/62	Elevation:	 85 metres
	Map Ref.:	Rainfall:	330
	Northing/Long.:	141.83333333	Runoff:	Slow
	Easting/Lat.:	-35.78333333	Drainage:	Poorly drained
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	No Data	Pattern Type:	No Data
	Morph. Type:	Flat	Relief:	No Data
	Elem. Type:	Plain	Slope Category:	Level
	Slope:	0 % 	Aspect:	No Data
	Surface Soil Condition (dry):
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	 N/A    	Principal Profile Form:	N/A
	ASC Confidence:	Great Soil Group:	N/A
	No analytical data are available but confidence is fair.
	Site Disturbance:
	Vegetation:
	Tall Strata - Tree mallee, 6.01-12m, . *Species includes - Eucalyptus camaldulensis
	Surface Coarse Fragments:
	Profile Morphology
	0 - 0.1 m	; Medium clay; 
	0.13 - 0.32 m	; Medium clay; 
	0.32 - 0.51 m	; Medium clay; 
	0.51 - 0.71 m	; Medium clay; 
	0.71 - 0.97 m	; Medium clay; 
	0.97 - 1.14 m	; Medium clay; 
	Morphological Notes
	shows clay skins
	Observation Notes
	Site Notes
	WEEAH

	Project Name:	Wimmera Rec. & Little Desert, Vic.
	Project Code:	WR	Site ID:	A838	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (VIC)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.1	9H	 0.86C
	0.13 - 0.32	9.2H	 1.2C
	0.32 - 0.51	9.2H	 1.1C
	0.51 - 0.71	9.2H	 1.1C
	0.71 - 0.97	9.2H	 1C
	0.97 - 1.14	9.1H	 1.1C
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.1	 10C	 18C	 22	 7	 41
	0.13 - 0.32	 8.5C	 16C	 18	 7	 48
	0.32 - 0.51	 2.4C
	0.51 - 0.71	 1C	 16C	 18	 6	 54
	0.71 - 0.97	 0.68C
	0.97 - 1.14	 0.15C	 14C	 16	 7	 58
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.1
	0.13 - 0.32
	0.32 - 0.51
	0.51 - 0.71
	0.71 - 0.97
	0.97 - 1.14

	Project Name:	Wimmera Rec. & Little Desert, Vic.
	Project Code:	WR	Site ID:	A838	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (VIC)
	Laboratory Analyses Completed for this profile
	19B_NR	Calcium Carbonate (CaCO3) - Not recorded
	2_LOI	Loss on Ignition (%)
	2A1	Air-dry moisture content
	3A_TSS	Electrical conductivity or soluble salts - Total soluble salts %
	4_NR	pH of soil - Not recorded
	5_NR	Water soluble Chloride - Cl(%) - Not recordede
	P10_NR_C	Clay (%) - Not recorded
	P10_NR_CS	Coarse sand (%) - Not recorded
	P10_NR_FS	Fine sand (%) - Not recorded
	P10_NR_Z	Silt (%) - Not recorded