Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	1918	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Site Information
	Desc. By:	Rogers, Gary	Locality:
	Date Desc.:	26/05/93	Elevation:	No Data
	Map Ref.:	Sheet No. : 8255   GPS	Rainfall:	No Data
	Northing/Long.:	7653442 AMG zone: 55	Runoff:	Moderately rapid
	Easting/Lat.:	473910  Datum: AGD66	Drainage:	Imperfectly drained
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	Undisturbed soil core, No Data
	Land Form
	Rel/Slope Class: 	Gently undulating plains <9m  	Pattern Type:	Plain
	1-3%
	Morph. Type:	No Data	Relief:	No Data
	Elem. Type:	Plain	Slope Category:	Very gently sloped
	Slope:	3 % 	Aspect:	No Data
	Surface Soil Condition (dry):	Hardsetting
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Bleached-Mottled Eutrophic Brown Chromosol Thick Non-	Principal Profile Form:	Dy3.42
	gravelly Silty Clayey Deep
	ASC Confidence:	Great Soil Group:	Yellow podzolic soil
	No analytical data are available but confidence is fair.
	Site Disturbance:	No effective disturbance other than grazing by hoofed animals
	Vegetation:	Low Strata - Tussock grass, 0.26-0.5m, Sparse. *Species includes - Aristida species, Heteropogon contortus, 
	Sporobolus species	Mid Strata - Tree, 1.01-3m, Sparse. *Species includes - Eucalyptus crebra, Erythroxylon australe, Acacia salicina
	Tall Strata - Tree, 6.01-12m, Sparse. *Species includes - Eucalyptus crebra, Eucalyptus papuana, Eucalyptus polycarpa
	Surface Coarse Fragments:	No surface coarse fragments
	Profile Morphology
	A11	0 - 0.1 m	Dark yellowish brown (10YR4/4-Moist); ; Silty clay loam (Heavy); Massive grade of structure; 
	Earthy fabric; Dry; Very firm consistence; , Calcareous, , ; , Gypseous, , ; Field pH 6 (Raupach, 
	0.05); Sharp change to - 
	A12	0.1 - 0.2 m	Dark brown (10YR3/3-Moist); ; Sandy clay loam (Heavy); Massive grade of structure; Earthy 
	fabric; Dry; Very firm consistence; , Calcareous, , ; , Gypseous, , ; Field pH 6 (Raupach, 0.15); 
	Clear change to - 
	A2e	0.2 - 0.35 m	Yellowish brown (10YR5/4-Moist); ; Clay loam, sandy; Massive grade of structure; Earthy fabric; 
	Dry; Firm consistence; 0-2%, fine gravelly, 2-6mm, subrounded, Quartz, coarse fragments; , 
	Calcareous, , ; , Gypseous, , ; Field pH 6 (Raupach, 0.3); Clear change to - 
	B21	0.35 - 0.75 m	Yellowish brown (10YR5/6-Moist); Mottles, 5YR56, 10-20% , 15-30mm, Distinct; Mottles, 10-20%
	 ; Sandy light medium clay; Moderate grade of structure, 20-50 mm, Angular blocky; Smooth-ped
	 fabric; Dry; Strong consistence; 0-2%, fine gravelly, 2-6mm, subrounded, Quartz, coarse 
	fragments; Few (2 - 10 %), , Medium (2 -6 mm), Nodules; , Calcareous, , ; , Gypseous, , ; Field 
	pH 6 (Raupach, 0.7); Gradual change to - 
	B22	0.75 - 1.5 m	Olive yellow (2.5Y6/7-Moist); Mottles, 10YR58, 20-50% , 5-15mm, Distinct; Mottles, 20-50% ; 
	Sandy light medium clay; Moderate grade of structure, 10-20 mm, Subangular blocky; Smooth-
	ped fabric; Dry; Strong consistence; 2-10%, fine gravelly, 2-6mm, subrounded, Quartz, coarse 
	fragments; Common (10 - 20 %), , Coarse (6 - 20 mm), Nodules; , Calcareous, , ; , Gypseous, , ; 
	Field pH 7.5 (Raupach, 1.5); 
	Morphological Notes
	Observation Notes
	Site Notes

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	1918	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	1918	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Analyses Completed for this profile