Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	2427	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Site Information
	Desc. By:	Rogers, Gary	Locality:
	Date Desc.:	12/01/94	Elevation:	No Data
	Map Ref.:	Sheet No. : 8158   GPS	Rainfall:	No Data
	Northing/Long.:	7800689 AMG zone: 55	Runoff:	Rapid
	Easting/Lat.:	414978  Datum: AGD66	Drainage:	Moderately well drained
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	Undisturbed soil core, No Data
	Land Form
	Rel/Slope Class: 	Gently undulating plains <9m  1-	Pattern Type:	Plain
	3%
	Morph. Type:	No Data	Relief:	No Data
	Elem. Type:	Plain	Slope Category:	Very gently sloped
	Slope:	2 % 	Aspect:	No Data
	Surface Soil Condition (dry):	Hardsetting
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Vertic Eutrophic Brown Dermosol Medium Slightly gravelly 	Principal Profile Form:	Db1.13
	Clay-loamy Clayey Deep
	ASC Confidence:	Great Soil Group:	Solodic soil
	Analytical data are incomplete but reasonable confidence.
	Site Disturbance:	No effective disturbance other than grazing by hoofed animals
	Vegetation:	Low Strata - Tussock grass, 0.26-0.5m, Very sparse. *Species includes - Bothriochloa ewartiana, Chrysopogon fallax
	Mid Strata - Shrub, 1.01-3m, Mid-dense. *Species includes - Eremophila mitchellii, Terminalia oblongata, Atalaya hemiglauca
	Tall Strata - Tree, 12.01-20m, Very sparse. *Species includes - Eucalyptus brownii
	Surface Coarse Fragments:	2-10%, cobbly, 60-200mm, subrounded, Quartz
	Profile Morphology
	A11	0 - 0.1 m	Brown (10YR4/3-Moist); ; Clay loam, coarse sandy; Massive grade of structure; Earthy fabric; 
	Moderately moist; Strong consistence; 10-20%, medium gravelly, 6-20mm, subangular, Quartz, 
	coarse fragments; Very few (0 - 2 %), Manganiferous, Fine (0 - 2 mm), Nodules; , Calcareous, ,
	 ; , Gypseous, , ; Field pH 6.5 (Raupach, 0.05); Clear change to - 
	B21	0.1 - 0.35 m	Dark brown (10YR3/3-Moist); ; Medium clay; Moderate grade of structure, 10-20 mm, 
	Subangular blocky; Smooth-ped fabric; Dry; Very strong consistence; 10-20%, fine gravelly, 2-
	6mm, subangular, Quartz, coarse fragments; Very few (0 - 2 %), Manganiferous, Fine (0 - 2 
	mm), Nodules; , Calcareous, , ; , Gypseous, , ; Soil matrix is Highly calcareous; Field pH 8.5 
	(Raupach, 0.3); Clear change to - 
	B22	0.35 - 0.8 m	Dark brown (10YR3/3-Moist); ; Medium heavy clay; Moderate grade of structure, 20-50 mm, 
	Subangular blocky; Smooth-ped fabric; Dry; Very strong consistence; 10-20%, fine gravelly, 2-
	6mm, subangular, Quartz, coarse fragments; Few cutans, <10% of ped faces or walls coated; 
	Very few (0 - 2 %), Manganiferous, Medium (2 -6 mm), Nodules; Few (2 - 10 %), Calcareous, 
	Medium (2 -6 mm), Soft segregations; , Gypseous, , ; Field pH 8.5 (Raupach, 0.7); Gradual 
	change to - 
	B23	0.8 - 1.1 m	Greyish brown (2.5Y5/2-Moist); ; Medium heavy clay; Strong grade of structure, 10-20 mm, 
	Subangular blocky; Strong grade of structure, 20-50 mm, Lenticular; Smooth-ped fabric; Dry; 
	Very strong consistence; 2-10%, fine gravelly, 2-6mm, subrounded, Quartz, coarse fragments; 
	Few cutans, <10% of ped faces or walls coated; Few (2 - 10 %), Manganiferous, Medium (2 -6
	 mm), Laminae; , Calcareous, , ; , Gypseous, , ; Field pH 7.5 (Raupach, 1); 
	Morphological Notes
	Observation Notes
	Site Notes

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	2427	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	2427	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Analyses Completed for this profile