Project Name:	APSRU Soil Reference Sites
	Project Code:	APSRU	Site ID:	272	Observation ID:	1
	Agency Name:	CSIRO Sustainable Ecosystems (QLD)
	Site Information
	Desc. By:	Locality:	Characterisation_Site: Maryville (MRV). 
	Farmer_Contact: Mr Lindsay Price
	Date Desc.:	20/06/06	Elevation:	No Data
	Map Ref.:	Rainfall:	No Data
	Northing/Long.:	138.03	Runoff:	No Data
	Easting/Lat.:	-33.989	Drainage:	No Data
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	No Data	Pattern Type:	No Data
	Morph. Type:	No Data	Relief:	No Data
	Elem. Type:	No Data	Slope Category:	No Data
	Slope:	 % 	Aspect:	No Data
	Surface Soil Condition (dry):
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	 N/A    	Principal Profile Form:	N/A
	ASC Confidence:	Great Soil Group:	N/A
	Confidence level not specified
	Site Disturbance:
	Vegetation:
	Surface Coarse Fragments:
	Profile Morphology
	0 - 0.15 m	; 
	0.15 - 0.3 m	; 
	0.3 - 0.5 m	; 
	0.5 - 0.8 m	; 
	0.8 - 1.1 m	; 
	1.1 - 1.5 m	; 
	Morphological Notes
	Observation Notes
	Soil_Classification: Loamy sand over sandy clay loam. Soil_Comments: Low -moderate clay soil with clay content increasing 
	with depth having moderate CEC, low-moderate bulk density and a PAWC of 154mm. Some impediment to root growth below ab
	Site Notes
	Kulpara

	Project Name:	APSRU Soil Reference Sites
	Project Code:	APSRU	Site ID:	272	Observation ID:	1
	Agency Name:	CSIRO Sustainable Ecosystems (QLD)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.15	8.6A	0.2A	11.3H	1.1	0.6	0.4	13.4E	2.99
	0.15 - 0.3	8.7A	0.2A	15.7H	1.7	0.6	0.4	18.4E	2.17
	0.3 - 0.5	8.8A	0.1A	15.9H	2.2	0.4	0.3	18.8E	1.60
	0.5 - 0.8	8.9A	0.1A	12.4H	4.6	0.3	0.3	17.5E	1.71
	0.8 - 1.1	9.2A	0.1A	8.7H	7.3	0.4	0.3	16.7E	1.80
	1.1 - 1.5	9.6A	0.2A	7.4H	8.3	0.7	0.8	17.2E	4.65
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.15	1A	1.56	87I	1	13
	0.15 - 0.3	0.8A	1.46	77I	3	20
	0.3 - 0.5	0.5A	1.37	74I	6	20
	0.5 - 0.8	0.25A	1.39	69I	8	23
	0.8 - 1.1	0.15A	1.40	63I	8	29
	1.1 - 1.5	0.1A	1.55	64I	7	29
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.15
	0.15 - 0.3
	0.3 - 0.5
	0.5 - 0.8
	0.8 - 1.1
	1.1 - 1.5

	Project Name:	APSRU Soil Reference Sites
	Project Code:	APSRU	Site ID:	272	Observation ID:	1
	Agency Name:	CSIRO Sustainable Ecosystems (QLD)
	Laboratory Analyses Completed for this profile
	12C2	Calcium chloride extractable boron - ICPAES
	15E1_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) by compulsive exchange, no pretreatment for soluble 
	15E1_CEC	CEC by compulsive exchange, no pretreatment for soluble salts
	15E1_K	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15E1_MG	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15E1_NA	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15N1	Exchangeable sodium percentage (ESP)
	2A1	Air-dry moisture content
	3A1	EC of 1:5 soil/water extract
	4A1	pH of 1:5 soil/water suspension
	5A2	Chloride - 1:5 soil/water extract, automated colour
	6A1	Organic carbon - Walkley and Black
	P10_NR_C	Clay (%) - Not recorded
	P10_NR_S	Sand (%) - Not recorded
	P10_NR_Z	Silt (%) - Not recorded
	P3A1	Bulk density - g/cm3
	P3B6VL_DUL	Drained Upper Limit (0.1 BAR) Moisture m3/m3 - Volumetric using APSRU in situ methodology
	P3B6VL_LL	Lower Limit (15 BAR) Moisture m3/m3 - Volumetric using APSRU in situ methodology
	P3B6VL_SAT	Saturated Moisture m3/m3 - Volumetric using APSRU in situ methodology