Project Name:	APSRU Soil Reference Sites
	Project Code:	APSRU	Site ID:	274	Observation ID:	1
	Agency Name:	CSIRO Sustainable Ecosystems (QLD)
	Site Information
	Desc. By:	Locality:	Characterisation_Site: Mallalla-Calomba (CAL). 
	Farmer_Contact: Mr Derrick Tiller
	Date Desc.:	20/06/06	Elevation:	No Data
	Map Ref.:	Rainfall:	No Data
	Northing/Long.:	138.491	Runoff:	No Data
	Easting/Lat.:	-34.394	Drainage:	No Data
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	No Data	Pattern Type:	No Data
	Morph. Type:	No Data	Relief:	No Data
	Elem. Type:	No Data	Slope Category:	No Data
	Slope:	 % 	Aspect:	No Data
	Surface Soil Condition (dry):
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	 N/A    	Principal Profile Form:	N/A
	ASC Confidence:	Great Soil Group:	N/A
	Confidence level not specified
	Site Disturbance:
	Vegetation:
	Surface Coarse Fragments:
	Profile Morphology
	0 - 0.1 m	; 
	0.1 - 0.3 m	; 
	0.3 - 0.5 m	; 
	0.5 - 0.8 m	; 
	0.8 - 1.1 m	; 
	1.1 - 1.5 m	; 
	Morphological Notes
	Observation Notes
	Soil_Classification: Loam over Clay. Soil_Comments: Moderate clay soil with moderate-high CEC and PAWC of 90mm. High ESP 
	and elevated levels of boron may impede root growth below about 55cm whilst the pH will also reduce trace element avail
	Site Notes
	Mallala

	Project Name:	APSRU Soil Reference Sites
	Project Code:	APSRU	Site ID:	274	Observation ID:	1
	Agency Name:	CSIRO Sustainable Ecosystems (QLD)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.1	7.7A	0.4A	9.8H	3.1	1.1	1.2	15.1E	7.95
	0.1 - 0.3	8.5A	0.4A	15.8H	10.6	1.5	5.3	33.1E	16.01
	0.3 - 0.5	9.4A	0.4A	14.1H	9.8	1.2	6.8	31.9E	21.32
	0.5 - 0.8	8.7A	1.7A	14.5H	9.5	1.2	7.8	33E	23.64
	0.8 - 1.1	9.1A	0.9A	10.2H	9.3	1.3	10.5	31.3E	33.55
	1.1 - 1.5	9A	0.9A	10.5H	9.9	1.4	11.3	33.2E	34.04
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.1	1A	1.59	55I	17	28
	0.1 - 0.3	0.8A	1.31	30I	15	56
	0.3 - 0.5	0.5A	1.40	32I	21	48
	0.5 - 0.8	0.25A	1.52	30I	23	47
	0.8 - 1.1	0.15A	1.49	26I	21	53
	1.1 - 1.5	0.1A	1.49	24I	19	57
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.1
	0.1 - 0.3
	0.3 - 0.5
	0.5 - 0.8
	0.8 - 1.1
	1.1 - 1.5

	Project Name:	APSRU Soil Reference Sites
	Project Code:	APSRU	Site ID:	274	Observation ID:	1
	Agency Name:	CSIRO Sustainable Ecosystems (QLD)
	Laboratory Analyses Completed for this profile
	12C2	Calcium chloride extractable boron - ICPAES
	15E1_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) by compulsive exchange, no pretreatment for soluble 
	15E1_CEC	CEC by compulsive exchange, no pretreatment for soluble salts
	15E1_K	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15E1_MG	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15E1_NA	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15N1	Exchangeable sodium percentage (ESP)
	2A1	Air-dry moisture content
	3A1	EC of 1:5 soil/water extract
	4A1	pH of 1:5 soil/water suspension
	5A2	Chloride - 1:5 soil/water extract, automated colour
	6A1	Organic carbon - Walkley and Black
	P10_NR_C	Clay (%) - Not recorded
	P10_NR_S	Sand (%) - Not recorded
	P10_NR_Z	Silt (%) - Not recorded
	P3A1	Bulk density - g/cm3
	P3B6VL_DUL	Drained Upper Limit (0.1 BAR) Moisture m3/m3 - Volumetric using APSRU in situ methodology
	P3B6VL_LL	Lower Limit (15 BAR) Moisture m3/m3 - Volumetric using APSRU in situ methodology
	P3B6VL_SAT	Saturated Moisture m3/m3 - Volumetric using APSRU in situ methodology