Project Name:	APSRU Soil Reference Sites
	Project Code:	APSRU	Site ID:	295	Observation ID:	1
	Agency Name:	CSIRO Sustainable Ecosystems (QLD)
	Site Information
	Desc. By:	Locality:	Characterisation_Site: Wally's East (WLE). 
	Farmer_Contact: Mr Kym I'anson
	Date Desc.:	20/07/07	Elevation:	No Data
	Map Ref.:	Rainfall:	No Data
	Northing/Long.:	138.922	Runoff:	No Data
	Easting/Lat.:	-34.103	Drainage:	No Data
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	No Data	Pattern Type:	No Data
	Morph. Type:	No Data	Relief:	No Data
	Elem. Type:	No Data	Slope Category:	No Data
	Slope:	 % 	Aspect:	No Data
	Surface Soil Condition (dry):
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	 N/A    	Principal Profile Form:	N/A
	ASC Confidence:	Great Soil Group:	N/A
	Confidence level not specified
	Site Disturbance:
	Vegetation:
	Surface Coarse Fragments:
	Profile Morphology
	0 - 0.1 m	; 
	0.1 - 0.25 m	; 
	0.25 - 0.4 m	; 
	0.4 - 0.7 m	; 
	0.7 - 1.1 m	; 
	Morphological Notes
	Observation Notes
	Site Notes
	Marabel

	Project Name:	APSRU Soil Reference Sites
	Project Code:	APSRU	Site ID:	295	Observation ID:	1
	Agency Name:	CSIRO Sustainable Ecosystems (QLD)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.1	6.9A	0.4A	16.2E	1.3	0.3	0	17.8K	0.00
	0.1 - 0.25	7A	0.3A	11.7E	1.1	0.3	0	13.1K	0.00
	0.25 - 0.4	7.5A	0.5A	13.9E	10.3	1.2	1.6	26.9K	5.95
	0.4 - 0.7	8.2A	0.6A	14.1E	14.9	1.3	3.3	33.6K	9.82
	0.7 - 1.1	8.7A	0.7A	9.7E	11.2	1	4.3	26.3K	16.35
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.1	1.7A	1.51	20	21
	0.1 - 0.25	1A	1.70	17	24
	0.25 - 0.4	0.6A	1.28	5	76
	0.4 - 0.7	0.4A	1.25	9	73
	0.7 - 1.1	0.3A	1.48	15	62
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.1
	0.1 - 0.25
	0.25 - 0.4
	0.4 - 0.7
	0.7 - 1.1

	Project Name:	APSRU Soil Reference Sites
	Project Code:	APSRU	Site ID:	295	Observation ID:	1
	Agency Name:	CSIRO Sustainable Ecosystems (QLD)
	Laboratory Analyses Completed for this profile
	12C2	Calcium chloride extractable boron - ICPAES
	15C1_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - alcoholic 1M ammonium chloride at pH 8.5, pretreatment 
	for soluble salts
	15C1_K	Exchangeable bases and CEC - alcoholic 1M ammonium chloride at pH 8.5, pretreatment for soluble 
	salts
	15C1_MG	Exchangeable bases and CEC - alcoholic 1M ammonium chloride at pH 8.5, pretreatment for soluble 
	salts
	15C1_NA	Exchangeable bases and CEC - alcoholic 1M ammonium chloride at pH 8.5, pretreatment for soluble 
	salts
	15I3	CEC measurement - automated determination of ammonium and chloride ions
	15N1	Exchangeable sodium percentage (ESP)
	2A1	Air-dry moisture content
	3A1	EC of 1:5 soil/water extract
	4A1	pH of 1:5 soil/water suspension
	5A2	Chloride - 1:5 soil/water extract, automated colour
	6A1	Organic carbon - Walkley and Black
	P10_HYD_C	Clay (%) - Hydrometer Method
	P10_HYD_S	Sand (%) - Hydrometer Method
	P10_HYD_Z	Silt (%) - Hydrometer Method
	P3A1	Bulk density - g/cm3
	P3B6VL_DUL	Drained Upper Limit (0.1 BAR) Moisture m3/m3 - Volumetric using APSRU in situ methodology
	P3B6VL_LL	Lower Limit (15 BAR) Moisture m3/m3 - Volumetric using APSRU in situ methodology
	P3B6VL_SAT	Saturated Moisture m3/m3 - Volumetric using APSRU in situ methodology