Project Name:	BB
	Project Code:	BB	Site ID:	B344	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Site Information
	Desc. By:	G.G. Beckmann	Locality:
	Date Desc.:	28/03/58	Elevation:	 40 metres
	Map Ref.:	Sheet No. : 9542   1:100000	Rainfall:	1384
	Northing/Long.:	153.242777777778	Runoff:	Moderately rapid
	Easting/Lat.:	-27.6155555555556	Drainage:	Moderately well drained
	Geology
	ExposureType:	Soil pit	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	 Pzn	Substrate Material:	Soil pit, 0.79 m deep,Mudstone 
	Land Form
	Rel/Slope Class: 	No Data	Pattern Type:	No Data
	Morph. Type:	Crest	Relief:	15 metres
	Elem. Type:	Hillcrest	Slope Category:	No Data
	Slope:	0 % 	Aspect:	No Data
	Surface Soil Condition (dry):	Hardsetting
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Bleached-Mottled Magnesic-Natric Red Kurosol     	Principal Profile Form:	Dr3.41
	ASC Confidence:	Great Soil Group:	Red podzolic soil
	All necessary analytical data are available.
	Site Disturbance:	Limited clearing, for example selective logging
	Vegetation:	Low Strata - Tussock grass, , . *Species includes - Aristida species
	Tall Strata - Tree, 6.01-12m, Mid-dense. *Species includes - None Recorded
	Surface Coarse Fragments:	10-20%, , angular, Quartz
	Profile Morphology
	A1	0 - 0.02 m	Very dark grey (10YR3/1-Moist); ; Loam; Massive grade of structure; Moist; Very weak 
	consistence; 2-10%, fine gravelly, 2-6mm, Quartz, coarse fragments; Field pH 5.4 (pH meter); 
	Many, very fine (0-1mm) roots; Abrupt change to - 
	A21	0.02 - 0.08 m	Pale yellow (2.5Y7/4-Moist); ; Loam; Massive grade of structure; Moist; Weak consistence; 20-
	50%, medium gravelly, 6-20mm, Quartz, coarse fragments; Field pH 5.4 (pH meter); Common, 
	very fine (0-1mm) roots; Gradual change to - 
	A22	0.08 - 0.16 m	Pale yellow (2.5Y7/4-Moist); , 10YR76, 0-2% , Faint; , 0-2% , Faint; Loam; Massive grade of 
	structure; Moist; Weak consistence; 20-50%, medium gravelly, 6-20mm, Quartz, coarse 
	fragments; Field pH 5.5 (pH meter); Clear change to - 
	B1	0.16 - 0.21 m	Red (2.5YR4/6-Moist); , 2.5Y74, 10-20% , Distinct; , 10-20% , Distinct; Light clay; Moderate 
	grade of structure, 10-20 mm, Angular blocky; Moist; Firm consistence; 2-10%, Quartz, coarse 
	fragments; Field pH 5.4 (pH meter); Gradual change to - 
	B21	0.22 - 0.35 m	Red (2.5YR4/8-Moist); , 2.5Y74, 10-20% , Distinct; , 10-20% , Distinct; Heavy clay; Moderate 
	grade of structure, 10-20 mm, Angular blocky; Moist; Firm consistence; 2-10%, Substrate 
	material, coarse fragments; Field pH 5.3 (pH meter); Gradual change to - 
	B22	0.36 - 0.56 m	Red (2.5YR4/8-Moist); , 2.5Y52, 10-20% , Distinct; , 10-20% , Distinct; Heavy clay; Moist; Firm 
	consistence; 10-20%, Substrate material, coarse fragments; Field pH 5.1 (pH meter); Diffuse 
	change to - 
	B3	0.56 - 0.74 m	Grey (10YR6/1-Moist); , 2.5Y52, 10-20% , Prominent; , 2.5YR48, 10-20% , Prominent; Heavy 
	clay; Moist; Weak consistence; 10-20%, Shale, coarse fragments; Field pH 5 (pH meter); 
	C	0.79 - 0.87 m	; 
	C	0.87 - 0.91 m	; 
	Morphological Notes
	Observation Notes
	Site Notes
	MT COTTON

	Project Name:	BB
	Project Code:	BB	Site ID:	B344	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)

	Project Name:	BB
	Project Code:	BB	Site ID:	B344	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.02	5.4H	 0.02C
	0.02 - 0.08	5.4H	 0.02C	 0.51K	 0.31	 0.28	 0.09	 4.5J	2.00
	0.08 - 0.16	5.5H	 0.01C
	0.16 - 0.21	5.4H	 0.01C
	0.22 - 0.35	5.3H	 0.02C	 0.1K	 2.9	 0.12	 0.23	 16.5J	1.39
	0.36 - 0.56	5.1H	 0.02C	 0.02K	 3	 0.06	 0.25	 20.4J	1.23
	0.56 - 0.74	5H	 0.03C
	0.79 - 0.87	4.9H	 0.03C
	0.87 - 0.91	4.9H	 0.03C
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.02	 15C	 0.024F
	0.02 - 0.08	 2.13E	 2C	 0.009F	 0.08B	 42	 2C	 19	 66	 13
	0.08 - 0.16	 0.61E	 43	 16C	 29	 45	 12
	0.16 - 0.21	 6	 10C	 21	 40	 32
	0.22 - 0.35	 0.013F	 7	 6C	 12	 27	 56
	0.36 - 0.56	 11	 4C	 9	 27	 63
	0.56 - 0.74	 0.011F
	0.79 - 0.87	 33
	0.87 - 0.91	 60
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.02
	0.02 - 0.08
	0.08 - 0.16
	0.16 - 0.21
	0.22 - 0.35
	0.36 - 0.56
	0.56 - 0.74
	0.79 - 0.87
	0.87 - 0.91

	Project Name:	BB
	Project Code:	BB	Site ID:	B344	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Analyses Completed for this profile
	15_NR_CA	Exch. basic cations (Ca++) - meq per 100g of soil - Not recorded
	15_NR_CEC	CEC - meq per 100g of soil - Not recorded
	15_NR_K	Exch. basic cations (K++) - meq per 100g of soil - Not recorded
	15_NR_MG	Exch. basic cations (Mg++) - meq per 100g of soil - Not recorded
	15_NR_NA	Exch. basic cations (Na++) - meq per 100g of soil - Not recorded
	2A1	Air-dry moisture content
	3A_TSS	Electrical conductivity or soluble salts - Total soluble salts %
	4_NR	pH of soil - Not recorded
	5_NR	Water soluble Chloride - Cl(%) - Not recordede
	6Z	Organic carbon (%) - Not recorded
	7_NR	Total nitrogen (%) - Not recorded
	9_NR	Available P (mg/kg) - Not recorded
	9A_NR	Total element - P(%) - Not recorded
	P10_GRAV	Gravel (%)
	P10_NR_C	Clay (%) - Not recorded
	P10_NR_CS	Coarse sand (%) - Not recorded
	P10_NR_FS	Fine sand (%) - Not recorded
	P10_NR_Z	Silt (%) - Not recorded