Project Name:	BB
	Project Code:	BB	Site ID:	B352	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Site Information
	Desc. By:	G.G. Beckmann	Locality:
	Date Desc.:	28/05/58	Elevation:	 15 metres
	Map Ref.:	Sheet No. : 9542   1:100000	Rainfall:	1194
	Northing/Long.:	153.146666666667	Runoff:	Very slow
	Easting/Lat.:	-27.7366666666667	Drainage:	Imperfectly drained
	Geology
	ExposureType:	Soil pit	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	 Pzn	Substrate Material:	Auger boring, 2 m deep,Clay 
	Land Form
	Rel/Slope Class: 	No Data	Pattern Type:	Terrace (alluvial)
	Morph. Type:	No Data	Relief:	12 metres
	Elem. Type:	No Data	Slope Category:	No Data
	Slope:	0 % 	Aspect:	No Data
	Surface Soil Condition (dry):
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Epiacidic Epipedal Grey Vertosol     	Principal Profile Form:	Gn3.91
	ASC Confidence:	Great Soil Group:	Grey clay
	All necessary analytical data are available.
	Site Disturbance:	Complete clearing. Pasture, native or improved, but never cultivated
	Vegetation:	Low Strata - Tussock grass, , . *Species includes - Imperata cylindrica
	Tall Strata - Tree, 6.01-12m, Isolated plants. *Species includes - None Recorded
	Surface Coarse Fragments:	No surface coarse fragments
	Profile Morphology
	A1	0 - 0.05 m	Olive grey (5Y5/2-Moist); ; Light clay; Moderate grade of structure, 2-5 mm, Granular; Moist; 
	Weak consistence; Very few (0 - 2 %), Ferruginous, Medium (2 -6 mm), Nodules; Field pH 4.4 
	(pH meter); Few, very fine (0-1mm) roots; Abrupt change to - 
	B21	0.05 - 0.3 m	Dark greyish brown (2.5Y4/2-Moist); ; Heavy clay; Moderate grade of structure, 10-20 mm, 
	Angular blocky; Moist; Firm consistence; Very few (0 - 2 %), Manganiferous, Fine (0 - 2 mm), 
	Nodules; Field pH 5.6 (pH meter); Gradual change to - 
	B22	0.3 - 0.45 m	Dark greyish brown (2.5Y4/2-Moist); , 10YR51; Heavy clay; Weak grade of structure, 20-50 
	mm, Angular blocky; Moist; Moderately plastic; Very few (0 - 2 %), Manganiferous, Medium (2 -
	6 mm), Nodules; Field pH 5.2 (pH meter); Gradual change to - 
	B23	0.45 - 0.9 m	Greyish brown (10YR5/2-Moist); ; Heavy clay; Weak grade of structure, 20-50 mm, Angular 
	blocky; Moist; Moderately plastic; Very few (0 - 2 %), Manganiferous, Medium (2 -6 mm), 
	Nodules; Field pH 4.7 (pH meter); Gradual change to - 
	B24	0.9 - 1.2 m	Greyish brown (10YR5/2-Moist); ; Heavy clay; Massive grade of structure; Moist; Moderately 
	plastic; Field pH 4.4 (pH meter); Gradual change to - 
	BC	1.3 - 1.83 m	Light grey (2.5Y7/2-Moist); , 2.5Y76; Heavy clay; Massive grade of structure; Moist; Moderately
	 plastic; Field pH 4.7 (pH meter); Gradual change to - 
	C	1.83 - 2.13 m	; Heavy clay; 
	C	2.13 - 2.87 m	; Heavy clay; 
	C	2.97 - 3.28 m	; Heavy clay; 
	C	3.28 - 3.73 m	; Heavy clay; 
	C	3.73 - 4.57 m	; Heavy clay; 
	Morphological Notes
	C	Layer continues
	Observation Notes
	CLASSIFIED AS GREY CLAY - ACID VARIANT:                                                                                 

	Project Name:	BB
	Project Code:	BB	Site ID:	B352	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Site Notes
	LOGANLEA

	Project Name:	BB
	Project Code:	BB	Site ID:	B352	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.05	4.4H	 0.03C
	0.05 - 0.3	5.6H	 0.01C	 1.3K	 6.2	 0.07	 1.3	 28J	4.64
	0.3 - 0.45	5.2H	 0.03C
	0.45 - 0.9	4.7H	 0.09C	 0.05K	 13.2	 0.15	 3.7	 40.9J	9.05
	0.9 - 1.2	4.4H	 0.18C
	1.3 - 1.83	4.7H	 0.19C
	1.83 - 2.13	4.7H	 0.24C
	2.13 - 2.87
	2.97 - 3.28
	3.28 - 3.73
	3.73 - 4.57
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.05	 3.47E	 6C	 1	 5C	 7	 39	 41
	0.05 - 0.3	 1.62E	<1C	 0.1B	 2C	 4	 31	 61
	0.3 - 0.45
	0.45 - 0.9	 0.28E	 0.01F	 1C	 5	 21	 76
	0.9 - 1.2
	1.3 - 1.83	 0.01F
	1.83 - 2.13
	2.13 - 2.87
	2.97 - 3.28
	3.28 - 3.73
	3.73 - 4.57
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.05
	0.05 - 0.3
	0.3 - 0.45
	0.45 - 0.9
	0.9 - 1.2
	1.3 - 1.83
	1.83 - 2.13
	2.13 - 2.87
	2.97 - 3.28
	3.28 - 3.73
	3.73 - 4.57

	Project Name:	BB
	Project Code:	BB	Site ID:	B352	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Analyses Completed for this profile
	15_NR_CA	Exch. basic cations (Ca++) - meq per 100g of soil - Not recorded
	15_NR_CEC	CEC - meq per 100g of soil - Not recorded
	15_NR_K	Exch. basic cations (K++) - meq per 100g of soil - Not recorded
	15_NR_MG	Exch. basic cations (Mg++) - meq per 100g of soil - Not recorded
	15_NR_NA	Exch. basic cations (Na++) - meq per 100g of soil - Not recorded
	2A1	Air-dry moisture content
	3A_TSS	Electrical conductivity or soluble salts - Total soluble salts %
	4_NR	pH of soil - Not recorded
	5_NR	Water soluble Chloride - Cl(%) - Not recordede
	6Z	Organic carbon (%) - Not recorded
	7_NR	Total nitrogen (%) - Not recorded
	9_NR	Available P (mg/kg) - Not recorded
	9A_NR	Total element - P(%) - Not recorded
	P10_GRAV	Gravel (%)
	P10_NR_C	Clay (%) - Not recorded
	P10_NR_CS	Coarse sand (%) - Not recorded
	P10_NR_FS	Fine sand (%) - Not recorded
	P10_NR_Z	Silt (%) - Not recorded