Project Name:	BL
	Project Code:	BL	Site ID:	B321	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Site Information
	Desc. By:	G.D. Hubble	Locality:
	Date Desc.:	01/07/57	Elevation:	 329 metres
	Map Ref.:	Sheet No. : 8943   1:100000	Rainfall:	584
	Northing/Long.:	150.490277777778	Runoff:	Moderately rapid
	Easting/Lat.:	-27.4388888888889	Drainage:	Imperfectly drained
	Geology
	ExposureType:	Soil pit	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	   T	Substrate Material:	Soil pit, 0.97 m deep,Unconsolidated 
	material (unidentified) 
	Land Form
	Rel/Slope Class: 	No Data	Pattern Type:	Plateau
	Morph. Type:	No Data	Relief:	24 metres
	Elem. Type:	Plain	Slope Category:	No Data
	Slope:	0 % 	Aspect:	No Data
	Surface Soil Condition (dry):	Hardsetting
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Bleached Magnesic-Natric Black Kurosol     	Principal Profile Form:	Dd1.41
	ASC Confidence:	Great Soil Group:	Soloth
	All necessary analytical data are available.
	Site Disturbance:
	Vegetation:	Low Strata - Tussock grass, , . *Species includes - Aristida species
	Tall Strata - Tree, 6.01-12m, Mid-dense. *Species includes - Eucalyptus crebra
	Surface Coarse Fragments:	No surface coarse fragments
	Profile Morphology
	A1	0 - 0.06 m	Brown (7.5YR4/3-Moist); ; Loam; Massive grade of structure; Many (>5 per 0.01m2) Medium (2-
	5mm) macropores, Moderately moist; Weak consistence; 0-2%, fine gravelly, 2-6mm, Substrate 
	material, coarse fragments; Field pH 5.7 (pH meter); Clear change to - 
	A2	0.09 - 0.14 m	Very pale brown (10YR7/3-Moist); ; Fine sandy loam (Heavy); Massive grade of structure; 
	Many (>5 per 100mm2) Very fine (0.075-1mm) macropores, Moderately moist; Weak 
	consistence; 2-10%, fine gravelly, 2-6mm, Substrate material, coarse fragments; Field pH 5.2 
	(pH meter); Abrupt change to - 
	B21	0.14 - 0.28 m	Dark reddish brown (5YR3/2-Moist); ; Medium heavy clay; Moderate grade of structure, 100-
	200 mm, Columnar; Strong grade of structure, 10-20 mm, Columnar; Moist; Very firm 
	consistence; 0-2%, medium gravelly, 6-20mm, Substrate material, coarse fragments; Field pH 
	4.9 (pH meter); Gradual change to - 
	B22	0.3 - 0.46 m	Dark reddish brown (5YR3/2-Moist); ; Medium heavy clay; Moderate grade of structure, 20-50 
	mm, Angular blocky; Moist; Very firm consistence; 2-10%, medium gravelly, 6-20mm, angular, 
	Substrate material, coarse fragments; Field pH 4.3 (pH meter); Gradual change to - 
	B3	0.51 - 0.91 m	Dark reddish brown (5YR3/2-Moist); ; Medium heavy clay; Moderate grade of structure, Angular
	 blocky; Firm consistence; 10-20%, cobbly, 60-200mm, angular, Substrate material, coarse 
	fragments; Field pH 4.1 (pH meter); Gradual change to - 
	C	0.97 - 0.99 m	; Field pH 4.5 (pH meter); 
	Morphological Notes
	C	Mottled LR + W + YB fragmented hardened mottled zone rock:
	Observation Notes
	LOW PLATEAU                                                                                                             
	Site Notes
	TARA

	Project Name:	BL
	Project Code:	BL	Site ID:	B321	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.06	5.7H	 0.03B	 4.6K	 5.2	 1	 0.7	 20.6J	3.40
	0.09 - 0.14	5.2H	 0.02B
	0.14 - 0.28	4.9H	 0.05B	 0.44K	 10.5	 0.69	 4.1	 41.8J	9.81
	0.3 - 0.46	4.3H	 0.19B
	0.51 - 0.91	4.1H	 0.46B	 13.2	 0.41	 7.4	 46.5J	15.91
	0.97 - 0.99	4.5H	 0.26B
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.06	 2.58E	 32C	 0.028F	 0.19B	 2	 11C	 51	 13	 18
	0.09 - 0.14	 0.76E	 4	 12C	 57	 16	 14
	0.14 - 0.28	 0.57E	 0.024F	 2	 6C	 23	 11	 63
	0.3 - 0.46	 3	 6C	 28	 15	 50
	0.51 - 0.91	 18	 4C	 20	 15	 61
	0.97 - 0.99	 0.003F	 14C	 43	 20	 25
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.06
	0.09 - 0.14
	0.14 - 0.28
	0.3 - 0.46
	0.51 - 0.91
	0.97 - 0.99

	Project Name:	BL
	Project Code:	BL	Site ID:	B321	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Analyses Completed for this profile
	15_NR_CA	Exch. basic cations (Ca++) - meq per 100g of soil - Not recorded
	15_NR_CEC	CEC - meq per 100g of soil - Not recorded
	15_NR_K	Exch. basic cations (K++) - meq per 100g of soil - Not recorded
	15_NR_MG	Exch. basic cations (Mg++) - meq per 100g of soil - Not recorded
	15_NR_NA	Exch. basic cations (Na++) - meq per 100g of soil - Not recorded
	2A1	Air-dry moisture content
	3_NR	Electrical conductivity or soluble salts - Not recorded
	4_NR	pH of soil - Not recorded
	5_NR	Water soluble Chloride - Cl(%) - Not recordede
	6Z	Organic carbon (%) - Not recorded
	7_NR	Total nitrogen (%) - Not recorded
	9_NR	Available P (mg/kg) - Not recorded
	9A_NR	Total element - P(%) - Not recorded
	P10_GRAV	Gravel (%)
	P10_NR_C	Clay (%) - Not recorded
	P10_NR_CS	Coarse sand (%) - Not recorded
	P10_NR_FS	Fine sand (%) - Not recorded
	P10_NR_Z	Silt (%) - Not recorded