Project Name:	CB
	Project Code:	CB	Site ID:	B373	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Site Information
	Desc. By:	C.J. de Mooy	Locality:
	Date Desc.:	22/04/59	Elevation:	 143 metres
	Map Ref.:	Sheet No. : 9246   1:100000	Rainfall:	762
	Northing/Long.:	151.623888888889	Runoff:	Moderately rapid
	Easting/Lat.:	-25.5494444444445	Drainage:	Imperfectly drained
	Geology
	ExposureType:	Soil pit	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	  Rg	Substrate Material:	Soil pit, 0.53 m deep,Detrital sedimentary 
	rock (unidentified) 
	Land Form
	Rel/Slope Class: 	Undulating plains <9m 3-10%	Pattern Type:	Plain
	Morph. Type:	Mid-slope	Relief:	12 metres
	Elem. Type:	Hillslope	Slope Category:	No Data
	Slope:	7 % 	Aspect:	No Data
	Surface Soil Condition (dry):	Hardsetting
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Hypocalcic Mottled-Subnatric Red Sodosol     	Principal Profile Form:	Dr3.33
	ASC Confidence:	Great Soil Group:	Solodized 
	Analytical data are incomplete but reasonable confidence.	solonetz
	Site Disturbance:	No effective disturbance other than grazing by hoofed animals
	Vegetation:
	Tall Strata - Tree, 6.01-12m, Mid-dense. *Species includes - Eucalyptus species, Acacia species
	Surface Coarse Fragments:	No surface coarse fragments
	Profile Morphology
	A1	0 - 0.1 m	Very dark grey (10YR3/1-Moist); , 10YR51; Loam; Massive grade of structure; Dry; Firm 
	consistence; 2-10%, medium gravelly, 6-20mm, Quartz, coarse fragments; Field pH 6.2 (pH 
	meter); Abrupt change to - 
	B2	0.1 - 0.23 m	Dark reddish brown (2.5YR3/4-Moist); , 5YR32; Heavy clay; Strong grade of structure, 50-100 
	mm, Columnar; Moderately moist; Strong consistence; 0-2%, fine gravelly, 2-6mm, Quartz, 
	coarse fragments; Field pH 6.4 (pH meter); Gradual change to - 
	B2	0.23 - 0.41 m	Light olive brown (2.5Y5/4-Moist); ; Heavy clay; Moderate grade of structure, 10-20 mm, 
	Angular blocky; Moderately moist; Strong consistence; 0-2%, fine gravelly, 2-6mm, Quartz, 
	coarse fragments; Very few (0 - 2 %), Calcareous, , Soft segregations; Field pH 8.3 (pH 
	meter); Gradual change to - 
	BC	0.41 - 0.53 m	Light olive brown (2.5Y5/4-Moist); ; Medium clay; Weak grade of structure, 10-20 mm, Angular 
	blocky; Moderately moist; Very firm consistence; Few (2 - 10 %), Calcareous, , Nodules; Field 
	pH 9.2 (pH meter); Gradual change to - 
	C	0.53 - 0.65 m	; Field pH 9.4 (pH meter); 
	Morphological Notes
	C	YG Weathered rock with carbonates + clay pockets:
	Observation Notes
	Site Notes
	CENTRAL BURNET

	Project Name:	CB
	Project Code:	CB	Site ID:	B373	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.1	6.2H	 0.02C	 5.7K	 4	 0.51	 0.65	 17.6J	3.69
	0.1 - 0.23	6.4H	 0.08C	 10.7K	 16.3	 0.26	 3.1	 37.1J	8.36
	0.23 - 0.41	8.3H	 0.22C
	0.41 - 0.53	9.2H	 0.29C	 5.7K	 15.4	 0.21	 4.7
	0.53 - 0.65	9.4H	 0.31C
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.1	 1.6E	 8C	 0.038F	 0.14B	1.50	 2	 14C	 40	 24	 19
	0.1 - 0.23	 0.9E	 0.028F	 0.09B	1.40	 1	 6C	 22	 17	 53
	0.23 - 0.41
	0.41 - 0.53	 6.3C	 2C	 23	 27	 44
	0.53 - 0.65
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.1	 0.31C	 0.21C
	0.1 - 0.23	 0.43C	 0.34C
	0.23 - 0.41
	0.41 - 0.53
	0.53 - 0.65

	Project Name:	CB
	Project Code:	CB	Site ID:	B373	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Analyses Completed for this profile
	15_NR_CA	Exch. basic cations (Ca++) - meq per 100g of soil - Not recorded
	15_NR_CEC	CEC - meq per 100g of soil - Not recorded
	15_NR_K	Exch. basic cations (K++) - meq per 100g of soil - Not recorded
	15_NR_MG	Exch. basic cations (Mg++) - meq per 100g of soil - Not recorded
	15_NR_NA	Exch. basic cations (Na++) - meq per 100g of soil - Not recorded
	19B_NR	Calcium Carbonate (CaCO3) - Not recorded
	2A1	Air-dry moisture content
	3A_TSS	Electrical conductivity or soluble salts - Total soluble salts %
	4_NR	pH of soil - Not recorded
	5_NR	Water soluble Chloride - Cl(%) - Not recordede
	6Z	Organic carbon (%) - Not recorded
	7_NR	Total nitrogen (%) - Not recorded
	9_NR	Available P (mg/kg) - Not recorded
	9A_NR	Total element - P(%) - Not recorded
	P10_GRAV	Gravel (%)
	P10_NR_C	Clay (%) - Not recorded
	P10_NR_CS	Coarse sand (%) - Not recorded
	P10_NR_FS	Fine sand (%) - Not recorded
	P10_NR_Z	Silt (%) - Not recorded
	P3A_NR	Bulk density - Not recorded
	P3B_VL_01	0.1 BAR Moisture m3/m3 - Volumetric using suction plate
	P3B_VL_15	15 BAR Moisture m3/m3 - Volumetric using pressure plate