Project Name:	CB
	Project Code:	CB	Site ID:	B384	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Site Information
	Desc. By:	C.J. de Mooy	Locality:
	Date Desc.:	25/04/59	Elevation:	 110 metres
	Map Ref.:	Sheet No. : 9240   1:100000	Rainfall:	762
	Northing/Long.:	151.751388888889	Runoff:	Slow
	Easting/Lat.:	-25.5144444444445	Drainage:	Imperfectly drained
	Geology
	ExposureType:	Soil pit	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	Czua	Substrate Material:	Auger boring, 1 m deep,Unconsolidated 
	material (unidentified) 
	Land Form
	Rel/Slope Class: 	Undulating rises 9-30m 3-10%	Pattern Type:	Rises
	Morph. Type:	No Data	Relief:	No Data
	Elem. Type:	Plain	Slope Category:	No Data
	Slope:	0 % 	Aspect:	No Data
	Surface Soil Condition (dry):	Hardsetting
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Vertic Subnatric Black Sodosol     	Principal Profile Form:	Dd1.13
	ASC Confidence:	Great Soil Group:	Solodic soil
	All necessary analytical data are available.
	Site Disturbance:	No effective disturbance other than grazing by hoofed animals
	Vegetation:
	Tall Strata - Tree, 6.01-12m, Sparse. *Species includes - Eucalyptus species
	Surface Coarse Fragments:	No surface coarse fragments
	Profile Morphology
	A1	0 - 0.05 m	Very dark grey (10YR3/1-Moist); ; Clay loam; Massive grade of structure; Dry; Firm 
	consistence; Field pH 6.5 (pH meter); Abrupt change to - 
	B2	0.05 - 0.23 m	Black (10YR2/1-Moist); ; Medium clay; Moderate grade of structure, Angular blocky; Dry; Very 
	firm consistence; Field pH 6.9 (pH meter); Gradual change to - 
	B2	0.23 - 0.38 m	Black (10YR2/1-Moist); ; Medium clay; Moderate grade of structure, Angular blocky; Moist; Firm 
	consistence; Field pH 8 (pH meter); Gradual change to - 
	0.46 - 0.61 m	Dark grey (10YR4/1-Moist); ; Light clay; Weak grade of structure, Angular blocky; Weak 
	consistence; Field pH 8.3 (pH meter); Gradual change to - 
	0.76 - 0.91 m	Greyish brown (10YR5/2-Moist); ; Light clay; Weak grade of structure, Angular blocky; Weak 
	consistence; Very few (0 - 2 %), Calcareous, , Nodules; Field pH 8.8 (pH meter); 
	Morphological Notes
	Observation Notes
	DEGRADED BLACK EARTH : 0-5CM DRIES LIGHT GREY:                                                                          
	Site Notes
	CENTRAL BURNET

	Project Name:	CB
	Project Code:	CB	Site ID:	B384	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.05	6.5H	 0.04C	 5K	 4.5	 0.27	 1	 16.5J	6.06
	0.05 - 0.23	6.9H	 0.09C	 11.7K	 13.8	 0.13	 4.6	 34.6J	13.29
	0.23 - 0.38	8H	 0.23C
	0.46 - 0.61	8.3H	 0.27C
	0.76 - 0.91	8.8H	 0.3C	 5.9K	 13.3	 0.15	 5.8
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.05	 1.2E	 10C	 0.013F	 0.1B	1.40	 7C	 30	 44	 19
	0.05 - 0.23	 1E	 4C	 0.009F	 0.1B	1.30	 3C	 18	 35	 45
	0.23 - 0.38
	0.46 - 0.61
	0.76 - 0.91	 1C	 7C	 21	 36	 38
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.05	 0.32C
	0.05 - 0.23	 0.45C
	0.23 - 0.38
	0.46 - 0.61
	0.76 - 0.91

	Project Name:	CB
	Project Code:	CB	Site ID:	B384	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Analyses Completed for this profile
	15_NR_CA	Exch. basic cations (Ca++) - meq per 100g of soil - Not recorded
	15_NR_CEC	CEC - meq per 100g of soil - Not recorded
	15_NR_K	Exch. basic cations (K++) - meq per 100g of soil - Not recorded
	15_NR_MG	Exch. basic cations (Mg++) - meq per 100g of soil - Not recorded
	15_NR_NA	Exch. basic cations (Na++) - meq per 100g of soil - Not recorded
	19B_NR	Calcium Carbonate (CaCO3) - Not recorded
	2A1	Air-dry moisture content
	3A_TSS	Electrical conductivity or soluble salts - Total soluble salts %
	4_NR	pH of soil - Not recorded
	5_NR	Water soluble Chloride - Cl(%) - Not recordede
	6Z	Organic carbon (%) - Not recorded
	7_NR	Total nitrogen (%) - Not recorded
	9_NR	Available P (mg/kg) - Not recorded
	9A_NR	Total element - P(%) - Not recorded
	P10_NR_C	Clay (%) - Not recorded
	P10_NR_CS	Coarse sand (%) - Not recorded
	P10_NR_FS	Fine sand (%) - Not recorded
	P10_NR_Z	Silt (%) - Not recorded
	P3A_NR	Bulk density - Not recorded
	P3B_VL_01	0.1 BAR Moisture m3/m3 - Volumetric using suction plate