Project Name:	CB
	Project Code:	CB	Site ID:	B401	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Site Information
	Desc. By:	C.J. de Mooy	Locality:
	Date Desc.:	19/05/59	Elevation:	 143 metres
	Map Ref.:	Sheet No. : 9246   1:100000	Rainfall:	762
	Northing/Long.:	151.778888888889	Runoff:	Moderately rapid
	Easting/Lat.:	-25.5127777777778	Drainage:	Well drained
	Geology
	ExposureType:	Soil pit	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	 Pgp	Substrate Material:	Soil pit, 0.53 m deep,No Data
	Land Form
	Rel/Slope Class: 	Undulating rises 9-30m 3-10%	Pattern Type:	No Data
	Morph. Type:	No Data	Relief:	No Data
	Elem. Type:	Hillslope	Slope Category:	No Data
	Slope:	0 % 	Aspect:	No Data
	Surface Soil Condition (dry):	Hardsetting
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Haplic Eutrophic Red Chromosol     	Principal Profile Form:	Dr2.12
	ASC Confidence:	Great Soil Group:	No suitable 
	All necessary analytical data are available.
	Site Disturbance:	No effective disturbance other than grazing by hoofed animals
	Vegetation:
	Tall Strata - Tree, , Mid-dense. *Species includes - Eucalyptus polycarpa
	Surface Coarse Fragments:	No surface coarse fragments
	Profile Morphology
	A1	0 - 0.18 m	Brown (7.5YR4/2-Moist); ; Loam (Light); Massive grade of structure; Moderately moist; Weak 
	consistence; Field pH 6.6 (pH meter); Clear change to - 
	B1	0.18 - 0.25 m	Reddish brown (5YR4/3-Moist); ; Sandy clay loam; Weak grade of structure, 10-20 mm, Angular
	 blocky; Moderately moist; Firm consistence; Field pH 6.6 (pH meter); Clear change to - 
	B2	0.25 - 0.38 m	Reddish brown (5YR4/3-Moist); ; Light clay; Moderate grade of structure, 20-50 mm, Angular 
	blocky; Moderately moist; Firm consistence; Field pH 6.9 (pH meter); Gradual change to - 
	B3	0.38 - 0.53 m	Reddish brown (2.5YR4/4-Moist); , 5YR44; Light clay; Moderate grade of structure, 20-50 mm, 
	Angular blocky; Moderately moist; Firm consistence; Field pH 7.1 (pH meter); Gradual change to 
	- 
	C	0.53 - 0.64 m	; Field pH 7.3 (pH meter); 
	Morphological Notes
	C	Yellow brown weathered rock.
	Observation Notes
	18-38CM PED SURFACES ARE 5YR4/4: 38-53CM INCLUDES POCKETS OF WEATHERED ROCK:                                            
	Site Notes
	CENTRAL BURNET

	Project Name:	CB
	Project Code:	CB	Site ID:	B401	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.18	6.6H	 0.01B	 5K	 3.3	 0.14	 0.1	 2.7D	 11J	0.91
	0.18 - 0.25	6.6H	 0.01B	 8K	 6.5	 0.15	 0.19	 6.4D	 21J	0.90
	0.25 - 0.38	6.9H	 0.01B	 12K	 11.1	 0.15	 0.32	 1.7D	 26J	1.23
	0.38 - 0.53	7.1H	 0.01B
	0.53 - 0.64	7.3H	 0.01B
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.18	 0.6A	 4C	 0.013F	 0.06B	1.50	 0	 25C	 49	 10	 14
	0.18 - 0.25	 0.6A	 2C	 0.012F	 0.06B	1.60	 0	 19C	 45	 10	 26
	0.25 - 0.38	 0.5A	 2C	 0.013F	1.50	 0	 13C	 38	 11	 40
	0.38 - 0.53
	0.53 - 0.64	 370C	 0.058F
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.18	 0.15C	 0.1C
	0.18 - 0.25	 0.27C	 0.16C
	0.25 - 0.38	 0.37C	 0.27C
	0.38 - 0.53
	0.53 - 0.64

	Project Name:	CB
	Project Code:	CB	Site ID:	B401	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Analyses Completed for this profile
	15_NR_CA	Exch. basic cations (Ca++) - meq per 100g of soil - Not recorded
	15_NR_CEC	CEC - meq per 100g of soil - Not recorded
	15_NR_H	Hydrogen Cation - meq per 100g of soil - Not recorded
	15_NR_K	Exch. basic cations (K++) - meq per 100g of soil - Not recorded
	15_NR_MG	Exch. basic cations (Mg++) - meq per 100g of soil - Not recorded
	15_NR_NA	Exch. basic cations (Na++) - meq per 100g of soil - Not recorded
	2A1	Air-dry moisture content
	3_NR	Electrical conductivity or soluble salts - Not recorded
	4_NR	pH of soil - Not recorded
	5_NR	Water soluble Chloride - Cl(%) - Not recordede
	6A1	Organic carbon - Walkley and Black
	7_NR	Total nitrogen (%) - Not recorded
	9_NR	Available P (mg/kg) - Not recorded
	9A_NR	Total element - P(%) - Not recorded
	P10_GRAV	Gravel (%)
	P10_NR_C	Clay (%) - Not recorded
	P10_NR_CS	Coarse sand (%) - Not recorded
	P10_NR_FS	Fine sand (%) - Not recorded
	P10_NR_Z	Silt (%) - Not recorded
	P3A_NR	Bulk density - Not recorded
	P3B_VL_01	0.1 BAR Moisture m3/m3 - Volumetric using suction plate
	P3B_VL_15	15 BAR Moisture m3/m3 - Volumetric using pressure plate