Project Name:	CB
	Project Code:	CB	Site ID:	B403	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Site Information
	Desc. By:	C.J. de Mooy	Locality:
	Date Desc.:	20/05/59	Elevation:	 183 metres
	Map Ref.:	Sheet No. : 9246   1:100000	Rainfall:	762
	Northing/Long.:	151.991666666667	Runoff:	Moderately rapid
	Easting/Lat.:	-25.5875	Drainage:	Moderately well drained
	Geology
	ExposureType:	Soil pit	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	  Ra	Substrate Material:	Auger boring, 1 m deep,Unconsolidated 
	material (unidentified) 
	Land Form
	Rel/Slope Class: 	No Data	Pattern Type:	Hills
	Morph. Type:	Mid-slope	Relief:	No Data
	Elem. Type:	Hillslope	Slope Category:	No Data
	Slope:	8.7 % 	Aspect:	No Data
	Surface Soil Condition (dry):	Hardsetting
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Vertic Subnatric Black Sodosol     	Principal Profile Form:	Dd1.13
	ASC Confidence:	Great Soil Group:	Black earth
	All necessary analytical data are available.
	Site Disturbance:	No effective disturbance other than grazing by hoofed animals
	Vegetation:
	Tall Strata - Tree, , Mid-dense. *Species includes - Eucalyptus crebra
	Surface Coarse Fragments:	No surface coarse fragments
	Profile Morphology
	A1	0 - 0.1 m	Very dark grey (10YR3/1-Moist); ; Loam (Heavy); Weak grade of structure, Angular blocky; 
	Dry; Firm consistence; 0-2%, medium gravelly, 6-20mm, coarse fragments; Field pH 6.1 (pH 
	meter); Clear change to - 
	A3	0.1 - 0.15 m	Very dark grey (10YR3/1-Moist); ; Clay loam; Weak grade of structure, Angular blocky; Dry; 
	Firm consistence; Clear change to - 
	B2	0.15 - 0.3 m	Very dark grey (10YR3/1-Moist); ; Medium clay; Strong grade of structure, 10-20 mm, Angular 
	blocky; Dry; Strong consistence; Field pH 6.8 (pH meter); Gradual change to - 
	B2	0.3 - 0.46 m	Very dark grey (10YR3/1-Moist); ; Medium clay; Strong grade of structure, 10-20 mm, Angular 
	blocky; Dry; Strong consistence; Field pH 7.5 (pH meter); Gradual change to - 
	B2	0.46 - 0.63 m	Very dark grey (10YR3/1-Moist); ; Medium clay; Strong grade of structure, 10-20 mm, Angular 
	blocky; Dry; Strong consistence; Very few (0 - 2 %), Calcareous, Medium (2 -6 mm), Nodules; 
	Field pH 8 (pH meter); Diffuse change to - 
	B2	0.71 - 0.84 m	Very dark grey (10YR3/1-Moist); ; Medium clay; Strong grade of structure, Lenticular; Strong 
	grade of structure, 20-50 mm, Angular blocky; Moist; Firm consistence; Few (2 - 10 %), 
	Calcareous, Medium (2 -6 mm), Nodules; Field pH 8.4 (pH meter); Diffuse change to - 
	BC	0.91 - 1.07 m	Very dark grey (10YR3/1-Moist); ; Medium clay; , Lenticular; Moist; Firm consistence; Few (2 - 
	10 %), Calcareous, Medium (2 -6 mm), Nodules; Field pH 8.3 (pH meter); Diffuse change to - 
	1.22 - 1.37 m	Very dark grey (10YR3/1-Moist); ; Medium clay; , Lenticular; Firm consistence; 0-2%, medium 
	gravelly, 6-20mm, coarse fragments; Very few (0 - 2 %), Calcareous, Medium (2 -6 mm), 
	Nodules; Field pH 8.7 (pH meter); Diffuse change to - 
	1.52 - 1.68 m	Very dark grey (10YR3/1-Moist); ; Medium clay; Firm consistence; Very few (0 - 2 %), 
	Calcareous, Medium (2 -6 mm), Nodules; Field pH 9 (pH meter); Diffuse change to - 
	1.83 - 1.98 m	; Field pH 9.1 (pH meter); 
	Morphological Notes
	DGB Clay with weathered rock fragments.
	Observation Notes

	Project Name:	CB
	Project Code:	CB	Site ID:	B403	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	DEGRADED BLACK EARTH:SLICENSIDES BELOW 46CM SUGGEST SOME LENTICULAR STRUCTURE: C.deMOODY INDICATES 
	BURIED PROFILE       AT 1.5M:SUBSTRATE IS COLLUVIUM FROM PORPHYRITIC ANDESITE AND METASEDIMENT:MINOR 
	INCLUSIONS OF WEATHERED ROCK FROM
	Site Notes
	CENTRAL BURNET

	Project Name:	CB
	Project Code:	CB	Site ID:	B403	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.1	6.1H	 0.01B	 5.7K	 7.1	 0.56	 0.51	 6.5D
	0.1 - 0.15
	0.15 - 0.3	6.8H	 0.02B	 6.5K	 11.8	 0.17	 1.7	 3.7D
	0.3 - 0.46	7.5H	 0.07B
	0.46 - 0.63	8H	 0.23B	 7.1K	 15	 0.13	 5.7	 0D
	0.71 - 0.84	8.4H	 0.41B
	0.91 - 1.07	8.3H	 0.28B
	1.22 - 1.37	8.7H	 0.16B
	1.52 - 1.68	9H	 0.17B
	1.83 - 1.96	9.1H	 0.16B
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.1	 1.8A	 12C	 0.033F	 0.15B	1.40	 4	 9C	 25	 35	 28
	0.1 - 0.15
	0.15 - 0.3	 0.9A	 2C	 0.02F	 0.08B	1.60	 0	 6C	 20	 28	 44
	0.3 - 0.46
	0.46 - 0.63	 0.06C	 0.4A	 1	 10C	 17	 24	 48
	0.71 - 0.84
	0.91 - 1.07
	1.22 - 1.37
	1.52 - 1.68	 0.5C	1.60	 12C	 20	 25	 39
	1.83 - 1.96	 2A
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.1	 0.34C
	0.1 - 0.15
	0.15 - 0.3	 0.36C
	0.3 - 0.46
	0.46 - 0.63
	0.71 - 0.84
	0.91 - 1.07
	1.22 - 1.37
	1.52 - 1.68	 0.38C
	1.83 - 1.96

	Project Name:	CB
	Project Code:	CB	Site ID:	B403	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Analyses Completed for this profile
	15_NR_CA	Exch. basic cations (Ca++) - meq per 100g of soil - Not recorded
	15_NR_H	Hydrogen Cation - meq per 100g of soil - Not recorded
	15_NR_K	Exch. basic cations (K++) - meq per 100g of soil - Not recorded
	15_NR_MG	Exch. basic cations (Mg++) - meq per 100g of soil - Not recorded
	15_NR_NA	Exch. basic cations (Na++) - meq per 100g of soil - Not recorded
	19B_NR	Calcium Carbonate (CaCO3) - Not recorded
	2A1	Air-dry moisture content
	3_NR	Electrical conductivity or soluble salts - Not recorded
	4_NR	pH of soil - Not recorded
	5_NR	Water soluble Chloride - Cl(%) - Not recordede
	6A1	Organic carbon - Walkley and Black
	7_NR	Total nitrogen (%) - Not recorded
	9_NR	Available P (mg/kg) - Not recorded
	9A_NR	Total element - P(%) - Not recorded
	P10_GRAV	Gravel (%)
	P10_NR_C	Clay (%) - Not recorded
	P10_NR_CS	Coarse sand (%) - Not recorded
	P10_NR_FS	Fine sand (%) - Not recorded
	P10_NR_Z	Silt (%) - Not recorded
	P3A_NR	Bulk density - Not recorded
	P3B_VL_01	0.1 BAR Moisture m3/m3 - Volumetric using suction plate