Project Name:	CB
	Project Code:	CB	Site ID:	B409	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Site Information
	Desc. By:	G.D. Hubble	Locality:
	Date Desc.:	01/06/59	Elevation:	No Data
	Map Ref.:	Sheet No. : 9147   1:100000	Rainfall:	762
	Northing/Long.:	151.416666666667	Runoff:	Moderately rapid
	Easting/Lat.:	-25.4777777777778	Drainage:	Moderately well drained
	Geology
	ExposureType:	Soil pit	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	  Tb	Substrate Material:	Auger boring, 1 m deep,Basalt 
	Land Form
	Rel/Slope Class: 	No Data	Pattern Type:	Plateau
	Morph. Type:	Crest	Relief:	No Data
	Elem. Type:	No Data	Slope Category:	No Data
	Slope:	1.75 % 	Aspect:	No Data
	Surface Soil Condition (dry):	Soft
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Haplic Eutrophic Red Ferrosol     	Principal Profile Form:	Gn4.10
	ASC Confidence:	Great Soil Group:	Krasnozem
	Analytical data are incomplete but reasonable confidence.
	Site Disturbance:	Extensive clearing, for example poisoning, ringbarking
	Vegetation:	Low Strata - Tussock grass, , . *Species includes - None recorded
	Tall Strata - Tree, 6.01-12m, Closed or dense. *Species includes - Alphitonia excelsa
	Surface Coarse Fragments:	No surface coarse fragments
	Profile Morphology
	A1	0 - 0.13 m	Dark red (2.5YR2/5-Moist); ; Loam (Heavy); Strong grade of structure, <2 mm, Granular; Moist; 
	Very weak consistence; Field pH 7.7 (pH meter); Abundant, fine (1-2mm) roots; Gradual 
	change to - 
	B1	0.13 - 0.28 m	Dark red (2.5YR3/5-Moist); ; Clay loam; Strong grade of structure, <2 mm, Granular; Moist; Very 
	weak consistence; Field pH 8 (pH meter); Abundant, fine (1-2mm) roots; Gradual change to - 
	B2	0.28 - 0.66 m	Dark red (2.5YR3/6-Moist); ; Light clay; Moderate grade of structure, 5-10 mm, Polyhedral; 
	Moist; Very weak consistence; Field pH 6.9 (pH meter); Diffuse change to - 
	B2	0.66 - 0.91 m	Dark red (10R3/7-Moist); ; Light clay; Moderate grade of structure, 5-10 mm, Polyhedral;  Coarse
	 (>5mm) macropores, Dry; Firm consistence; Field pH 4.8 (pH meter); Diffuse change to - 
	B2	0.91 - 1.17 m	Dark red (10R3/7-Moist); ; Light clay; Moderate grade of structure, Polyhedral; Dry; Firm 
	consistence; Field pH 4.6 (pH meter); Diffuse change to - 
	B2	1.17 - 1.47 m	Weak red (10R4/4-Moist); ; Light medium clay; Moderate grade of structure, Polyhedral; Dry; 
	Firm consistence; Field pH 4.5 (pH meter); 
	Morphological Notes
	Observation Notes
	VEGETATION IS REMNANT OF REGROWTH SOFTWOOD SCRUB:0-28cm POROUS GRANULARSTRUCTURE:FEW 5-10MM 
	BRITTLE CLAY AGGREGATES     (NODULES) BELOW 66CM
	Site Notes
	BINJOUR PLATEA

	Project Name:	CB
	Project Code:	CB	Site ID:	B409	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.13	7.7H	 0.09B	 20.8K	 1.1	 2	 0.21	 0D
	0.13 - 0.28	8H	 0.04B
	0.28 - 0.66	6.9H	 0.04B	 6.6K	 0.5	 2.7	 0.08	 3.9D
	0.66 - 0.91	4.8H	 0.03B
	0.91 - 1.17	4.6H	 0.03B	 3.1K	 0.8	 0.08	 0.02	 5.4D
	1.17 - 1.47	4.5H	 0.02B
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.13	 3.68A	 75C	 0.062F	 0.3B	1.20	 0	 12C	 26	 19	 38
	0.13 - 0.28	 0.09C	 1.2A	 0	 12C	 21	 12	 53
	0.28 - 0.66	 0.65A	 4C	 0.037F	 0.8B	1.20	 0	 10C	 22	 13	 57
	0.66 - 0.91
	0.91 - 1.17	 0	 8C	 20	 10	 63
	1.17 - 1.47	 2C
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.13	 0.32C
	0.13 - 0.28
	0.28 - 0.66	 0.32C
	0.66 - 0.91
	0.91 - 1.17
	1.17 - 1.47

	Project Name:	CB
	Project Code:	CB	Site ID:	B409	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Analyses Completed for this profile
	15_NR_CA	Exch. basic cations (Ca++) - meq per 100g of soil - Not recorded
	15_NR_H	Hydrogen Cation - meq per 100g of soil - Not recorded
	15_NR_K	Exch. basic cations (K++) - meq per 100g of soil - Not recorded
	15_NR_MG	Exch. basic cations (Mg++) - meq per 100g of soil - Not recorded
	15_NR_NA	Exch. basic cations (Na++) - meq per 100g of soil - Not recorded
	19B_NR	Calcium Carbonate (CaCO3) - Not recorded
	2A1	Air-dry moisture content
	3_NR	Electrical conductivity or soluble salts - Not recorded
	4_NR	pH of soil - Not recorded
	5_NR	Water soluble Chloride - Cl(%) - Not recordede
	6A1	Organic carbon - Walkley and Black
	7_NR	Total nitrogen (%) - Not recorded
	9_NR	Available P (mg/kg) - Not recorded
	9A_NR	Total element - P(%) - Not recorded
	P10_GRAV	Gravel (%)
	P10_NR_C	Clay (%) - Not recorded
	P10_NR_CS	Coarse sand (%) - Not recorded
	P10_NR_FS	Fine sand (%) - Not recorded
	P10_NR_Z	Silt (%) - Not recorded
	P3A_NR	Bulk density - Not recorded
	P3B_VL_01	0.1 BAR Moisture m3/m3 - Volumetric using suction plate