Project Name:	CB
	Project Code:	CB	Site ID:	B411	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Site Information
	Desc. By:	G.D. Hubble	Locality:
	Date Desc.:	03/06/59	Elevation:	 244 metres
	Map Ref.:	Sheet No. : 9246   1:100000	Rainfall:	762
	Northing/Long.:	151.518333333333	Runoff:	Rapid
	Easting/Lat.:	-25.75	Drainage:	Well drained
	Geology
	ExposureType:	Soil pit	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	 Pgw	Substrate Material:	Soil pit, 0.89 m deep,Granite 
	Land Form
	Rel/Slope Class: 	Undulating rises 9-30m 3-10%	Pattern Type:	No Data
	Morph. Type:	No Data	Relief:	No Data
	Elem. Type:	Hillslope	Slope Category:	No Data
	Slope:	7 % 	Aspect:	No Data
	Surface Soil Condition (dry):	Soft
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Haplic Mesotrophic Red Chromosol     	Principal Profile Form:	Dr4.62
	ASC Confidence:	Great Soil Group:	Red podzolic soil
	All necessary analytical data are available.
	Site Disturbance:	No effective disturbance other than grazing by hoofed animals
	Vegetation:
	Tall Strata - Tree, , Closed or dense. *Species includes - None Recorded
	Surface Coarse Fragments:	No surface coarse fragments
	Profile Morphology
	A1	0 - 0.1 m	Very dark greyish brown (10YR3/2-Moist); ; Loamy sand; Single grain grade of structure; Moist;
	 Loose consistence; 10-20%, fine gravelly, 2-6mm, Quartz, coarse fragments; Field pH 6.6 (pH 
	meter); Clear change to - 
	A2	0.1 - 0.25 m	Reddish brown (5YR4/4-Moist); ; Sand; Single grain grade of structure; Moist; Loose 
	consistence; 20-50%, fine gravelly, 2-6mm, Quartz, coarse fragments; Field pH 6.5 (pH meter); 
	Gradual change to - 
	A3	0.25 - 0.36 m	Reddish brown (5YR4/4-Moist); ; Clayey sand; Massive grade of structure; Moist; Loose 
	consistence; 20-50%, fine gravelly, 2-6mm, Quartz, coarse fragments; Field pH 6.6 (pH meter); 
	Clear change to - 
	B21	0.41 - 0.58 m	Dark red (2.5YR3/6-Moist); ; Light clay; Massive grade of structure; Moist; Very weak 
	consistence; 20-50%, fine gravelly, 2-6mm, Quartz, coarse fragments; Field pH 6.5 (pH meter); 
	Gradual change to - 
	B22	0.58 - 0.89 m	Dark red (2.5YR3/6-Moist); ; Clay loam; Massive grade of structure; Moist; Very weak 
	consistence; 20-50%, fine gravelly, 2-6mm, Quartz, coarse fragments; Field pH 6.5 (pH meter); 
	Diffuse change to - 
	C	0.89 - 1.17 m	Red (2.5YR4/6-Moist); , 7.5YR66; Clayey coarse sand; Massive grade of structure; Moist; Very 
	weak consistence; 50-90%, medium gravelly, 6-20mm, Quartz, coarse fragments; Field pH 6.5 
	(pH meter); Diffuse change to - 
	C	1.68 - 1.83 m	Red (2.5YR4/6-Moist); , 7.5YR66; Clayey coarse sand; Massive grade of structure; Moist; Very 
	weak consistence; 50-90%, medium gravelly, 6-20mm, Quartz, coarse fragments; Field pH 6.8 
	(pH meter); 
	Morphological Notes
	Observation Notes
	Site Notes
	CENTRAL BURNET

	Project Name:	CB
	Project Code:	CB	Site ID:	B411	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.1	6.6H	 0.013B	 3.2K	 0.8	 0.28	 0	 1.4D
	0.1 - 0.25	6.5H	 0.007B
	0.25 - 0.36	6.6H	 0.006B
	0.41 - 0.58	6.5H	 0.007B	 3.1K	 1.1	 0.37	 0.1	 2.3D
	0.58 - 0.89	6.5H	 0.006B
	0.89 - 1.17	6.5H	 0.005B
	1.68 - 1.83	6.8H	 0.005B
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.1	 0.89A	 20C	 0.018F	 0.06B	1.50	 20	 59C	 23	 7	 6
	0.1 - 0.25
	0.25 - 0.36
	0.41 - 0.58	 0.2A	 6C	 0.022F	 0.03B	1.80	 30	 34C	 21	 9	 37
	0.58 - 0.89
	0.89 - 1.17
	1.68 - 1.83	 10C	 0.027F
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.1	 0.15C	 0.06C
	0.1 - 0.25
	0.25 - 0.36
	0.41 - 0.58	 0.2C	 0.16C
	0.58 - 0.89
	0.89 - 1.17
	1.68 - 1.83

	Project Name:	CB
	Project Code:	CB	Site ID:	B411	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Analyses Completed for this profile
	15_NR_CA	Exch. basic cations (Ca++) - meq per 100g of soil - Not recorded
	15_NR_H	Hydrogen Cation - meq per 100g of soil - Not recorded
	15_NR_K	Exch. basic cations (K++) - meq per 100g of soil - Not recorded
	15_NR_MG	Exch. basic cations (Mg++) - meq per 100g of soil - Not recorded
	15_NR_NA	Exch. basic cations (Na++) - meq per 100g of soil - Not recorded
	2A1	Air-dry moisture content
	3_NR	Electrical conductivity or soluble salts - Not recorded
	4_NR	pH of soil - Not recorded
	5_NR	Water soluble Chloride - Cl(%) - Not recordede
	6A1	Organic carbon - Walkley and Black
	7_NR	Total nitrogen (%) - Not recorded
	9_NR	Available P (mg/kg) - Not recorded
	9A_NR	Total element - P(%) - Not recorded
	P10_GRAV	Gravel (%)
	P10_NR_C	Clay (%) - Not recorded
	P10_NR_CS	Coarse sand (%) - Not recorded
	P10_NR_FS	Fine sand (%) - Not recorded
	P10_NR_Z	Silt (%) - Not recorded
	P3A_NR	Bulk density - Not recorded
	P3B_VL_01	0.1 BAR Moisture m3/m3 - Volumetric using suction plate
	P3B_VL_15	15 BAR Moisture m3/m3 - Volumetric using pressure plate