Project Name:	CL
	Project Code:	CL	Site ID:	B277	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Site Information
	Desc. By:	J.E. Coaldrake	Locality:
	Date Desc.:	24/11/55	Elevation:	 8 metres
	Map Ref.:	Sheet No. : 9546   1:100000	Rainfall:	1397
	Northing/Long.:	153.08	Runoff:	No runoff
	Easting/Lat.:	-25.9183333333333	Drainage:	Very poorly drained
	Geology
	ExposureType:	Soil pit	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	Auger boring, 3 m deep,Unconsolidated 
	material (unidentified) 
	Land Form
	Rel/Slope Class: 	No Data	Pattern Type:	Dunefield
	Morph. Type:	No Data	Relief:	No Data
	Elem. Type:	Plain	Slope Category:	No Data
	Slope:	0 % 	Aspect:	0 degrees
	Surface Soil Condition (dry):	Soft
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	No Available Class Acidic Sapric Organosol     	Principal Profile Form:	O
	ASC Confidence:	Great Soil Group:	Acid peat
	All necessary analytical data are available.
	Site Disturbance:	No effective disturbance. Natural
	Vegetation:
	Tall Strata - Sedge, 0.26-0.5m, Closed or dense. *Species includes - None Recorded
	Surface Coarse Fragments:	No surface coarse fragments
	Profile Morphology
	P1	0 - 0.23 m	Black (2.5YR2/0-Moist); ; Fibric peat; Wet; Field pH 4.1 (pH meter); Abundant, fine (1-2mm) 
	roots; Diffuse change to - 
	P1	0.23 - 0.69 m	Black (2.5YR2/0-Moist); ; Fibric peat; Wet; Field pH 4 (pH meter); Abundant, fine (1-2mm) roots; 
	Diffuse change to - 
	P2	0.69 - 1.52 m	Black (2.5Y2/0-Moist); ; Sapric peat; Wet; Field pH 4.2 (pH meter); Many, very fine (0-1mm) 
	roots; Diffuse change to - 
	P2	1.52 - 2.54 m	Black (2.5Y2/0-Moist); ; Sapric peat; Wet; Field pH 4.3 (pH meter); Common, very fine (0-1mm) 
	roots; Diffuse change to - 
	A1	2.54 - 2.79 m	Very dusky red (2.5YR2/2-Moist); ; Hemic peat; Wet; Field pH 4.7 (pH meter); Few, very fine (0-
	1mm) roots; Diffuse change to - 
	A2Bh	2.79 - 3.05 m	Dark reddish grey (5YR4/2-Moist); , 5YR22; Sand (Fibric); Massive grade of structure; Wet; 
	Field pH 4.8 (pH meter); 
	Morphological Notes
	Observation Notes
	0-69CM FIBROUS PEAT:69-254CM HUMIFIED PEAT                                                                              
	Site Notes
	RAINBOW BEACH

	Project Name:	CL
	Project Code:	CL	Site ID:	B277	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.23	4.1H	 0.25B
	0.23 - 0.69	4H	 0.19B
	0.69 - 1.52	4.2H	 0.09B	 5.6K	 15.1	 0.15	 1.6	 170D
	1.52 - 2.54	4.3H	 0.08B
	2.54 - 2.79	4.7H	 0.04B
	2.79 - 3.05	4.8H	 0.02B
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.23	 43.7A	 1.35B
	0.23 - 0.69
	0.69 - 1.52	 40.1A	 35C	 0.011F	 0.97B
	 15C	 0.005F
	1.52 - 2.54
	2.54 - 2.79	 9.83A	 0.15B	 0	 48C	 19	 12	 4
	2.79 - 3.05	 2.12A	 0.003F	 0	 78C	 14	 2	 1
	 0.001F
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.23
	0.23 - 0.69
	0.69 - 1.52
	1.52 - 2.54
	2.54 - 2.79
	2.79 - 3.05

	Project Name:	CL
	Project Code:	CL	Site ID:	B277	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Analyses Completed for this profile
	15_NR_CA	Exch. basic cations (Ca++) - meq per 100g of soil - Not recorded
	15_NR_H	Hydrogen Cation - meq per 100g of soil - Not recorded
	15_NR_K	Exch. basic cations (K++) - meq per 100g of soil - Not recorded
	15_NR_MG	Exch. basic cations (Mg++) - meq per 100g of soil - Not recorded
	15_NR_NA	Exch. basic cations (Na++) - meq per 100g of soil - Not recorded
	2_LOI	Loss on Ignition (%)
	2A1	Air-dry moisture content
	3_NR	Electrical conductivity or soluble salts - Not recorded
	4_NR	pH of soil - Not recorded
	5_NR	Water soluble Chloride - Cl(%) - Not recordede
	6A1	Organic carbon - Walkley and Black
	7_NR	Total nitrogen (%) - Not recorded
	9_NR	Available P (mg/kg) - Not recorded
	9A_NR	Total element - P(%) - Not recorded
	P10_GRAV	Gravel (%)
	P10_NR_C	Clay (%) - Not recorded
	P10_NR_CS	Coarse sand (%) - Not recorded
	P10_NR_FS	Fine sand (%) - Not recorded
	P10_NR_Z	Silt (%) - Not recorded