Project Name:	COL
	Project Code:	COL	Site ID:	B471	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Site Information
	Desc. By:	R.F. Isbell	Locality:
	Date Desc.:	07/08/61	Elevation:	No Data
	Map Ref.:	Sheet No. : 8456   1:100000	Rainfall:	0
	Northing/Long.:	147.861111111111	Runoff:	Moderately rapid
	Easting/Lat.:	-20.9111111111111	Drainage:	Imperfectly drained
	Geology
	ExposureType:	Soil pit	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	 Puw	Substrate Material:	Soil pit, 0.61 m deep,Sandstone 
	Land Form
	Rel/Slope Class: 	No Data	Pattern Type:	No Data
	Morph. Type:	Crest	Relief:	5 metres
	Elem. Type:	No Data	Slope Category:	No Data
	Slope:	0 % 	Aspect:	No Data
	Surface Soil Condition (dry):	Cracking
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Endocalcareous Epipedal Brown Vertosol     	Principal Profile Form:	Ug5.13
	ASC Confidence:	Great Soil Group:	Brown clay
	All necessary analytical data are available.
	Site Disturbance:	No effective disturbance other than grazing by hoofed animals
	Vegetation:	Low Strata - Tussock grass, , Closed or dense. *Species includes - Bothriochloa ewartiana
	Tall Strata - Tree, , Isolated clumps. *Species includes - Acacia harpophylla, Eucalyptus papuana
	Surface Coarse Fragments:	2-10%, coarse gravelly, 20-60mm, , Substrate material
	Profile Morphology
	AB	0 - 0.25 m	Dark brown (7.5YR3/2-Moist); ; Heavy clay; Strong grade of structure, 20-50 mm, Angular 
	blocky; Dry; Very firm consistence; 0-2%, Substrate material, coarse fragments; Field pH 7.4 
	(pH meter); Gradual change to - 
	B2	0.25 - 0.41 m	Brown (10YR4/3-Moist); ; Medium clay; Moderate grade of structure, 20-50 mm, Angular blocky;
	 Dry; Very firm consistence; 2-10%, Substrate material, coarse fragments; Field pH 8.2 (pH 
	meter); Gradual change to - 
	BC	0.41 - 0.61 m	Yellowish brown (10YR5/4-Moist); ; Light clay; Massive grade of structure; Dry; Firm 
	consistence; 2-10%, Substrate material, coarse fragments; Common (10 - 20 %), Calcareous, , 
	Soft segregations; Field pH 8.6 (pH meter); Gradual change to - 
	C	0.61 - 0.76 m	; Field pH 8.6 (pH meter); 
	Morphological Notes
	C	LYB (10YR6/4) soft fels. sandstone with moderate Ca nods.
	Observation Notes
	0-25CM THIN PLATY SURFACE OVER MODERATE (6MM) GRANULAR,GRADING TO BLOCKY STRUCTURE BELOW 
	1.5CM:CALCAREOUS SEGREGATIONS  BOTH SOFT AND NODULAR:
	Site Notes
	COLLINSVILLE

	Project Name:	COL
	Project Code:	COL	Site ID:	B471	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.25	7.4H	 0.03B	 29.8K	 7.2	 0.65	 0.1	 2.12D
	0.25 - 0.41	8.2H	 0.05B
	0.41 - 0.61	8.6H	 0.04B	 23.2K	 8.3	 0.11	 0.1	 0D
	0.61 - 0.76	8.6H	 0.04B
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.25	 1.6A	 82C	 0.055F	 0.196B	 8C	 19	 51	 51
	0.25 - 0.41	 186C
	0.41 - 0.61	 23.5C	 5	 5C	 22	 23	 23
	0.61 - 0.76	 500C	 0.152F
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.25
	0.25 - 0.41
	0.41 - 0.61
	0.61 - 0.76

	Project Name:	COL
	Project Code:	COL	Site ID:	B471	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Analyses Completed for this profile
	15_NR_CA	Exch. basic cations (Ca++) - meq per 100g of soil - Not recorded
	15_NR_H	Hydrogen Cation - meq per 100g of soil - Not recorded
	15_NR_K	Exch. basic cations (K++) - meq per 100g of soil - Not recorded
	15_NR_MG	Exch. basic cations (Mg++) - meq per 100g of soil - Not recorded
	15_NR_NA	Exch. basic cations (Na++) - meq per 100g of soil - Not recorded
	19B_NR	Calcium Carbonate (CaCO3) - Not recorded
	2A1	Air-dry moisture content
	3_NR	Electrical conductivity or soluble salts - Not recorded
	4_NR	pH of soil - Not recorded
	5_NR	Water soluble Chloride - Cl(%) - Not recordede
	6A1	Organic carbon - Walkley and Black
	7_NR	Total nitrogen (%) - Not recorded
	9_NR	Available P (mg/kg) - Not recorded
	9A_NR	Total element - P(%) - Not recorded
	P10_GRAV	Gravel (%)
	P10_NR_C	Clay (%) - Not recorded
	P10_NR_CS	Coarse sand (%) - Not recorded
	P10_NR_FS	Fine sand (%) - Not recorded
	P10_NR_Z	Silt (%) - Not recorded