Project Name:	COL
	Project Code:	COL	Site ID:	B480	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Site Information
	Desc. By:	R.F. Isbell	Locality:
	Date Desc.:	23/07/61	Elevation:	No Data
	Map Ref.:	Sheet No. : 8456   1:100000	Rainfall:	0
	Northing/Long.:	147.838888888889	Runoff:	Moderately rapid
	Easting/Lat.:	-20.7916666666667	Drainage:	Imperfectly drained
	Geology
	ExposureType:	Soil pit	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	 Puw	Substrate Material:	Soil pit, 1.2 m deep,Unconsolidated material 
	(unidentified) 
	Land Form
	Rel/Slope Class: 	No Data	Pattern Type:	Terrace (alluvial)
	Morph. Type:	No Data	Relief:	No Data
	Elem. Type:	No Data	Slope Category:	No Data
	Slope:	0 % 	Aspect:	No Data
	Surface Soil Condition (dry):	Hardsetting
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Calcic Subnatric Black Sodosol     	Principal Profile Form:	Dd1.33
	ASC Confidence:	Great Soil Group:	Solodic soil
	All necessary analytical data are available.
	Site Disturbance:	Limited clearing, for example selective logging
	Vegetation:
	Tall Strata - Tree, 3.01-6m, Very sparse. *Species includes - Eremophila mitchellii
	Surface Coarse Fragments:	No surface coarse fragments
	Profile Morphology
	A1	0 - 0.13 m	Dark brown (7.5YR3/4-Moist); ; Clay loam; Massive grade of structure; Dry; Weak consistence; 
	Very few (0 - 2 %), Manganiferous, , Soft segregations; Field pH 6.5 (pH meter); Abrupt 
	change to - 
	B21	0.13 - 0.36 m	Dark brown (7.5YR3/2-Moist); ; Medium clay; Weak grade of structure, 50-100 mm, Prismatic; 
	Moderate grade of structure, 20-50 mm, Angular blocky; Dry; Very firm consistence; Very few 
	(0 - 2 %), Calcareous, , Nodules; Field pH 7 (pH meter); Gradual change to - 
	B22	0.36 - 0.76 m	Dark brown (7.5YR3/4-Moist); ; Medium clay; Weak grade of structure, Angular blocky; Dry; 
	Very firm consistence; Common (10 - 20 %), Calcareous, , Nodules; Field pH 8.7 (pH meter); 
	Gradual change to - 
	BC	0.76 - 1.17 m	Brown (10YR4/3-Moist); ; Light clay; Massive grade of structure; Dry; Firm consistence; Very 
	few (0 - 2 %), Calcareous, , Nodules; Field pH 8.7 (pH meter); Gradual change to - 
	C	1.17 - 1.52 m	Yellowish brown (10YR5/5-Moist); ; Clay loam, fine sandy; Massive grade of structure; 
	Moderately moist; Weak consistence; Very few (0 - 2 %), Calcareous, , Soft segregations; Field
	 pH 8.3 (pH meter); 
	Morphological Notes
	Observation Notes
	SPORADIC BLEACH AT BASE OF A HORIZON:CALCAREOUS SEGREGATIONS BOTH SOFT AND NODULAR:                               
	      
	Site Notes
	COLLINSVILLE

	Project Name:	COL
	Project Code:	COL	Site ID:	B480	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.13	6.5H	 0.03B	 11.3K	 4	 0.29	 0.56	 3.5D
	0.13 - 0.36	7H	 0.1B	 14.3K	 10.2	 0.27	 2.6	 3D
	0.36 - 0.73	8.7H	 0.3B
	0.76 - 1.17	8.7H	 0.21B	 10.5K	 8.6	 0.33	 4.2	 0D
	1.17 - 1.52	8.3H	 0.14B
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.13	 1.1A	 16C	 0.035F	 0.125B	 0	 10C	 46	 16	 25
	0.13 - 0.36	 0.49A	 7C	 0	 6C	 32	 16	 43
	0.36 - 0.73
	0.76 - 1.17	 0.19C	 118C	 0.032F	 0	 5C	 48	 13	 33
	1.17 - 1.52
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.13
	0.13 - 0.36
	0.36 - 0.73
	0.76 - 1.17
	1.17 - 1.52

	Project Name:	COL
	Project Code:	COL	Site ID:	B480	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Analyses Completed for this profile
	15_NR_CA	Exch. basic cations (Ca++) - meq per 100g of soil - Not recorded
	15_NR_H	Hydrogen Cation - meq per 100g of soil - Not recorded
	15_NR_K	Exch. basic cations (K++) - meq per 100g of soil - Not recorded
	15_NR_MG	Exch. basic cations (Mg++) - meq per 100g of soil - Not recorded
	15_NR_NA	Exch. basic cations (Na++) - meq per 100g of soil - Not recorded
	19B_NR	Calcium Carbonate (CaCO3) - Not recorded
	2A1	Air-dry moisture content
	3_NR	Electrical conductivity or soluble salts - Not recorded
	4_NR	pH of soil - Not recorded
	5_NR	Water soluble Chloride - Cl(%) - Not recordede
	6A1	Organic carbon - Walkley and Black
	7_NR	Total nitrogen (%) - Not recorded
	9_NR	Available P (mg/kg) - Not recorded
	9A_NR	Total element - P(%) - Not recorded
	P10_GRAV	Gravel (%)
	P10_NR_C	Clay (%) - Not recorded
	P10_NR_CS	Coarse sand (%) - Not recorded
	P10_NR_FS	Fine sand (%) - Not recorded
	P10_NR_Z	Silt (%) - Not recorded