Project Name:	Cooloola
	Project Code:	Cooloola	Site ID:	B872	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Site Information
	Desc. By:	C.H. Thompson	Locality:	Townshend Island.  SWB survey site SD32.
	Date Desc.:	17/05/76	Elevation:	30 metres
	Map Ref.:	Sheet No. : 8953-1   1:50000	Rainfall:	No Data
	Northing/Long.:	150.4799825	Runoff:	No Data
	Easting/Lat.:	-22.21152083	Drainage:	Imperfectly drained
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	No Data	Pattern Type:	No Data
	Morph. Type:	No Data	Relief:	30 metres
	Elem. Type:	Dune	Slope Category:	No Data
	Slope:	 % 	Aspect:	No Data
	Surface Soil Condition (dry):
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	 Podosol     	Principal Profile Form:	N/A
	ASC Confidence:	Great Soil Group:	Podzol
	Confidence level not specified
	Site Disturbance:
	Vegetation:
	Surface Coarse Fragments:
	Profile Morphology
	A11	0 - 0.01 m	Grey (10YR6/1-Moist); Grey (10YR5/1-Moist); ; Sand; Single grain grade of structure; Loose 
	consistence; 
	A12	0.01 - 0.1 m	Very dark grey (10YR3/1-Moist); , 10YR41; Sand; Single grain grade of structure; Weak 
	consistence; Field pH 4.5 (Raupach); 
	A12	0.1 - 0.2 m	Very dark grey (10YR3/1-Moist); , 10YR41; Sand; Single grain grade of structure; Weak 
	consistence; 
	A12	0.2 - 0.3 m	Very dark grey (10YR3/1-Moist); , 10YR41; Sand; Single grain grade of structure; Weak 
	consistence; 
	A12	0.3 - 0.5 m	Very dark grey (10YR3/1-Moist); , 10YR41; Sand; Single grain grade of structure; Weak 
	consistence; Many, coarse (>5mm) roots; Diffuse change to - 
	A13	0.5 - 0.6 m	Dark grey (10YR4/1-Moist); Very dark grey (10YR3/1-Moist); ; Sand; Single grain grade of 
	structure; Weak consistence; 
	A14	0.6 - 0.9 m	Dark greyish brown (10YR4/2-Moist); Grey (10YR5/1-Moist); ; Sand; Single grain grade of 
	structure; Very weak consistence; 
	A15	0.9 - 1.2 m	Greyish brown (10YR5/2-Moist); Dark grey (10YR4/1-Moist); ; Sand; Single grain grade of 
	structure; Very weak consistence; 
	A2	1.2 - 1.35 m	Pale brown (10YR6/3-Moist); Very pale brown (10YR7/3-Dry); ; Sand; Single grain grade of 
	structure; Loose consistence; Field pH 6.3 (Raupach); 
	B2	1.35 - 1.5 m	Dark reddish brown (5YR3/4-Moist); Dark brown (7.5YR3/3-Moist); ; Sand; Single grain grade 
	of structure; Weak consistence; Field pH 5.5 (Raupach); 
	B2	1.5 - 1.8 m	Dark reddish brown (5YR3/4-Moist); Dark brown (7.5YR3/3-Moist); ; Sand; Weak consistence; 
	B22	1.8 - 2.1 m	Dark brown (7.5YR3/3-Moist); Brown (7.5YR4/4-Moist); , 7.5YR56; Sand; Single grain grade of 
	structure; Weak consistence; 
	B3	2.1 - 2.4 m	Strong brown (7.5YR5/6-Moist); , 7.5YR44; , 7.5YR66; Sand; Single grain grade of structure; 
	Very weak consistence; 
	B3	2.4 - 2.7 m	Strong brown (7.5YR5/6-Moist); , 7.5YR44; , 7.5YR66; Sand; Very weak consistence; 

	Project Name:	Cooloola
	Project Code:	Cooloola	Site ID:	B872	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	C1	2.7 - 3 m	Reddish yellow (7.5YR6/6-Moist); Strong brown (7.5YR5/6-Moist); ; Sand; Single grain grade of
	 structure; Loose consistence; 
	C1	3 - 3.3 m	Reddish yellow (7.5YR6/6-Moist); ; Sand; 
	C1	3.3 - 3.6 m	Reddish yellow (7.5YR6/6-Moist); ; Sand; 
	C2	3.6 - 3.9 m	Reddish yellow (7.5YR6/6-Moist); ; Sand; 
	Morphological Notes
	A11	Discrete OM.  Rain washed surface is much thinner than at Cooloola - rainfall intensities 
	are unlikely to be lower but are fires less frequent?
	A12	Thick A2 with diffuse OM.  A2 is bleached dry and boundary to B is clear and uneven 
	over 135/145cm depth.
	A12	Many roots at 30 - 40cm depth - up to 20mm size slight root development 5-10mm size 
	top of B but few roots in lower A1 and A2.
	A13	Diffuse OM.
	A14	Sl diffuse OM.
	A15	Sl diffuse OM.
	B2	Translocated OM and Fe.
	B22	Translocated OM and Fe.
	B3	Sl translocated OM and Fe > with depth.
	Observation Notes
	Parent material: Aeolian siliceous sands.  Landform: nose of V-shaped sand dune.
	Site Notes

	Project Name:	Cooloola
	Project Code:	Cooloola	Site ID:	B872	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.01
	0 - 0.1	4.9H	<0.03B
	0.1 - 0.2	4.7H	<0.03B	0.6K	0.6	<0.1	<0.1	0.7D	1.9F
	0.2 - 0.3	4.6H	<0.03B
	0.3 - 0.5	4.5H	<0.03B
	0.5 - 0.6	4.6H	<0.03B
	0.6 - 0.9	4.7H	<0.03B
	0.9 - 1.2	4.9H	<0.03B
	1.2 - 1.35	4.9H	<0.03B
	1.35 - 1.5	4.7H	<0.03B	<0.1K	<0.1	<1	<0.1	0.6D	0.6F
	1.5 - 1.8	4.9H	<0.03B
	1.8 - 2.1	5H	<0.03B
	2.1 - 2.4	4.9H	<0.03B	<0.1K	<0.1	<0.1	<0.1	0.3D	0.4F
	2.4 - 2.7	5H	<0.03B
	2.7 - 3
	3 - 3.3	4.9H	<0.03B	<0.1K	<0.1	<0.1	<0.1	0.4D	0.5F
	3.3 - 3.6
	3.6 - 3.9	5H	<0.03B
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.01
	0 - 0.1
	0.1 - 0.2	98I	0	0
	0.2 - 0.3
	0.3 - 0.5
	0.5 - 0.6
	0.6 - 0.9
	0.9 - 1.2
	1.2 - 1.35
	1.35 - 1.5	99I	0	0
	1.5 - 1.8
	1.8 - 2.1
	2.1 - 2.4
	2.4 - 2.7	0.04E	0.004B
	2.7 - 3	99I	0	0
	3 - 3.3	0.07E	4B	0.003B
	3.3 - 3.6
	3.6 - 3.9	0.03E	4B	0.001B
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.01
	0 - 0.1
	0.1 - 0.2
	0.2 - 0.3
	0.3 - 0.5

	Project Name:	Cooloola
	Project Code:	Cooloola	Site ID:	B872	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	0.5 - 0.6
	0.6 - 0.9
	0.9 - 1.2
	1.2 - 1.35
	1.35 - 1.5
	1.5 - 1.8
	1.8 - 2.1
	2.1 - 2.4
	2.4 - 2.7
	2.7 - 3
	3 - 3.3
	3.3 - 3.6
	3.6 - 3.9

	Project Name:	Cooloola
	Project Code:	Cooloola	Site ID:	B872	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Analyses Completed for this profile
	15_NR_CA	Exch. basic cations (Ca++) - meq per 100g of soil - Not recorded
	15_NR_H	Hydrogen Cation - meq per 100g of soil - Not recorded
	15_NR_K	Exch. basic cations (K++) - meq per 100g of soil - Not recorded
	15_NR_MG	Exch. basic cations (Mg++) - meq per 100g of soil - Not recorded
	15_NR_NA	Exch. basic cations (Na++) - meq per 100g of soil - Not recorded
	15J1	Effective CEC
	2A1	Air-dry moisture content
	3_NR	Electrical conductivity or soluble salts - Not recorded
	4_NR	pH of soil - Not recorded
	5_NR	Water soluble Chloride - Cl(%) - Not recordede
	6Z	Organic carbon (%) - Not recorded
	7_NR	Total nitrogen (%) - Not recorded
	8A1	Total organic carbon/total nitrogen ratio
	9G_BSES	Available P (mg/kg) - Acid P - 0.005M H2SO4 (BSES)
	P10_NR_C	Clay (%) - Not recorded
	P10_NR_S	Sand (%) - Not recorded
	P10_NR_Z	Silt (%) - Not recorded