Project Name:	DD
	Project Code:	DD	Site ID:	B200	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Site Information
	Desc. By:	C.H. Thompson	Locality:
	Date Desc.:	01/10/53	Elevation:	 427 metres
	Map Ref.:	Sheet No. : 9242   1:100000	Rainfall:	660
	Northing/Long.:	151.525	Runoff:	Moderately rapid
	Easting/Lat.:	-27.5580555555556	Drainage:	Moderately well drained
	Geology
	ExposureType:	Soil pit	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	 Czw	Substrate Material:	Soil pit, 1.6 m deep,Basalt 
	Land Form
	Rel/Slope Class: 	Undulating low hills 30-90m 3-	Pattern Type:	Low hills
	10%
	Morph. Type:	No Data	Relief:	30 metres
	Elem. Type:	Pediment	Slope Category:	No Data
	Slope:	0 % 	Aspect:	No Data
	Surface Soil Condition (dry):	Self-mulching
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Epicalcareous-Endohypersodic Self-Mulching Red Vertosol    	Principal Profile Form:	Ug5.16
	ASC Confidence:	Great Soil Group:	Black earth
	All necessary analytical data are available.
	Site Disturbance:	No effective disturbance other than grazing by hoofed animals
	Vegetation:
	Tall Strata - Tussock grass, 0.26-0.5m, Sparse. *Species includes - Aristida species, Dichanthium sericeum
	Surface Coarse Fragments:	0-2%, cobbly, 60-200mm, , Basalt
	Profile Morphology
	AB	0 - 0.1 m	Very dark grey (10YR3/1-Dry); ; Heavy clay; Strong grade of structure, <2 mm, Granular; 
	Moderately moist; Very weak consistence; Very few (0 - 2 %), Calcareous, Medium (2 -6 mm), 
	Nodules; Field pH 8.6 (pH meter); Common, fine (1-2mm) roots; Clear change to - 
	B21	0.1 - 0.3 m	Very dark grey (10YR3/1-Dry); ; Heavy clay; Moderate grade of structure, 20-50 mm, Angular 
	blocky; Moderately moist; Very firm consistence; 0-2%, Quartz, coarse fragments; Common (10
	 - 20 %), Calcareous, Medium (2 -6 mm), Nodules; Field pH 9.3 (pH meter); Common, fine (1-
	2mm) roots; Gradual change to - 
	B21	0.3 - 0.64 m	Very dark grey (10YR3/1-Dry); ; Heavy clay; Moderate grade of structure, Lenticular; , Angular 
	blocky; Moderately moist; Very firm consistence; 0-2%, Quartz, coarse fragments; Common (10
	 - 20 %), Calcareous, Medium (2 -6 mm), Nodules; Field pH 9.4 (pH meter); Few, fine (1-2mm) 
	roots; Gradual change to - 
	B21	0.64 - 0.91 m	Very dark grey (10YR3/1-Dry); ; Heavy clay; Moderate grade of structure, Lenticular; , Angular 
	blocky; Moderately moist; Very firm consistence; Very few (0 - 2 %), Calcareous, Medium (2 -6 
	mm), Nodules; Field pH 9 (pH meter); Few, fine (1-2mm) roots; Gradual change to - 
	B22	0.91 - 1.14 m	Very dark brown (10YR2/2-Moist); , 10YR43; Heavy clay; Moderate grade of structure, 
	Lenticular; , Angular blocky; Moist; Firm consistence; Very few (0 - 2 %), Calcareous, Medium 
	(2 -6 mm), Nodules; Field pH 9 (pH meter); Gradual change to - 
	B22	1.19 - 1.52 m	Yellowish brown (10YR5/4-Moist); , 10YR43; Heavy clay; Moderate grade of structure, 
	Lenticular; , Angular blocky; Moist; Firm consistence; 0-2%, Substrate material, coarse 
	fragments; Few (2 - 10 %), Calcareous, Coarse (6 - 20 mm), Nodules; Field pH 9 (pH meter); 
	Morphological Notes
	Observation Notes
	0-10CM GRANULAR GRADING TO BLOCKY STRUCTURE                                                                             
	Site Notes
	DARLING DOWNS

	Project Name:	DD
	Project Code:	DD	Site ID:	B200	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.1	8.6H	 0.06B
	0.1 - 0.3	9.3H	 0.12B	 31.6K	 18.9	 0.56	 6.3	 57.4E
	0.3 - 0.64	9.4H	 0.38B
	0.64 - 0.91	9H	 0.68B
	0.91 - 1.14	9H	 0.74B
	1.19 - 1.52	9H	 0.74B
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.1	 1.9E	 980C	 0.126F
	0.1 - 0.3	 11.1C	 1.26A	 4C	 15	 14	 52
	0.3 - 0.64	 1E
	0.64 - 0.91	 0.75E
	0.91 - 1.14	 0.47E
	1.19 - 1.52	 0.2E
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.1
	0.1 - 0.3
	0.3 - 0.64
	0.64 - 0.91
	0.91 - 1.14
	1.19 - 1.52

	Project Name:	DD
	Project Code:	DD	Site ID:	B200	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Analyses Completed for this profile
	15_NR	Sum of Ex. cations + Ex. acidity - Not recorded
	15_NR_CA	Exch. basic cations (Ca++) - meq per 100g of soil - Not recorded
	15_NR_K	Exch. basic cations (K++) - meq per 100g of soil - Not recorded
	15_NR_MG	Exch. basic cations (Mg++) - meq per 100g of soil - Not recorded
	15_NR_NA	Exch. basic cations (Na++) - meq per 100g of soil - Not recorded
	19B_NR	Calcium Carbonate (CaCO3) - Not recorded
	2_LOI	Loss on Ignition (%)
	2A1	Air-dry moisture content
	3_NR	Electrical conductivity or soluble salts - Not recorded
	4_NR	pH of soil - Not recorded
	5_NR	Water soluble Chloride - Cl(%) - Not recordede
	6A1	Organic carbon - Walkley and Black
	6Z	Organic carbon (%) - Not recorded
	9_NR	Available P (mg/kg) - Not recorded
	9A_NR	Total element - P(%) - Not recorded
	P10_NR_C	Clay (%) - Not recorded
	P10_NR_CS	Coarse sand (%) - Not recorded
	P10_NR_FS	Fine sand (%) - Not recorded
	P10_NR_Z	Silt (%) - Not recorded