Project Name:	DD
	Project Code:	DD	Site ID:	B206	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Site Information
	Desc. By:	C.H. Thompson	Locality:
	Date Desc.:	01/10/53	Elevation:	 442 metres
	Map Ref.:	Sheet No. : 9242   1:100000	Rainfall:	660
	Northing/Long.:	151.755555555556	Runoff:	Moderately rapid
	Easting/Lat.:	-27.7480555555556	Drainage:	Moderately well drained
	Geology
	ExposureType:	Soil pit	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	 Czb	Substrate Material:	Auger boring, 2 m deep,Porous, 
	Unconsolidated material (unidentified) 
	Land Form
	Rel/Slope Class: 	No Data	Pattern Type:	Pediplain
	Morph. Type:	No Data	Relief:	15 metres
	Elem. Type:	Pediment	Slope Category:	No Data
	Slope:	3.5 % 	Aspect:	No Data
	Surface Soil Condition (dry):	Self-mulching
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Epicalcareous-Endohypersodic Self-Mulching Black Vertosol  	Principal Profile Form:	Ug5.15
	   
	ASC Confidence:	Great Soil Group:	Black earth
	All necessary analytical data are available.
	Site Disturbance:	No effective disturbance other than grazing by hoofed animals
	Vegetation:
	Tall Strata - Tussock grass, 0.51-1m, Mid-dense. *Species includes - None Recorded
	Surface Coarse Fragments:	No surface coarse fragments
	Profile Morphology
	AB	0 - 0.04 m	Very dark greyish brown (10YR3/2-Moist); ; Heavy clay; Strong grade of structure, <2 mm, 
	Granular; Dry; Loose consistence; 0-2%, medium gravelly, 6-20mm, Basalt, coarse fragments; 
	Very few (0 - 2 %), Calcareous, Medium (2 -6 mm), Nodules; Field pH 8.2 (pH meter); Common, 
	very fine (0-1mm) roots; Clear change to - 
	B2	0.04 - 0.28 m	Very dark greyish brown (10YR3/2-Moist); , 5YR32; Heavy clay; Moderate grade of structure, 
	Angular blocky; Moderately moist; Firm consistence; Few (2 - 10 %), Calcareous, Medium (2 -6 
	mm), Nodules; Field pH 8.9 (pH meter); Few, very fine (0-1mm) roots; Gradual change to - 
	B2	0.28 - 0.79 m	Dark brown (7.5YR3/2-Moist); , 10YR32; Heavy clay; Moderate grade of structure, Lenticular; 
	Moist; Firm consistence; Few (2 - 10 %), Calcareous, Medium (2 -6 mm), Nodules; Field pH 9.2 
	(pH meter); Gradual change to - 
	B2	0.79 - 1.07 m	Dark brown (7.5YR3/2-Moist); , 5YR43; Heavy clay; Moderate grade of structure, Lenticular; 
	Moist; Firm consistence; 0-2%, medium gravelly, 6-20mm, Basalt, coarse fragments; Few (2 - 
	10 %), Calcareous, Medium (2 -6 mm), Nodules; Field pH 9.1 (pH meter); Diffuse change to - 
	B2	1.12 - 1.52 m	Reddish brown (5YR4/3-Moist); ; Heavy clay; Moderate grade of structure, Lenticular; Moist; 
	Firm consistence; 0-2%, fine gravelly, 2-6mm, Basalt, coarse fragments; Few (2 - 10 %), 
	Calcareous, Medium (2 -6 mm), Nodules; Field pH 9 (pH meter); 
	Morphological Notes
	Observation Notes
	0-4CM GRANULAR GRADING TO BLOCKY STRUCTURE:BANK PROFILE                                                                 
	Site Notes
	DARLING DOWNS

	Project Name:	DD
	Project Code:	DD	Site ID:	B206	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.04	8.2H	 0.07B
	0.04 - 0.28	8.9H	 0.08B
	0.28 - 0.79	9.2H	 0.14B	 19.6K	 29.5	 0.47	 5.8
	0.79 - 1.07	9.1H	 0.28B
	1.12 - 1.52	9H	 0.33B
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.04	 1.26A
	0.04 - 0.28	 0.96A	 472C	 0.16F
	0.28 - 0.79	 9.49C	 0.63A	 0.2	 0.5C	 7	 14	 68
	0.79 - 1.07	 0.44A
	1.12 - 1.52	 0.17A
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.04
	0.04 - 0.28
	0.28 - 0.79
	0.79 - 1.07
	1.12 - 1.52

	Project Name:	DD
	Project Code:	DD	Site ID:	B206	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Analyses Completed for this profile
	15_NR_CA	Exch. basic cations (Ca++) - meq per 100g of soil - Not recorded
	15_NR_K	Exch. basic cations (K++) - meq per 100g of soil - Not recorded
	15_NR_MG	Exch. basic cations (Mg++) - meq per 100g of soil - Not recorded
	15_NR_NA	Exch. basic cations (Na++) - meq per 100g of soil - Not recorded
	19B_NR	Calcium Carbonate (CaCO3) - Not recorded
	2_LOI	Loss on Ignition (%)
	2A1	Air-dry moisture content
	3_NR	Electrical conductivity or soluble salts - Not recorded
	4_NR	pH of soil - Not recorded
	5_NR	Water soluble Chloride - Cl(%) - Not recordede
	6A1	Organic carbon - Walkley and Black
	9_NR	Available P (mg/kg) - Not recorded
	9A_NR	Total element - P(%) - Not recorded
	P10_GRAV	Gravel (%)
	P10_NR_C	Clay (%) - Not recorded
	P10_NR_CS	Coarse sand (%) - Not recorded
	P10_NR_FS	Fine sand (%) - Not recorded
	P10_NR_Z	Silt (%) - Not recorded