Project Name:	DD
	Project Code:	DD	Site ID:	B216	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Site Information
	Desc. By:	G.D. Hubble	Locality:
	Date Desc.:	01/11/53	Elevation:	 610 metres
	Map Ref.:	Sheet No. : 9242   1:100000	Rainfall:	889
	Northing/Long.:	151.9075	Runoff:	Moderately rapid
	Easting/Lat.:	-27.5366666666667	Drainage:	Moderately well drained
	Geology
	ExposureType:	Soil pit	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	Auger boring, 1.6 m deep,Porous, Basalt 
	Land Form
	Rel/Slope Class: 	No Data	Pattern Type:	Plateau
	Morph. Type:	Crest	Relief:	15 metres
	Elem. Type:	Plain	Slope Category:	No Data
	Slope:	0 % 	Aspect:	No Data
	Surface Soil Condition (dry):
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Haplic Eutrophic Red Ferrosol     	Principal Profile Form:	Gn3.12
	ASC Confidence:	Great Soil Group:	Euchrozem
	Analytical data are incomplete but reasonable confidence.
	Site Disturbance:
	Vegetation:
	Tall Strata - Tussock grass, 0.26-0.5m, . *Species includes - Aristida species
	Surface Coarse Fragments:	No surface coarse fragments
	Profile Morphology
	A1	0 - 0.2 m	Dark reddish brown (5YR3/3-Moist); ; Light clay; Strong grade of structure, 5-10 mm, Angular 
	blocky; Moist; Weak consistence; Field pH 6.8 (pH meter); Many, very fine (0-1mm) roots; 
	Gradual change to - 
	B2	0.2 - 0.29 m	Dark red (2.5YR3/5-Moist); ; Medium clay; Strong grade of structure, 10-20 mm, Angular blocky;
	 Moist; Firm consistence; Field pH 7.2 (pH meter); Common, very fine (0-1mm) roots; Gradual 
	change to - 
	B2	0.29 - 0.53 m	Dark red (2.5YR3/6-Moist); ; Heavy clay; Moderate grade of structure, 5-10 mm, Angular blocky;
	 Moist; Weak consistence; Very few (0 - 2 %), Unidentified, , Nodules; Field pH 7 (pH meter); 
	Few, very fine (0-1mm) roots; Gradual change to - 
	B2	0.53 - 0.81 m	Dark red (2.5YR3/6-Moist); ; Heavy clay; Moderate grade of structure, 5-10 mm, Angular blocky;
	 Moist; Weak consistence; 0-2%, medium gravelly, 6-20mm, Basalt, coarse fragments; Very 
	few (0 - 2 %), Unidentified, , Nodules; Field pH 7.1 (pH meter); Few, very fine (0-1mm) roots; 
	Diffuse change to - 
	B31	0.81 - 1.07 m	Dark red (2.5YR3/6-Moist); ; Heavy clay; Moderate grade of structure, 5-10 mm, Angular blocky;
	 Moist; Weak consistence; 0-2%, medium gravelly, 6-20mm, Basalt, coarse fragments; Very 
	few (0 - 2 %), Unidentified, , Nodules; Field pH 6.6 (pH meter); Few, very fine (0-1mm) roots; 
	Diffuse change to - 
	B32	1.12 - 1.52 m	Reddish brown (5YR4/4-Moist); , 10YR76; , 10YR51; Light clay; Weak grade of structure, 
	Angular blocky; Moist; Weak consistence; 20-50%, medium gravelly, 6-20mm, Basalt, coarse 
	fragments; Field pH 6.8 (pH meter); 
	Morphological Notes
	Observation Notes
	PREVIOUSLY EUCALYPT WOODLAND (EUORG)                                                                                    
	Site Notes
	DARLING DOWNS

	Project Name:	DD
	Project Code:	DD	Site ID:	B216	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.2	6.8H	 0.02B	 20.7K	 6.1	 1.6	 0	 14.7D
	0.2 - 0.29	7.2H	 0.02B	 13.4K	 5.8	 0.79	 0	 11.1D
	0.29 - 0.53	7H	 0.02B
	0.53 - 0.81	7.1H	 0.02B	 8.4K	 7.4	 0.49	 0.3	 10.7D
	0.81 - 1.07	6.6H	 0.01B
	1.12 - 1.52	6.8H	 0.01B
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.2	 3.95A	 106C	 0.409F	 0.26B	1.30	 1	 1C	 13	 15	 63
	0.2 - 0.29	 1.28A	1.50	 0.5	 0.7C	 9	 11	 79
	0.29 - 0.53	 0.67A	 51C	 0.317F	1.30	 0.2	 0.5C	 6	 7	 86
	0.53 - 0.81	 0.36A	 0.2	 0.2C	 7	 11	 82
	0.81 - 1.07	 0.17A	 0.2	 0.7C	 10	 16	 74
	1.12 - 1.52	 0.11A	 0.29F	 0.2	 2C	 26	 32	 40
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.2	 0.3C
	0.2 - 0.29	 0.4C
	0.29 - 0.53	 0.37C
	0.53 - 0.81
	0.81 - 1.07
	1.12 - 1.52

	Project Name:	DD
	Project Code:	DD	Site ID:	B216	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Analyses Completed for this profile
	15_NR_CA	Exch. basic cations (Ca++) - meq per 100g of soil - Not recorded
	15_NR_H	Hydrogen Cation - meq per 100g of soil - Not recorded
	15_NR_K	Exch. basic cations (K++) - meq per 100g of soil - Not recorded
	15_NR_MG	Exch. basic cations (Mg++) - meq per 100g of soil - Not recorded
	15_NR_NA	Exch. basic cations (Na++) - meq per 100g of soil - Not recorded
	2_LOI	Loss on Ignition (%)
	2A1	Air-dry moisture content
	3_NR	Electrical conductivity or soluble salts - Not recorded
	4_NR	pH of soil - Not recorded
	5_NR	Water soluble Chloride - Cl(%) - Not recordede
	6A1	Organic carbon - Walkley and Black
	7_NR	Total nitrogen (%) - Not recorded
	9_NR	Available P (mg/kg) - Not recorded
	9A_NR	Total element - P(%) - Not recorded
	P10_GRAV	Gravel (%)
	P10_NR_C	Clay (%) - Not recorded
	P10_NR_CS	Coarse sand (%) - Not recorded
	P10_NR_FS	Fine sand (%) - Not recorded
	P10_NR_Z	Silt (%) - Not recorded
	P3A_NR	Bulk density - Not recorded
	P3B_VL_15	15 BAR Moisture m3/m3 - Volumetric using pressure plate