Project Name:	DD
	Project Code:	DD	Site ID:	B229	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Site Information
	Desc. By:	G.D. Hubble	Locality:
	Date Desc.:	18/05/54	Elevation:	 1067 metres
	Map Ref.:	Sheet No. : 9342   1:100000	Rainfall:	1143
	Northing/Long.:	152.345555555556	Runoff:	Moderately rapid
	Easting/Lat.:	-27.9386111111111	Drainage:	Well drained
	Geology
	ExposureType:	Soil pit	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	  Tm	Substrate Material:	Auger boring, 2 m deep,Basalt 
	Land Form
	Rel/Slope Class: 	No Data	Pattern Type:	Plateau
	Morph. Type:	No Data	Relief:	No Data
	Elem. Type:	Hillslope	Slope Category:	No Data
	Slope:	8.7 % 	Aspect:	No Data
	Surface Soil Condition (dry):
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Humose-Acidic Dystrophic Red Ferrosol     	Principal Profile Form:	Gn3.11
	ASC Confidence:	Great Soil Group:	Krasnozem
	Analytical data are incomplete but reasonable confidence.
	Site Disturbance:	Limited clearing, for example selective logging
	Vegetation:
	Tall Strata - Tree, 12.01-20m, Closed or dense. *Species includes - None Recorded
	Surface Coarse Fragments:	0-2%, large Boulders, >2m, , Basalt
	Profile Morphology
	A1	0 - 0.06 m	Dark reddish brown (5YR3/4-Moist); ; Clay loam; Strong grade of structure, 2-5 mm, Granular; 
	Moist; Very weak consistence; Field pH 5.4 (pH meter); Abundant, coarse (>5mm) roots; Clear 
	change to - 
	B1	0.1 - 0.24 m	Dark reddish brown (2.5YR3/4-Moist); ; Light clay; Strong grade of structure, 5-10 mm, 
	Polyhedral; Moist; Weak consistence; Field pH 5.3 (pH meter); Abundant, coarse (>5mm) roots; 
	Gradual change to - 
	B2	0.24 - 0.48 m	Dark reddish brown (2.5YR3/4-Moist); ; Light medium clay; Strong grade of structure, 5-10 mm, 
	Polyhedral; Moist; Weak consistence; Field pH 5.1 (pH meter); Common, coarse (>5mm) roots; 
	Gradual change to - 
	B2	0.53 - 0.91 m	Dark red (2.5YR3/6-Moist); ; Medium clay; , Polyhedral; Moist; Weak consistence; 0-2%, Basalt, 
	coarse fragments; Field pH 5.1 (pH meter); Few, coarse (>5mm) roots; Gradual change to - 
	B2	0.91 - 1.37 m	Dark red (2.5YR3/6-Moist); ; Medium clay; , Polyhedral; Moist; Weak consistence; Field pH 5 (pH 
	meter); Few, very fine (0-1mm) roots; Diffuse change to - 
	B2	1.42 - 1.78 m	Reddish brown (2.5YR4/4-Moist); , 10YR81; Light medium clay; , Polyhedral; Moist; Weak 
	consistence; Field pH 4.9 (pH meter); Few, very fine (0-1mm) roots; 
	Morphological Notes
	Observation Notes
	0-6CM POROUS GRANULAR STRUCTURE                                                                                         
	Site Notes
	MISTAKE RANGE

	Project Name:	DD
	Project Code:	DD	Site ID:	B229	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.06	5.4H	 0.084B	 16.2K	 7.7	 1.3	 0.01	 44.4D
	0.1 - 0.24	5.3H	 0.038B
	0.24 - 0.48	5.1H	 0.023B
	0.53 - 0.91	5.1H	 0.013B
	0.91 - 1.37	5H	 0.013B	 0.22K	 1.7	 0.06	 0.26	 22.3D
	1.42 - 1.78	4.9H	 0.016B
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.06	 10.6A	 62C	 0.223F	 0.82B	 0.1	 3C	 9	 11	 55
	0.1 - 0.24	 5.94A	 0.3B
	0.24 - 0.48	 2.66A	 0	 2C	 10	 12	 67
	0.53 - 0.91
	0.91 - 1.37	 0.54A	 0	 1C	 21	 17	 63
	1.42 - 1.78
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.06
	0.1 - 0.24
	0.24 - 0.48
	0.53 - 0.91
	0.91 - 1.37
	1.42 - 1.78

	Project Name:	DD
	Project Code:	DD	Site ID:	B229	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Analyses Completed for this profile
	15_NR_CA	Exch. basic cations (Ca++) - meq per 100g of soil - Not recorded
	15_NR_H	Hydrogen Cation - meq per 100g of soil - Not recorded
	15_NR_K	Exch. basic cations (K++) - meq per 100g of soil - Not recorded
	15_NR_MG	Exch. basic cations (Mg++) - meq per 100g of soil - Not recorded
	15_NR_NA	Exch. basic cations (Na++) - meq per 100g of soil - Not recorded
	2_LOI	Loss on Ignition (%)
	2A1	Air-dry moisture content
	3_NR	Electrical conductivity or soluble salts - Not recorded
	4_NR	pH of soil - Not recorded
	5_NR	Water soluble Chloride - Cl(%) - Not recordede
	6A1	Organic carbon - Walkley and Black
	7_NR	Total nitrogen (%) - Not recorded
	9_NR	Available P (mg/kg) - Not recorded
	9A_NR	Total element - P(%) - Not recorded
	P10_GRAV	Gravel (%)
	P10_NR_C	Clay (%) - Not recorded
	P10_NR_CS	Coarse sand (%) - Not recorded
	P10_NR_FS	Fine sand (%) - Not recorded
	P10_NR_Z	Silt (%) - Not recorded