Project Name:	DD
	Project Code:	DD	Site ID:	B244	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Site Information
	Desc. By:	G.D. Hubble	Locality:
	Date Desc.:	06/10/54	Elevation:	No Data
	Map Ref.:	Sheet No. : 9142   1:100000	Rainfall:	610
	Northing/Long.:	151.317777777778	Runoff:	Moderately rapid
	Easting/Lat.:	-27.7097222222222	Drainage:	Moderately well drained
	Geology
	ExposureType:	Soil pit	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	 Qpc	Substrate Material:	Auger boring, 1 m deep,Unconsolidated 
	material (unidentified) 
	Land Form
	Rel/Slope Class: 	Gently undulating plains <9m  1-	Pattern Type:	Alluvial plain
	3%
	Morph. Type:	No Data	Relief:	No Data
	Elem. Type:	Plain	Slope Category:	No Data
	Slope:	0 % 	Aspect:	No Data
	Surface Soil Condition (dry):	Self-mulching
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Epicalcareous Self-Mulching Black Vertosol     	Principal Profile Form:	Ug5.15
	ASC Confidence:	Great Soil Group:	Black earth
	No analytical data are available but confidence is fair.
	Site Disturbance:	No effective disturbance other than grazing by hoofed animals
	Vegetation:
	Tall Strata - Tussock grass, 0.51-1m, Mid-dense. *Species includes - Dichanthium sericeum, Aristida species
	Surface Coarse Fragments:	No surface coarse fragments
	Profile Morphology
	AB	0 - 0.08 m	Very dark brown (10YR2/2-Moist); ; Heavy clay; Moderate grade of structure, 5-10 mm, 
	Granular; Many (>5 per 100mm2)  macropores, Moderately moist; Very firm consistence; 0-2%, 
	fine gravelly, 2-6mm, subrounded, Quartz, coarse fragments; Very few (0 - 2 %), Calcareous, 
	Fine (0 - 2 mm), Nodules; Field pH 8 (pH meter); Common, very fine (0-1mm) roots; Clear change
	B2	0.08 - 0.38 m	Very dark brown (10YR2/2-Moist); ; Heavy clay; Moderate grade of structure, Angular blocky; 
	Many (>5 per 100mm2)  macropores, Moist; Firm consistence; 0-2%, fine gravelly, 2-6mm, 
	subrounded, Quartz, coarse fragments; Few (2 - 10 %), Calcareous, Medium (2 -6 mm), 
	Nodules; Field pH 8.4 (pH meter); Common, very fine (0-1mm) roots; Gradual change to - 
	B2	0.38 - 0.91 m	Very dark greyish brown (10YR3/2-Moist); ; Heavy clay; Moderate grade of structure, 
	Lenticular; Moderately moist; Firm consistence; 0-2%, fine gravelly, 2-6mm, subrounded, 
	Quartz, coarse fragments; Few (2 - 10 %), Calcareous, Medium (2 -6 mm), Nodules; Field pH 
	8.7 (pH meter); Few, very fine (0-1mm) roots; 
	Morphological Notes
	Observation Notes
	0-8CM GRANULAR GRADING TO BLOCKY STRUCTURE:PUFF PROFILE:ANT CAVATIES DOWN PROFILE FACE:                           
	      
	Site Notes
	DARLING DOWNS

	Project Name:	DD
	Project Code:	DD	Site ID:	B244	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.08	8H	 0.056B
	0.08 - 0.38	8.4H	 0.069B
	0.38 - 0.91	8.7H	 0.113B
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.08	 1.66A	 2259C	 0.3
	0.08 - 0.38	 0.97A	 3
	0.38 - 0.91	 0.61A	 5
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.08
	0.08 - 0.38
	0.38 - 0.91

	Project Name:	DD
	Project Code:	DD	Site ID:	B244	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Analyses Completed for this profile
	2A1	Air-dry moisture content
	3_NR	Electrical conductivity or soluble salts - Not recorded
	4_NR	pH of soil - Not recorded
	5_NR	Water soluble Chloride - Cl(%) - Not recordede
	6A1	Organic carbon - Walkley and Black
	9_NR	Available P (mg/kg) - Not recorded
	P10_GRAV	Gravel (%)