Project Name:	DD
	Project Code:	DD	Site ID:	B256	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Site Information
	Desc. By:	G.D. Hubble	Locality:
	Date Desc.:	14/10/54	Elevation:	No Data
	Map Ref.:	Sheet No. : 9142   1:100000	Rainfall:	686
	Northing/Long.:	151.038888888889	Runoff:	Moderately rapid
	Easting/Lat.:	-27.6166666666667	Drainage:	Imperfectly drained
	Geology
	ExposureType:	Soil pit	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	QsJk	Substrate Material:	Auger boring, 2 m deep,Unconsolidated 
	material (unidentified) 
	Land Form
	Rel/Slope Class: 	No Data	Pattern Type:	Low hills
	Morph. Type:	No Data	Relief:	No Data
	Elem. Type:	Hillslope	Slope Category:	No Data
	Slope:	0 % 	Aspect:	No Data
	Surface Soil Condition (dry):	Soft
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Magnesic Mottled-Subnatric Grey Sodosol     	Principal Profile Form:	Dg2.81
	ASC Confidence:	Great Soil Group:	Soloth
	All necessary analytical data are available.
	Site Disturbance:	No effective disturbance other than grazing by hoofed animals
	Vegetation:
	Mid Strata - Shrub, , . *Species includes - None recorded
	Tall Strata - Tree, 6.01-12m, Closed or dense. *Species includes - None Recorded
	Surface Coarse Fragments:	No surface coarse fragments
	Profile Morphology
	A1	0 - 0.08 m	Light grey (10YR7/2-Dry); ; Loamy fine sand; Massive grade of structure; Many (>5 per 
	100mm2) Very fine (0.075-1mm) macropores, Dry; Very weak consistence; 0-2%, fine gravelly,
	 2-6mm, Quartz, coarse fragments; Field pH 6.3 (pH meter); Common, very fine (0-1mm) roots; 
	Clear change to - 
	A21	0.08 - 0.38 m	Very pale brown (10YR8/4-Dry); ; Fine sand; Massive grade of structure; Many (>5 per 
	100mm2) Very fine (0.075-1mm) macropores, Dry; Very weak consistence; 0-2%, fine gravelly,
	 2-6mm, Quartz, coarse fragments; Field pH 5.9 (pH meter); Few, fine (1-2mm) roots; Gradual 
	A22	0.38 - 0.65 m	Very pale brown (10YR8/4-Moist); ; Fine sand; Massive grade of structure; Many (>5 per 
	100mm2) Very fine (0.075-1mm) macropores, Moist; Very weak consistence; 0-2%, fine 
	gravelly, 2-6mm, Quartz, coarse fragments; Field pH 6.4 (pH meter); Abrupt, Wavy change to - 
	B21	0.65 - 0.91 m	Light grey (2.5Y7/1-Moist); , 7.5YR68; Sandy clay loam; Massive grade of structure; Moist; 
	Weak consistence; 2-10%, fine gravelly, 2-6mm, Quartz, coarse fragments; Field pH 5.9 (pH 
	meter); Gradual change to - 
	B22	0.91 - 1.75 m	Brownish yellow (10YR6/8-Moist); , 2.5Y71; Sandy clay loam; Massive grade of structure; 
	Moist; Weak consistence; 0-2%, fine gravelly, 2-6mm, Quartz, coarse fragments; Field pH 6 (pH 
	meter); Gradual change to - 
	B23	1.75 - 2.08 m	Light grey (2.5Y7/1-Moist); , 10YR68; Medium clay; Massive grade of structure; Moist; Firm 
	consistence; 2-10%, fine gravelly, 2-6mm, Quartz, coarse fragments; Field pH 5.2 (pH meter); 
	Diffuse change to - 
	B24	2.08 - 2.18 m	White (2.5Y8/1-Moist); ; Sandy medium clay; Massive grade of structure; Very firm 
	consistence; Fragipan, Continuous, Massive; Field pH 5.4 (pH meter); 
	Morphological Notes
	Observation Notes
	Site Notes
	DARLING DOWNS

	Project Name:	DD
	Project Code:	DD	Site ID:	B256	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)

	Project Name:	DD
	Project Code:	DD	Site ID:	B256	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.08	6.3H	 0.008B
	0.08 - 0.38	5.9H	 0.003B
	0.38 - 0.65	6.4H	 0.003B
	0.65 - 0.91	5.9H	 0.045B	 0.15K	 3.1	 0.08	 0.93	 2.2D
	0.91 - 1.75	6H	 0.075B
	1.75 - 2.08	5.2H	 0.132B
	2.08 - 2.18	5.4H	 0.094B
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.08	 0.72A	 11C	 0.034F	 0.04B	 0	 57C	 34	 3	 3
	0.08 - 0.38	 0.01B
	0.38 - 0.65	 0.02A	 2	 53C	 41	 4	 2
	0.65 - 0.91	 0.05A	 7	 39C	 28	 4	 27
	0.91 - 1.75
	1.75 - 2.08	 0.02A	 0.038F	 2	 28C	 21	 3	 46
	2.08 - 2.18	 0.02A	 0	 59C	 25	 3	 32
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.08
	0.08 - 0.38
	0.38 - 0.65
	0.65 - 0.91
	0.91 - 1.75
	1.75 - 2.08
	2.08 - 2.18

	Project Name:	DD
	Project Code:	DD	Site ID:	B256	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Analyses Completed for this profile
	15_NR_CA	Exch. basic cations (Ca++) - meq per 100g of soil - Not recorded
	15_NR_H	Hydrogen Cation - meq per 100g of soil - Not recorded
	15_NR_K	Exch. basic cations (K++) - meq per 100g of soil - Not recorded
	15_NR_MG	Exch. basic cations (Mg++) - meq per 100g of soil - Not recorded
	15_NR_NA	Exch. basic cations (Na++) - meq per 100g of soil - Not recorded
	2A1	Air-dry moisture content
	3_NR	Electrical conductivity or soluble salts - Not recorded
	4_NR	pH of soil - Not recorded
	5_NR	Water soluble Chloride - Cl(%) - Not recordede
	6A1	Organic carbon - Walkley and Black
	7_NR	Total nitrogen (%) - Not recorded
	9_NR	Available P (mg/kg) - Not recorded
	9A_NR	Total element - P(%) - Not recorded
	P10_GRAV	Gravel (%)
	P10_NR_C	Clay (%) - Not recorded
	P10_NR_CS	Coarse sand (%) - Not recorded
	P10_NR_FS	Fine sand (%) - Not recorded
	P10_NR_Z	Silt (%) - Not recorded