Project Name:	EAR
	Project Code:	EAR	Site ID:	T345	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Site Information
	Desc. By:	R.J. Coventry	Locality:	18 Km E. of Torrens Ck.
	Date Desc.:	03/10/73	Elevation:	No Data
	Map Ref.:	Sheet No. : 7956   1:100000	Rainfall:	600
	Northing/Long.:	145.195833333333	Runoff:	No Data
	Easting/Lat.:	-20.7277777777778	Drainage:	No Data
	Geology
	ExposureType:	Undisturbed soil core	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	No Data	Pattern Type:	No Data
	Morph. Type:	No Data	Relief:	No Data
	Elem. Type:	No Data	Slope Category:	No Data
	Slope:	0 % 	Aspect:	No Data
	Surface Soil Condition (dry):	N/A
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Ferric Magnesic Grey Chromosol     	Principal Profile Form:	Dy5.62
	ASC Confidence:	Great Soil Group:	Gleyed podzolic 
	Analytical data are incomplete but reasonable confidence.	soil
	Site Disturbance:	No effective disturbance other than grazing by hoofed animals
	Vegetation:	Low Strata - Tussock grass, 0.51-1m, Sparse. *Species includes - Heteropogon contortus, Bothriochloa bladhii
	Tall Strata - Tree, 3.01-6m, Very sparse. *Species includes - None Recorded
	Surface Coarse Fragments:	No surface coarse fragments
	Profile Morphology
	A1	0 - 0.1 m	Dark grey (10YR4/1-Moist); Grey (10YR5/1-Dry); ; Sandy loam; Massive grade of structure; 
	Moderately moist; Weak consistence; Many, fine (1-2mm) roots; 
	A1	0.1 - 0.2 m	Dark grey (10YR4/1-Moist); Grey (10YR5/1-Dry); ; Sandy loam; Massive grade of structure; 
	Moderately moist; Weak consistence; Many, fine (1-2mm) roots; Gradual change to - 
	A2	0.2 - 0.3 m	Dark grey (10YR4/1-Moist); Grey (10YR6/1-Dry); ; Loamy sand; Massive grade of structure; 
	Moderately moist; Weak consistence; Many, very fine (0-1mm) roots; 
	A2	0.3 - 0.45 m	Dark grey (10YR4/1-Moist); Grey (10YR6/1-Dry); ; Loamy sand; Massive grade of structure; 
	Moderately moist; Weak consistence; Many, very fine (0-1mm) roots; Abrupt change to - 
	B2	0.45 - 0.6 m	Grey (10YR5/1-Moist); , 7.5YR56; , 5YR56; Sandy medium clay; Massive grade of structure; 
	Moist; Very firm consistence; Very few (0 - 2 %), Ferruginous, , Nodules; 
	B2	0.6 - 0.9 m	Grey (10YR5/1-Moist); , 7.5YR56; , 5YR56; Sandy medium clay; Massive grade of structure; 
	Moist; Very firm consistence; Few (2 - 10 %), Ferruginous, , Nodules; 
	B2	0.9 - 1.2 m	Grey (10YR5/1-Moist); , 7.5YR56; , 5YR56; Sandy medium clay; Massive grade of structure; 
	Dry; Strong consistence; Common (10 - 20 %), Ferruginous, , Nodules; 
	B2	1.2 - 1.5 m	Grey (10YR5/1-Moist); , 5YR57; , 2.5YR47; Sandy medium clay; Massive grade of structure; 
	Dry; Strong consistence; Common (10 - 20 %), Ferruginous, , Nodules; 
	B2	1.5 - 1.65 m	Grey (10YR5/1-Moist); , 5YR57; , 2.5YR47; Sandy medium clay; Massive grade of structure; 
	Dry; Strong consistence; 0-2%, rounded, Quartz, coarse fragments; Common (10 - 20 %), 
	Ferruginous, , Nodules; Diffuse change to - 
	B3	1.65 - 1.8 m	Grey (10YR5/1-Moist); , 5YR57; , 2.5YR47; Sandy medium clay; Massive grade of structure; 
	Dry; Strong consistence; 0-2%, rounded, Quartz, coarse fragments; Many (20 - 50 %), 
	Ferruginous, , Nodules; Abrupt change to - 
	C	1.8 - 2.1 m	Strong brown (7.5YR4/7-Moist); , 5YR58; , 10YR61; Sandy medium clay; Massive grade of 
	structure; Dry; Very strong consistence; 0-2%, rounded, Quartz, coarse fragments; Many (20 -
	 50 %), Ferruginous, , Nodules; 

	Project Name:	EAR
	Project Code:	EAR	Site ID:	T345	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	C	2.1 - 2.4 m	Strong brown (7.5YR4/7-Moist); , 5YR58; , 10YR61; Sandy medium clay; Massive grade of 
	structure; Dry; Very strong consistence; 2-10%, rounded, Quartz, coarse fragments; Few (2 - 
	10 %), Ferruginous, , Nodules; 
	C	2.4 - 2.7 m	Strong brown (7.5YR4/7-Moist); , 5YR58; , 10YR61; Sandy medium clay; Massive grade of 
	structure; Dry; Very strong consistence; 10-20%, rounded, Quartz, coarse fragments; 
	Morphological Notes
	Observation Notes
	RUSTY LINING TO ROOT CHANNELS.                                                                                          
	Site Notes
	TORRENS CK

	Project Name:	EAR
	Project Code:	EAR	Site ID:	T345	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.1	5.2A	 0.038A	 0.03H	 0.44	 0.09	 0.2	 0.65F	 1.44A	 1.4F	13.89
	 2.9C	6.90
	0.1 - 0.2	5.7A	 0.022A
	0.2 - 0.3	6.1A	 0.021A	<0.02H	 0.5	 0.04	 0.22	 1.18F	 1.2A	 2F	18.33
	 1.2C
	0.3 - 0.45	6.1A	 0.014A
	0.45 - 0.6	6.1A	 0.027A	<0.02H	 2.14	 0.04	 0.36	 0.52F	 3.17A	 3.1F	11.36
	 3.4C	10.59
	0.6 - 0.9	6A	 0.038A	 0.04H	 3.4	 0.04	 0.55	 0.38F	 4.19A	 4.4F	13.13
	 5.2C	10.58
	0.9 - 1.2	6.5A	 0.032A
	1.2 - 1.5	6.8A	 0.026A	 0.06H	 3.05	 0.04	 0.55	 0.16F	 4.49A	 3.9F	12.25
	 4.5C	12.22
	1.5 - 1.65	6.7A	 0.026A
	1.65 - 1.8	6.7A	 0.029A
	1.8 - 2.1	6.7A	 0.044A
	2.1 - 2.4	6.7A	 0.044A
	2.4 - 2.7	6.2A	 0.088A
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.1	 0.8D	 5B	 0.005A	 0.052A	 0.05A	 35A	 47	 8	 10
	0.1 - 0.2	 0.36D	 2B	 0.041A	 35A	 48	 7	 10
	0.2 - 0.3	 0.24D	 2B	 0.004A	 0.015A	 0.04A	 1	 36A	 49	 7	 8
	0.3 - 0.45	 1	 39A	 50	 6	 4
	0.45 - 0.6	 1	 33A	 31	 4	 32
	0.6 - 0.9	 0.007A	 0.1A	 10	 29A	 25	 5	 41
	0.9 - 1.2	 14	 28A	 25	 6	 41
	1.2 - 1.5	 13	 36A	 24	 7	 33
	1.5 - 1.65	 15	 37A	 24	 6	 32
	1.65 - 1.8	 25	 38A	 24	 7	 30
	1.8 - 2.1	 44	 32A	 24	 7	 37
	2.1 - 2.4	 48	 36A	 22	 6	 36
	2.4 - 2.7	 48	 40A	 22	 9	 30
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.1
	0.1 - 0.2
	0.2 - 0.3
	0.3 - 0.45
	0.45 - 0.6
	0.6 - 0.9
	0.9 - 1.2
	1.2 - 1.5
	1.5 - 1.65
	1.65 - 1.8

	Project Name:	EAR
	Project Code:	EAR	Site ID:	T345	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	1.8 - 2.1
	2.1 - 2.4
	2.4 - 2.7

	Project Name:	EAR
	Project Code:	EAR	Site ID:	T345	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Analyses Completed for this profile
	10A1	Total sulfur - X-ray fluorescence
	13C1_FE	Citrate/dithionite-extractable iron, aluminium, Manganese and Silicon
	15A2_CEC	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	15D1_CEC	CEC - 1M ammonium acetate at pH 7.0, pretreatment for soluble salts; manual leach
	15E1_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) by compulsive exchange, no pretreatment for soluble 
	15E1_K	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15E1_MG	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15E1_NA	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15G_C	Exchange acidity (hydrogen and aluminium) - meq per 100g of soil - By 1M KCl exch. acidity by 
	titration to pH 8.4
	15J1	Effective CEC
	17A1	Total potassium - X-ray fluorescence
	2A1	Air-dry moisture content
	3A1	EC of 1:5 soil/water extract
	4A1	pH of 1:5 soil/water suspension
	6A1_UC	Organic carbon (%) - Uncorrected Walkley and Black method
	7A2	Total nitrogen - semimicro Kjeldahl , automated colour
	9A1	Total phosphorus - X-ray fluorescence
	9G_BSES	Available P (mg/kg) - Acid P - 0.005M H2SO4 (BSES)
	MIN_EC	Exchange Capacity - Minerology
	P10_CF_C	Clay (%) - Coventry and Fett pipette method
	P10_CF_CS	Coarse sand (%) - Coventry and Fett pipette method
	P10_CF_FS	Fine sand (%) - Coventry and Fett pipette method
	P10_CF_Z	Silt (%) - Coventry and Fett pipette method
	P10_GRAV	Gravel (%)
	XRD_C_Ch	Chlorite - X-Ray Diffraction
	XRD_C_Hm	Hematite - X-Ray Diffraction
	XRD_C_K2O	K2O - X-Ray Diffraction or Clay Fraction (air dry)
	XRD_C_Ka	Kaolin - X-Ray Diffraction
	XRD_C_Qz	Quartz - X-Ray Diffraction
	XRD_C_Vm	Vermiculte - X-Ray Diffraction