Project Name:	GYC
	Project Code:	GYC	Site ID:	B527	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Site Information
	Desc. By:	G.D. Hubble	Locality:
	Date Desc.:	19/11/63	Elevation:	 80 metres
	Map Ref.:	Sheet No. : 9445   1:100000	Rainfall:	1143
	Northing/Long.:	152.654166666667	Runoff:	Rapid
	Easting/Lat.:	-26.2138888888889	Drainage:	Moderately well drained
	Geology
	ExposureType:	Soil pit	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	 Rlk	Substrate Material:	Shale 
	Land Form
	Rel/Slope Class: 	No Data	Pattern Type:	Low hills
	Morph. Type:	No Data	Relief:	30 metres
	Elem. Type:	Hillslope	Slope Category:	No Data
	Slope:	0 % 	Aspect:	No Data
	Surface Soil Condition (dry):	Hardsetting
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Acidic Class Undetermined Bleached Tenosol     	Principal Profile Form:	Um2.12
	ASC Confidence:	Great Soil Group:	Lithosol
	All necessary analytical data are available.
	Site Disturbance:	Complete clearing. Pasture, native or improved, but never cultivated
	Vegetation:	Low Strata - Tussock grass, , . *Species includes - None recorded
	Tall Strata - Tree, 6.01-12m, Mid-dense. *Species includes - Eucalyptus punctata, Eucalyptus species
	Surface Coarse Fragments:	No surface coarse fragments
	Profile Morphology
	A1	0 - 0.06 m	Very dark greyish brown (10YR3/2-Moist); ; Loam; Weak grade of structure, 5-10 mm, 
	Polyhedral; Few (<1 per 100mm2) Fine (1-2mm) macropores, Dry; Weak consistence; 10-20%, 
	fine gravelly, 2-6mm, coarse fragments; Field pH 5.7 (pH meter); Many, fine (1-2mm) roots; 
	Clear change to - 
	A2	0.06 - 0.28 m	Pale brown (10YR6/3-Moist); ; Loam; Massive grade of structure; Few (<1 per 0.01m2) Coarse 
	(>5mm) macropores, Moderately moist; Firm consistence; 20-50%, coarse gravelly, 20-60mm, 
	coarse fragments; Field pH 5.3 (pH meter); Few, fine (1-2mm) roots; Clear change to - 
	C	0.28 - 0.46 m	Red (10R4/6-Moist); , 10YR72, 10-20% , 15-30mm, Prominent; , 10-20% , 15-30mm, Prominent; 
	Loam; Massive grade of structure; 
	Morphological Notes
	Observation Notes
	Site Notes
	GYMPIE

	Project Name:	GYC
	Project Code:	GYC	Site ID:	B527	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.06	5.7H	 0.02B	 2.4K	 3.5	 0.8	 0.41	 10.8D
	0.06 - 0.28	5.3H	 0.01B	 0.05K	 0.9	 0.39	 0.22	 11.9D
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.06	 2.33A	 21C	 0.029F	 0.17B	 15	 20C	 27	 31	 16
	0.06 - 0.28	 0.76A	 5C	 0.016F	 0.079B	 25	 19C	 24	 35	 21
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.06
	0.06 - 0.28

	Project Name:	GYC
	Project Code:	GYC	Site ID:	B527	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Analyses Completed for this profile
	15_NR_CA	Exch. basic cations (Ca++) - meq per 100g of soil - Not recorded
	15_NR_H	Hydrogen Cation - meq per 100g of soil - Not recorded
	15_NR_K	Exch. basic cations (K++) - meq per 100g of soil - Not recorded
	15_NR_MG	Exch. basic cations (Mg++) - meq per 100g of soil - Not recorded
	15_NR_NA	Exch. basic cations (Na++) - meq per 100g of soil - Not recorded
	2A1	Air-dry moisture content
	3_NR	Electrical conductivity or soluble salts - Not recorded
	4_NR	pH of soil - Not recorded
	5_NR	Water soluble Chloride - Cl(%) - Not recordede
	6A1	Organic carbon - Walkley and Black
	7_NR	Total nitrogen (%) - Not recorded
	9_NR	Available P (mg/kg) - Not recorded
	9A_NR	Total element - P(%) - Not recorded
	P10_GRAV	Gravel (%)
	P10_NR_C	Clay (%) - Not recorded
	P10_NR_CS	Coarse sand (%) - Not recorded
	P10_NR_FS	Fine sand (%) - Not recorded
	P10_NR_Z	Silt (%) - Not recorded