Project Name:	GYC
	Project Code:	GYC	Site ID:	B534	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Site Information
	Desc. By:	G.D. Hubble	Locality:
	Date Desc.:	22/11/63	Elevation:	 110 metres
	Map Ref.:	Sheet No. : 9445   1:100000	Rainfall:	0
	Northing/Long.:	152.819444444444	Runoff:	Slow
	Easting/Lat.:	-26.1708333333334	Drainage:	Moderately well drained
	Geology
	ExposureType:	Soil pit	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	 Rlk	Substrate Material:	Soil pit, 1 m deep,Unconsolidated material 
	(unidentified) 
	Land Form
	Rel/Slope Class: 	No Data	Pattern Type:	Low hills
	Morph. Type:	No Data	Relief:	No Data
	Elem. Type:	Valley flat	Slope Category:	No Data
	Slope:	0 % 	Aspect:	No Data
	Surface Soil Condition (dry):
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Haplic Dystrophic Red Kandosol     	Principal Profile Form:	Gn2.14
	ASC Confidence:	Great Soil Group:	Red earth
	All necessary analytical data are available.
	Site Disturbance:	Limited clearing, for example selective logging
	Vegetation:	Low Strata - Tussock grass, , Closed or dense. *Species includes - Imperata cylindrica
	Mid Strata - Tree, , . *Species includes - Banksia integrifolia
	Tall Strata - Tree, , Mid-dense. *Species includes - Eucalyptus propinqua, Trigonella suavissima
	Surface Coarse Fragments:	No surface coarse fragments
	Profile Morphology
	A1	0 - 0.13 m	Dark brown (7.5YR3/2-Moist); ; Sandy loam (Heavy); Strong grade of structure, 2-5 mm, 
	Granular; Moist; Very weak consistence; 2-10%, medium gravelly, 6-20mm, Quartz, coarse 
	fragments; Very few (0 - 2 %), Manganiferous, Fine (0 - 2 mm), Nodules; Clear change to - 
	B1	0.13 - 0.24 m	Reddish brown (5YR4/3-Moist); ; Sandy clay loam; Weak grade of structure, 10-20 mm, 
	Subangular blocky; Moist; Very weak consistence; 2-10%, medium gravelly, 6-20mm, Quartz, 
	coarse fragments; Very few (0 - 2 %), Manganiferous, Fine (0 - 2 mm), Nodules; Gradual 
	change to - 
	B21	0.24 - 0.58 m	Dark red (2.5YR3/6-Moist); ; Sandy medium clay; Massive grade of structure; Earthy fabric; 
	Moist; Very weak consistence; 10-20%, coarse gravelly, 20-60mm, Sandstone, coarse 
	fragments; Gradual change to - 
	B22	0.58 - 0.91 m	Red (2.5YR4/6-Moist); ; Sandy medium clay; Massive grade of structure; Earthy fabric; Moist; 
	Weak consistence; 20-50%, coarse gravelly, 20-60mm, Sandstone, coarse fragments; 
	Morphological Notes
	Observation Notes
	0-13CM POROUS GRANULAR STRUCTURE.                                                                                       
	Site Notes
	NEUSAVALE

	Project Name:	GYC
	Project Code:	GYC	Site ID:	B534	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.13	5.6H	 0.01B	 1.1K	 0.87	 0.14	 0.33	 11.1D
	0.13 - 0.24	5.4H	 0.01B	 0.51K	 0.56	 0.04	 0.32	 6.3D
	0.24 - 0.58	5.9H	 0.01B	 0.46K	 0.39	 0.02	 0.2	 6.4D
	0.58 - 0.91	6H	 0.01B
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.13	 1.83A	 6C	 0.026F	 0.146B	 3	 44C	 22	 14	 15
	0.13 - 0.24	 0.93A	 10	 43C	 21	 14	 18
	0.24 - 0.58	 0.44A	 0.023F	 17	 40C	 20	 14	 27
	0.58 - 0.91	 45	 32C	 16	 12	 42
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.13
	0.13 - 0.24
	0.24 - 0.58
	0.58 - 0.91

	Project Name:	GYC
	Project Code:	GYC	Site ID:	B534	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Analyses Completed for this profile
	15_NR_CA	Exch. basic cations (Ca++) - meq per 100g of soil - Not recorded
	15_NR_H	Hydrogen Cation - meq per 100g of soil - Not recorded
	15_NR_K	Exch. basic cations (K++) - meq per 100g of soil - Not recorded
	15_NR_MG	Exch. basic cations (Mg++) - meq per 100g of soil - Not recorded
	15_NR_NA	Exch. basic cations (Na++) - meq per 100g of soil - Not recorded
	2A1	Air-dry moisture content
	3_NR	Electrical conductivity or soluble salts - Not recorded
	4_NR	pH of soil - Not recorded
	5_NR	Water soluble Chloride - Cl(%) - Not recordede
	6A1	Organic carbon - Walkley and Black
	7_NR	Total nitrogen (%) - Not recorded
	9_NR	Available P (mg/kg) - Not recorded
	9A_NR	Total element - P(%) - Not recorded
	P10_GRAV	Gravel (%)
	P10_NR_C	Clay (%) - Not recorded
	P10_NR_CS	Coarse sand (%) - Not recorded
	P10_NR_FS	Fine sand (%) - Not recorded
	P10_NR_Z	Silt (%) - Not recorded