Project Name:	LBV
	Project Code:	LBV	Site ID:	B121	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Site Information
	Desc. By:	G.D. Hubble	Locality:	29 miles north of Springsure on main road to 
	Date Desc.:	01/06/50	Elevation:	 259 metres
	Map Ref.:	Sheet No. : 8550   1:100000	Rainfall:	610
	Northing/Long.:	148.083333333333	Runoff:	Very slow
	Easting/Lat.:	-23.7166666666667	Drainage:	Poorly drained
	Geology
	ExposureType:	Soil pit	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	  TB	Substrate Material:	Soil pit, 0.84 m deep,Slightly porous, 
	Land Form
	Rel/Slope Class: 	Undulating rises 9-30m 3-10%	Pattern Type:	Rises
	Morph. Type:	No Data	Relief:	15 metres
	Elem. Type:	Hillslope	Slope Category:	No Data
	Slope:	0 % 	Aspect:	No Data
	Surface Soil Condition (dry):
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Epicalcareous Epipedal Black Vertosol     	Principal Profile Form:	Ug5.12
	ASC Confidence:	Great Soil Group:	Black earth
	All necessary analytical data are available.
	Site Disturbance:	No effective disturbance other than grazing by hoofed animals
	Vegetation:
	Tall Strata - Tussock grass, 0.51-1m, Mid-dense. *Species includes - None Recorded
	Surface Coarse Fragments:	No surface coarse fragments
	Profile Morphology
	AB	0 - 0.15 m	Very dark grey (10YR3/1-Moist); ; Heavy clay; Strong grade of structure, Granular; Dry; Firm 
	consistence; Very few (0 - 2 %), Calcareous, , Concretions; Field pH 7.9 (pH meter); Gradual 
	change to - 
	B2	0.15 - 0.46 m	Very dark grey (10YR3/1-Moist); ; Heavy clay; Moderate grade of structure, Angular blocky; Dry; 
	Very firm consistence; Very few (0 - 2 %), Calcareous, , Concretions; Field pH 8.1 (pH meter); 
	Diffuse change to - 
	B2	0.46 - 0.84 m	Very dark grey (10YR3/1-Moist); ; Heavy clay; Moderate grade of structure, Lenticular; Dry; Very 
	firm consistence; Very few (0 - 2 %), Calcareous, , Concretions; Field pH 8.4 (pH meter); Diffuse
	 change to - 
	C	0.84 - 1.07 m	; 
	Morphological Notes
	C	Mottled weathered basalt
	Observation Notes
	0-15 GRANULAR GRADING TO MODERATE BLOCKY STRUCTURE                                                                      
	Site Notes
	SPRINGSURE

	Project Name:	LBV
	Project Code:	LBV	Site ID:	B121	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.15	7.9H	 0.02B	 43.5K	 23.5	 0.21	 0.35	 3.02D	 67.5J	 70.6E	0.52
	0.15 - 0.46	8.1H	 0.027B
	0.46 - 0.84	8.4H	 0.046B	 37.9K	 22	 0.16	 0.79	 60.8E
	0.84 - 1.07	8.8H	 0.062B
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.15	 0.081C	 22C	 0.029F	 0.065B	 3C	 14	 11	 61
	0.15 - 0.46	 1.04E
	0.46 - 0.84	 0.244C	 3C	 14	 9	 62
	0.84 - 1.07
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.15
	0.15 - 0.46
	0.46 - 0.84
	0.84 - 1.07

	Project Name:	LBV
	Project Code:	LBV	Site ID:	B121	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Analyses Completed for this profile
	15_NR	Sum of Ex. cations + Ex. acidity - Not recorded
	15_NR_CA	Exch. basic cations (Ca++) - meq per 100g of soil - Not recorded
	15_NR_CEC	CEC - meq per 100g of soil - Not recorded
	15_NR_H	Hydrogen Cation - meq per 100g of soil - Not recorded
	15_NR_K	Exch. basic cations (K++) - meq per 100g of soil - Not recorded
	15_NR_MG	Exch. basic cations (Mg++) - meq per 100g of soil - Not recorded
	15_NR_NA	Exch. basic cations (Na++) - meq per 100g of soil - Not recorded
	19B_NR	Calcium Carbonate (CaCO3) - Not recorded
	2_LOI	Loss on Ignition (%)
	2A1	Air-dry moisture content
	3_NR	Electrical conductivity or soluble salts - Not recorded
	4_NR	pH of soil - Not recorded
	5_NR	Water soluble Chloride - Cl(%) - Not recordede
	6Z	Organic carbon (%) - Not recorded
	7_NR	Total nitrogen (%) - Not recorded
	9_NR	Available P (mg/kg) - Not recorded
	9A_NR	Total element - P(%) - Not recorded
	P10_NR_C	Clay (%) - Not recorded
	P10_NR_CS	Coarse sand (%) - Not recorded
	P10_NR_FS	Fine sand (%) - Not recorded
	P10_NR_Z	Silt (%) - Not recorded