Project Name:	LBV
	Project Code:	LBV	Site ID:	B19	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Site Information
	Desc. By:	G.D. Hubble	Locality:
	Date Desc.:	14/10/48	Elevation:	 33 metres
	Map Ref.:	Sheet No. : 8358   1:100000	Rainfall:	800
	Northing/Long.:	147.155555555556	Runoff:	Slow
	Easting/Lat.:	-19.8888888888889	Drainage:	Imperfectly drained
	Geology
	ExposureType:	Soil pit	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	  Qu	Substrate Material:	Auger boring, 0.9 m deep,Porous, 
	Unconsolidated material (unidentified) 
	Land Form
	Rel/Slope Class: 	No Data	Pattern Type:	Plain
	Morph. Type:	No Data	Relief:	No Data
	Elem. Type:	Fan	Slope Category:	No Data
	Slope:	0 % 	Aspect:	No Data
	Surface Soil Condition (dry):	Soft
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Eutrophic Mottled-Mesonatric Grey Sodosol     	Principal Profile Form:	Dy5.43
	ASC Confidence:	Great Soil Group:	Solodized solonetz
	All necessary analytical data are available.
	Site Disturbance:	No effective disturbance other than grazing by hoofed animals
	Vegetation:	Low Strata - Tussock grass, , Very sparse. *Species includes - Heteropogon contortus, Heteropogon triticeus
	Tall Strata - Tree, 6.01-12m, Very sparse. *Species includes - None Recorded
	Surface Coarse Fragments:	No surface coarse fragments
	Profile Morphology
	A1	0 - 0.1 m	Light brownish grey (10YR6/2-Moist); ; Sand; Massive grade of structure; Many (>5 per 100mm2) 
	Fine (1-2mm) macropores, Dry; Field pH 6.4 (pH meter); Gradual change to - 
	A21	0.1 - 0.23 m	Light grey (10YR7/2-Moist); ; Sand; Massive grade of structure; Many (>5 per 100mm2) Fine (1-
	2mm) macropores, Dry; Very weak consistence; Field pH 6.8 (pH meter); Gradual change to - 
	A22	0.23 - 0.36 m	Light grey (10YR7/2-Moist); ; Sand; Massive grade of structure; Many (>5 per 100mm2) Fine (1-
	2mm) macropores, Dry; Very weak consistence; 0-2%, fine gravelly, 2-6mm, Quartz, coarse 
	fragments; Field pH 6.9 (pH meter); Abrupt change to - 
	B21	0.36 - 0.43 m	Grey (10YR5/1-Moist); , 10YR56; , 7.5YR44; Sandy medium clay; Strong grade of structure, 100-
	200 mm, Columnar; Moderately moist; Strong consistence; 10-20%, fine gravelly, 2-6mm, 
	Quartz, coarse fragments; Very few (0 - 2 %), Manganiferous, , Soft segregations; Field pH 6.3 
	(pH meter); Gradual change to - 
	B22	0.43 - 0.61 m	Grey (10YR5/1-Moist); , 10YR56; Sandy medium clay; Moderate grade of structure, 100-200 mm, 
	Columnar; Moderately moist; Strong consistence; 10-20%, fine gravelly, 2-6mm, Quartz, coarse 
	fragments; Field pH 7.3 (pH meter); Diffuse change to - 
	B3	0.66 - 0.99 m	Grey (10YR6/1-Moist); , 10YR68; Coarse sandy medium clay; Massive grade of structure; Moist; 
	Weak consistence; 50-90%, fine gravelly, 2-6mm, Quartz, coarse fragments; Field pH 9.7 (pH 
	meter); 
	Morphological Notes
	Observation Notes
	Site Notes
	BURDEKIN VALLE

	Project Name:	LBV
	Project Code:	LBV	Site ID:	B19	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.1	6.4H	 0.01B	 0.62K	 0.43	 0.17	 0.07	 1.9D	 3.2E
	0.1 - 0.23	6.8H	 0.06B
	0.23 - 0.36	6.9H	 0.01B
	0.36 - 0.43	6.3H	 0.06B	 1K	 4.2	 0.03	 2.4	 3.6D	 11.2E
	0.43 - 0.61	7.3H	 0.08B
	0.66 - 0.99	9.7H	 0.18B	 2.2K	 5	 0.23	 6.9	 14.3E
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.1	 3C	 0.04B	 57C	 36	 5	 4
	0.1 - 0.23	 53C	 38	 4	 4
	0.23 - 0.36	 54C	 39	 4	 3
	0.36 - 0.43	 38C	 24	 10	 25
	0.43 - 0.61	 40C	 27	 4	 26
	0.66 - 0.99	 1C	 35C	 28	 5	 30
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.1
	0.1 - 0.23
	0.23 - 0.36
	0.36 - 0.43
	0.43 - 0.61
	0.66 - 0.99

	Project Name:	LBV
	Project Code:	LBV	Site ID:	B19	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Analyses Completed for this profile
	15_NR	Sum of Ex. cations + Ex. acidity - Not recorded
	15_NR_CA	Exch. basic cations (Ca++) - meq per 100g of soil - Not recorded
	15_NR_H	Hydrogen Cation - meq per 100g of soil - Not recorded
	15_NR_K	Exch. basic cations (K++) - meq per 100g of soil - Not recorded
	15_NR_MG	Exch. basic cations (Mg++) - meq per 100g of soil - Not recorded
	15_NR_NA	Exch. basic cations (Na++) - meq per 100g of soil - Not recorded
	19B_NR	Calcium Carbonate (CaCO3) - Not recorded
	2_LOI	Loss on Ignition (%)
	2A1	Air-dry moisture content
	3_NR	Electrical conductivity or soluble salts - Not recorded
	4_NR	pH of soil - Not recorded
	5_NR	Water soluble Chloride - Cl(%) - Not recordede
	7_NR	Total nitrogen (%) - Not recorded
	9_NR	Available P (mg/kg) - Not recorded
	P10_NR_C	Clay (%) - Not recorded
	P10_NR_CS	Coarse sand (%) - Not recorded
	P10_NR_FS	Fine sand (%) - Not recorded
	P10_NR_Z	Silt (%) - Not recorded