Project Name:	LBV
	Project Code:	LBV	Site ID:	B41	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Site Information
	Desc. By:	G.D. Hubble	Locality:
	Date Desc.:	17/08/50	Elevation:	 70 metres
	Map Ref.:	Sheet No. : 8357   1:100000	Rainfall:	750
	Northing/Long.:	147.325	Runoff:	Slow
	Easting/Lat.:	-20.34	Drainage:	Imperfectly drained
	Geology
	ExposureType:	Soil pit	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	 CZA	Substrate Material:	Auger boring, 2 m deep,Porous, 
	Unconsolidated material (unidentified) 
	Land Form
	Rel/Slope Class: 	Gently undulating plains <9m  	Pattern Type:	Alluvial plain
	1-3%
	Morph. Type:	No Data	Relief:	No Data
	Elem. Type:	Levee	Slope Category:	No Data
	Slope:	0 % 	Aspect:	No Data
	Surface Soil Condition (dry):	Hardsetting
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Eutrophic Subnatric Red Sodosol     	Principal Profile Form:	Dy3.42
	ASC Confidence:	Great Soil Group:	Solodic soil
	No analytical data are available but confidence is fair.
	Site Disturbance:
	Vegetation:	Low Strata - Tussock grass, , Mid-dense. *Species includes - Heteropogon triticeus, Heteropogon contortus
	Tall Strata - Tree, 6.01-12m, Sparse. *Species includes - None Recorded
	Surface Coarse Fragments:	No surface coarse fragments
	Profile Morphology
	A1	0 - 0.1 m	Brown (7.5YR4/2-Moist); ; Loamy fine sand; Massive grade of structure; Weak grade of structure,
	 Granular; Many (>5 per 100mm2)  macropores, Moist; Very weak consistence; Field pH 6.7 (pH 
	meter); FewGradual change to - 
	A2	0.1 - 0.36 m	Strong brown (7.5YR5/5-Moist); ; Loamy fine sand; Massive grade of structure, Granular; Many 
	(>5 per 100mm2)  macropores, Moist; Very weak consistence; Field pH 7 (pH meter); FewDiffuse
	 change to - 
	A2	0.36 - 0.71 m	Very pale brown (10YR7/4-Moist); ; Clay loam, fine sandy; Massive grade of structure; Many (>5 
	per 100mm2)  macropores, Moist; Very weak consistence; Few (2 - 10 %), Manganiferous, 
	Medium (2 -6 mm), Nodules; Field pH 6.9 (pH meter); FewClear change to - 
	B21	0.71 - 0.86 m	Reddish yellow (5YR6/6-Moist); ; Light medium clay; , Prismatic; Moderate grade of structure, 
	20-50 mm, Angular blocky; Moist; Firm consistence; Field pH 7.3 (pH meter); Diffuse change to - 
	B22	0.86 - 1.17 m	Reddish yellow (5YR6/7-Moist); ; Fine sandy medium clay; Massive grade of structure; Moist; 
	Very weak consistence; Few (2 - 10 %), , Medium (2 -6 mm), Soft segregations; Field pH 7.8 (pH 
	meter); Diffuse change to - 
	B3	1.17 - 1.83 m	Reddish yellow (5YR6/7-Moist); ; Fine sandy clay loam; Massive grade of structure; Moist; Very 
	weak consistence; Few (2 - 10 %), , Medium (2 -6 mm), Soft segregations; Field pH 8.3 (pH 
	meter); 
	Morphological Notes
	Observation Notes
	SAND DOWN FINE CRACKS 71-86CM                                                                                           
	Site Notes
	BURDEKIN VALLE

	Project Name:	LBV
	Project Code:	LBV	Site ID:	B41	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.1	6.7H	 0.01B
	0.1 - 0.36	7H	 0.01B
	0.36 - 0.71	6.9H	 0.02B
	0.71 - 0.86	7.3H	 0.02B
	0.86 - 1.17	7.8H	 0.02B
	1.17 - 1.83	8.3H	 0.04B
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.1	 36C	 0.017F	 0.04B	 10C	 72	 11	 6
	0.1 - 0.36
	0.36 - 0.71
	0.71 - 0.86	 8C	 49	 9	 34
	0.86 - 1.17
	1.17 - 1.83	 0.01C	 6C	 57	 12	 26
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.1
	0.1 - 0.36
	0.36 - 0.71
	0.71 - 0.86
	0.86 - 1.17
	1.17 - 1.83

	Project Name:	LBV
	Project Code:	LBV	Site ID:	B41	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Analyses Completed for this profile
	19B_NR	Calcium Carbonate (CaCO3) - Not recorded
	2_LOI	Loss on Ignition (%)
	2A1	Air-dry moisture content
	3_NR	Electrical conductivity or soluble salts - Not recorded
	4_NR	pH of soil - Not recorded
	5_NR	Water soluble Chloride - Cl(%) - Not recordede
	7_NR	Total nitrogen (%) - Not recorded
	9_NR	Available P (mg/kg) - Not recorded
	9A_NR	Total element - P(%) - Not recorded
	P10_NR_C	Clay (%) - Not recorded
	P10_NR_CS	Coarse sand (%) - Not recorded
	P10_NR_FS	Fine sand (%) - Not recorded
	P10_NR_Z	Silt (%) - Not recorded