Project Name:	LBV
	Project Code:	LBV	Site ID:	B46	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Site Information
	Desc. By:	C.H. Thompson	Locality:
	Date Desc.:	06/09/50	Elevation:	 60 metres
	Map Ref.:	Sheet No. : 8357   1:100000	Rainfall:	750
	Northing/Long.:	147.4	Runoff:	No runoff
	Easting/Lat.:	-20.05	Drainage:	Poorly drained
	Geology
	ExposureType:	Soil pit	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	 PLZ	Substrate Material:	Auger boring, 3 m deep,Slightly porous, 
	Unconsolidated material (unidentified) 
	Land Form
	Rel/Slope Class: 	Gently undulating plains <9m  	Pattern Type:	Alluvial plain
	1-3%
	Morph. Type:	No Data	Relief:	No Data
	Elem. Type:	Plain	Slope Category:	No Data
	Slope:	0 % 	Aspect:	No Data
	Surface Soil Condition (dry):	Self-mulching
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Epicalcareous-Endohypersodic Self-Mulching Grey Vertosol   	Principal Profile Form:	Ug5.24
	  
	ASC Confidence:	Great Soil Group:	Grey clay
	All necessary analytical data are available.
	Site Disturbance:	No effective disturbance other than grazing by hoofed animals
	Vegetation:	Low Strata - Tussock grass, , Very sparse. *Species includes - Chloris species
	Tall Strata - Tree, 3.01-6m, Mid-dense. *Species includes - Acacia species, Bassia species, Excoecaria parvifolia
	Surface Coarse Fragments:	No surface coarse fragments
	Profile Morphology
	A1	0 - 0.03 m	Light grey (2.5Y7/0-Moist); ; Heavy clay; Moderate grade of structure, 20-50 mm, Angular blocky; 
	Weak grade of structure, 10-20 mm, Granular; Dry; Firm consistence; Field pH 7 (pH meter); 
	Clear, Irregular change to - 
	B2	0.03 - 0.3 m	Grey (2.5Y6/0-Moist); ; Heavy clay; Moderate grade of structure, 50-100 mm, Angular blocky; Wet;
	 Very plastic; 0-2%, fine gravelly, 2-6mm, rounded, Quartz, coarse fragments; Field pH 8 (pH 
	meter); Diffuse change to - 
	B2	0.3 - 0.61 m	Grey (2.5Y5/0-Moist); ; Heavy clay; Weak grade of structure, 50-100 mm, Angular blocky; Wet; 
	Very plastic; 0-2%, fine gravelly, 2-6mm, rounded, Quartz, coarse fragments; Very few (0 - 2 %), 
	Manganiferous, Fine (0 - 2 mm), Soft segregations; Field pH 8.1 (pH meter); 
	Morphological Notes
	Observation Notes
	Site Notes
	BURDEKIN VALLE

	Project Name:	LBV
	Project Code:	LBV	Site ID:	B46	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.03	7H	 0.01B
	0.03 - 0.3	8H	 0.06B	 25.2K	 12.9	 0.63	 3.44	 2.1D	 44.3E
	0.3 - 0.61	8.1H	 0.37B
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.03	 18C	 0.012F
	0.03 - 0.3	 0.01C	 0.65E	 0.05B	 4C	 16	 21	 57
	0.3 - 0.61
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.03
	0.03 - 0.3
	0.3 - 0.61

	Project Name:	LBV
	Project Code:	LBV	Site ID:	B46	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Analyses Completed for this profile
	15_NR	Sum of Ex. cations + Ex. acidity - Not recorded
	15_NR_CA	Exch. basic cations (Ca++) - meq per 100g of soil - Not recorded
	15_NR_H	Hydrogen Cation - meq per 100g of soil - Not recorded
	15_NR_K	Exch. basic cations (K++) - meq per 100g of soil - Not recorded
	15_NR_MG	Exch. basic cations (Mg++) - meq per 100g of soil - Not recorded
	15_NR_NA	Exch. basic cations (Na++) - meq per 100g of soil - Not recorded
	19B_NR	Calcium Carbonate (CaCO3) - Not recorded
	2_LOI	Loss on Ignition (%)
	2A1	Air-dry moisture content
	3_NR	Electrical conductivity or soluble salts - Not recorded
	4_NR	pH of soil - Not recorded
	5_NR	Water soluble Chloride - Cl(%) - Not recordede
	6Z	Organic carbon (%) - Not recorded
	7_NR	Total nitrogen (%) - Not recorded
	9_NR	Available P (mg/kg) - Not recorded
	9A_NR	Total element - P(%) - Not recorded
	P10_NR_C	Clay (%) - Not recorded
	P10_NR_CS	Coarse sand (%) - Not recorded
	P10_NR_FS	Fine sand (%) - Not recorded
	P10_NR_Z	Silt (%) - Not recorded