Project Name:	LBV
	Project Code:	LBV	Site ID:	B9	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Site Information
	Desc. By:	R. Hare	Locality:
	Date Desc.:	12/10/48	Elevation:	 40 metres
	Map Ref.:	Sheet No. : 8358   1:100000	Rainfall:	800
	Northing/Long.:	147.216666666667	Runoff:	Slow
	Easting/Lat.:	-19.8777777777778	Drainage:	Imperfectly drained
	Geology
	ExposureType:	Soil pit	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	 Cza	Substrate Material:	Auger boring, 1 m deep,Unconsolidated 
	material (unidentified) 
	Land Form
	Rel/Slope Class: 	Level plain <9m <1%	Pattern Type:	Alluvial plain
	Morph. Type:	No Data	Relief:	No Data
	Elem. Type:	Plain	Slope Category:	No Data
	Slope:	0 % 	Aspect:	No Data
	Surface Soil Condition (dry):	Hardsetting
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Calcic Hypernatric Grey Sodosol     	Principal Profile Form:	Dy2.33
	ASC Confidence:	Great Soil Group:	Solonetz
	All necessary analytical data are available.
	Site Disturbance:	No effective disturbance other than grazing by hoofed animals
	Vegetation:	Low Strata - , , . *Species includes - Chloris species, Unknown species
	Mid Strata - Shrub, , Closed or dense. *Species includes - None recorded
	Tall Strata - Tree, 3.01-6m, Very sparse. *Species includes - Eremophila mitchellii
	Surface Coarse Fragments:	No surface coarse fragments
	Profile Morphology
	A1	0 - 0.03 m	Grey (10YR6/1-Moist); ; Clay loam; Weak grade of structure, 2-5 mm, Platy; Dry; Firm 
	consistence; Field pH 6.2 (pH meter); Sharp, Irregular change to - 
	B2	0.03 - 0.15 m	Greyish brown (2.5Y5/2-Moist); ; Medium clay; 50-100 mm, Prismatic; Moderate grade of 
	structure, 10-20 mm, Angular blocky; Dry; Strong consistence; Very few (0 - 2 %), 
	Manganiferous, Fine (0 - 2 mm), Nodules; Field pH 6.9 (pH meter); Diffuse change to - 
	B2	0.18 - 0.38 m	Greyish brown (2.5Y5/3-Moist); ; Light clay (Heavy); Moderate grade of structure, 5-10 mm, 
	Angular blocky; Moist; Firm consistence; Common (10 - 20 %), Calcareous, , Nodules; Field pH 
	9.2 (pH meter); Diffuse change to - 
	B3	0.38 - 0.61 m	Greyish brown (2.5Y5/3-Moist); ; Light clay; Moderate grade of structure, 5-10 mm, Angular 
	blocky; Moist; Weak consistence; Common (10 - 20 %), Calcareous, , Nodules; Field pH 9.1 (pH
	 meter); Diffuse change to - 
	B3	0.61 - 1.02 m	Yellowish brown (10YR5/4-Moist); ; Light clay; Moist; Weak consistence; Few (2 - 10 %), 
	Calcareous, , Nodules; Field pH 9.3 (pH meter); 
	Morphological Notes
	Observation Notes
	Site Notes
	BURDEKIN VALLE

	Project Name:	LBV
	Project Code:	LBV	Site ID:	B9	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.03	6.2H	 0.05B	 4.4K	 4.4	 0.56	 0.97	 5.4D	 15.7E
	0.03 - 0.15	6.9H	 0.1B	 3.2K	 6.4	 0.24	 3.4	 2.8D	 21E
	0.18 - 0.38	9.2H	 0.39B
	0.38 - 0.61	9.1H	 0.48B
	0.61 - 1.02	9.3H	 0.52B	 7.4K	 5.4	 0.22	 15.8	 28.8E
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.03	 21C	 0.022F	 0.11B	 3C	 44	 32	 21
	0.03 - 0.15	 0.013F	 2C	 38	 30	 30
	0.18 - 0.38	 0.66C
	0.38 - 0.61	 0.47C
	0.61 - 1.02	 1.41C	 4C	 27	 26	 41
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.03
	0.03 - 0.15
	0.18 - 0.38
	0.38 - 0.61
	0.61 - 1.02

	Project Name:	LBV
	Project Code:	LBV	Site ID:	B9	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Analyses Completed for this profile
	15_NR	Sum of Ex. cations + Ex. acidity - Not recorded
	15_NR_CA	Exch. basic cations (Ca++) - meq per 100g of soil - Not recorded
	15_NR_H	Hydrogen Cation - meq per 100g of soil - Not recorded
	15_NR_K	Exch. basic cations (K++) - meq per 100g of soil - Not recorded
	15_NR_MG	Exch. basic cations (Mg++) - meq per 100g of soil - Not recorded
	15_NR_NA	Exch. basic cations (Na++) - meq per 100g of soil - Not recorded
	19B_NR	Calcium Carbonate (CaCO3) - Not recorded
	2_LOI	Loss on Ignition (%)
	2A1	Air-dry moisture content
	3_NR	Electrical conductivity or soluble salts - Not recorded
	4_NR	pH of soil - Not recorded
	5_NR	Water soluble Chloride - Cl(%) - Not recordede
	7_NR	Total nitrogen (%) - Not recorded
	9_NR	Available P (mg/kg) - Not recorded
	9A_NR	Total element - P(%) - Not recorded
	P10_NR_C	Clay (%) - Not recorded
	P10_NR_CS	Coarse sand (%) - Not recorded
	P10_NR_FS	Fine sand (%) - Not recorded
	P10_NR_Z	Silt (%) - Not recorded