Project Name:	LOC
	Project Code:	LOC	Site ID:	B946	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Site Information
	Desc. By:	K.J. Smith	Locality:	Forest Hill-Laidley northern connection road,200m 
	SE of Forest Hill-Fernvale intersection.
	Date Desc.:	//	Elevation:	No Data
	Map Ref.:	Sheet No. : 9342   1:100000	Rainfall:	0
	Northing/Long.:	Runoff:	No Data
	Easting/Lat.:	Drainage:	Imperfectly drained
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	Undulating rises 9-30m 3-10%	Pattern Type:	Low hills
	Morph. Type:	No Data	Relief:	No Data
	Elem. Type:	No Data	Slope Category:	No Data
	Slope:	 % 	Aspect:	No Data
	Surface Soil Condition (dry):
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	 N/A    	Principal Profile Form:	Dy2.43
	ASC Confidence:	Great Soil Group:	Solodized solonetz
	Confidence level not specified
	Site Disturbance:
	Vegetation:
	Surface Coarse Fragments:
	Profile Morphology
	A1	0 - 0.07 m	Dark brown (7.5YR3/2-Moist); ; Fine sandy loam; Moderate grade of structure, 5-10 mm, Granular;
	 Dry; Very weak consistence; AbundantClear change to - 
	A2	0.07 - 0.23 m	Brown (10YR5/3-Moist); Light grey (10YR7/2-Dry); ; Sand; Massive grade of structure; Dry; Strong
	 consistence; FewAbrupt change to - 
	B21	0.23 - 0.48 m	Yellowish brown (10YR5/5-Moist); ; Medium heavy clay; Strong grade of structure, 20-50 mm, 
	Angular blocky; Dry; Strong consistence; FewDiffuse change to - 
	B22	0.48 - 0.74 m	Brownish yellow (10YR6/6-Moist); ; Medium clay; Strong grade of structure, 20-50 mm, Angular 
	blocky; Dry; Strong consistence; FewDiffuse change to - 
	BC	0.74 - 1.06 m	Very pale brown (10YR7/4-Moist); ; Light medium clay; Moderate grade of structure, 20-50 mm, 
	Angular blocky; Dry; Strong consistence; FewGradual change to - 
	C	1.06 - 1.16 m	; 
	Morphological Notes
	C	Weathered white & pale yellow calcareous sandstone.
	Observation Notes
	WAS LV237:                                                                                                              
	Site Notes
	LOCKYER

	Project Name:	LOC
	Project Code:	LOC	Site ID:	B946	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.08	5.9A	 0.1A	 4.6J	 3.8	 1	 0.24	 9.4F	2.55
	0.08 - 0.38	5.9A	 0.04A	 1.5J	 1.2	 0.52	 0.13	 3.1F	4.19
	0.23 - 0.48	6.7A	 0.14A	 4.1J	 14.7	 2	 1	 19.8F	5.05
	0.38 - 0.9	8.3A	 0.24A	 3.6J	 14.6	 0.34	 3.9	 18.8F	20.74
	0.74 - 1.06	9.6A	 0.54A	 11.4J	 12.3	 0.16	 4.1	 16.7F	24.55
	1.4 - 1.5	9.2A	 0.18A	 2.4J	 9.1	 0.14	 3.9	 13.5F	28.89
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.08	 2.83A	 0.084A	 0.78A	 46D	 30	 8	 11
	0.08 - 0.38	 0.8A	 0.059A	 0.72A	 54D	 23	 11	 8
	0.23 - 0.48	 0.65A	 0.023A	 0.81A	 29D	 16	 7	 44
	0.38 - 0.9	 0.017A	 1.2A	 33D	 19	 11	 36
	0.74 - 1.06	 0.047A	 1.68A	 34D	 17	 13	 24
	1.4 - 1.5	 0.052A	 1.88A	 46D	 20	 16	 15
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.08
	0.08 - 0.38
	0.23 - 0.48
	0.38 - 0.9
	0.74 - 1.06
	1.4 - 1.5

	Project Name:	LOC
	Project Code:	LOC	Site ID:	B946	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Analyses Completed for this profile
	10A1	Total sulfur - X-ray fluorescence
	12_XRF_CU	Total element - Cu(mg/kg) - X-Ray Fuoresence
	12_XRF_ZN	Total element - Zn(mg/kg) - X-Ray Fuoresence
	15F1_CA	Exchangeable bases by 0.01M silver-thiourea (AgTU)+, no pretreatment for soluble salts
	15F1_CEC	Exchangeable bases by 0.01m (AgTU)+, no pretreatment for soluble salts
	15F1_K	Exchangeable bases by 0.01m (AgTU)+, no pretreatment for soluble salts
	15F1_MG	Exchangeable bases by 0.01m (AgTU)+, no pretreatment for soluble salts
	15F1_NA	Exchangeable bases by 0.01m (AgTU)+, no pretreatment for soluble salts
	17A1	Total potassium - X-ray fluorescence
	3A1	EC of 1:5 soil/water extract
	4A1	pH of 1:5 soil/water suspension
	5A2	Chloride - 1:5 soil/water extract, automated colour
	6A1	Organic carbon - Walkley and Black
	9A1	Total phosphorus - X-ray fluorescence
	MIN_EC	Exchange Capacity - Minerology
	MIN_NR_K2O	Kaolin minerals
	P10_PB_C	Clay (%) - Plummet balance
	P10_PB_CS	Coarse sand (%) - Plummet balance
	P10_PB_FS	Fine sand (%) - Plummet balance
	P10_PB_Z	Silt (%) - Plummet balance
	XRD_C_Il	Illite - X-Ray Diffraction
	XRD_C_Ka	Kaolin - X-Ray Diffraction
	XRD_C_Qz	Quartz - X-Ray Diffraction
	XRD_C_St	Smectite - X-Ray Diffraction