Project Name:	LOC
	Project Code:	LOC	Site ID:	B971	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Site Information
	Desc. By:	K.J. Smith	Locality:
	Date Desc.:	//	Elevation:	No Data
	Map Ref.:	Sheet No. : 9342   1:100000	Rainfall:	0
	Northing/Long.:	Runoff:	No Data
	Easting/Lat.:	Drainage:	Moderately well drained
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	Unconsolidated material (unidentified) 
	Land Form
	Rel/Slope Class: 	No Data	Pattern Type:	Pediment
	Morph. Type:	No Data	Relief:	No Data
	Elem. Type:	No Data	Slope Category:	No Data
	Slope:	0 % 	Aspect:	No Data
	Surface Soil Condition (dry):
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	 N/A    	Principal Profile Form:	Ug5.16
	ASC Confidence:	Great Soil Group:	Grey clay
	Confidence level not specified
	Site Disturbance:
	Vegetation:
	Surface Coarse Fragments:
	Profile Morphology
	A1	0 - 0.04 m	Very dark grey (10YR3/1-Moist); ; Light clay; Moderate grade of structure, 5-10 mm, Subangular 
	blocky; Moist; Very weak consistence; Clear change to - 
	B1	0.04 - 0.2 m	Very dark grey (10YR3/1-Moist); ; Light clay; Moderate grade of structure, 20-50 mm, Angular 
	blocky; Moist; Weak consistence; Gradual change to - 
	B21	0.2 - 0.6 m	Dark greyish brown (10YR4/2-Moist); ; Medium clay; Strong grade of structure, Angular blocky; 
	Moist; Firm consistence; Diffuse change to - 
	B22	0.6 - 1.1 m	Yellowish brown (10YR5/4-Moist); ; Medium heavy clay; Moderate grade of structure, Subangular
	 blocky; Moderately moist; Firm consistence; 
	Morphological Notes
	Observation Notes
	WAS LV344:                                                                                                              
	Site Notes
	LOCKYER

	Project Name:	LOC
	Project Code:	LOC	Site ID:	B971	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.1	5.2A	 0.053A	 8J	 4.3	 0.66	 0.1	 16.3F	0.61
	0.04 - 0.2	6.2A	 0.053A	 10.6J	 6.1	 0.28	 0.63	 21.4F	2.94
	0.4 - 0.5	8.3A	 0.4A	 10.2J	 11.3	 0.13	 5.5	 27.6F	19.93
	0.9 - 1	5.7A	 0.64A	 5.9J	 13.8	 0.14	 9.3	 27.3F	34.07
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.1	 3.33A	 79B
	0.04 - 0.2	 2.05A	 21B
	0.4 - 0.5
	0.9 - 1
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.1
	0.04 - 0.2
	0.4 - 0.5
	0.9 - 1

	Project Name:	LOC
	Project Code:	LOC	Site ID:	B971	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Analyses Completed for this profile
	15F1_CA	Exchangeable bases by 0.01M silver-thiourea (AgTU)+, no pretreatment for soluble salts
	15F1_CEC	Exchangeable bases by 0.01m (AgTU)+, no pretreatment for soluble salts
	15F1_K	Exchangeable bases by 0.01m (AgTU)+, no pretreatment for soluble salts
	15F1_MG	Exchangeable bases by 0.01m (AgTU)+, no pretreatment for soluble salts
	15F1_NA	Exchangeable bases by 0.01m (AgTU)+, no pretreatment for soluble salts
	3A1	EC of 1:5 soil/water extract
	4A1	pH of 1:5 soil/water suspension
	6A1	Organic carbon - Walkley and Black
	9G_BSES	Available P (mg/kg) - Acid P - 0.005M H2SO4 (BSES)