Project Name:	NAR
	Project Code:	NAR	Site ID:	B579	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Site Information
	Desc. By:	G.D. Hubble	Locality:	Narayen Research Station.
	Date Desc.:	14/08/69	Elevation:	 290 metres
	Map Ref.:	Sheet No. : 9046   1:100000	Rainfall:	712
	Northing/Long.:	150.883333333333	Runoff:	Moderately rapid
	Easting/Lat.:	-25.6833333333333	Drainage:	Moderately well drained
	Geology
	ExposureType:	Soil pit	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	 PRt	Substrate Material:	Undisturbed soil core, 0.7 m 
	deep,Adamellite 
	Land Form
	Rel/Slope Class: 	Undulating rises 9-30m 3-10%	Pattern Type:	Low hills
	Morph. Type:	Mid-slope	Relief:	24 metres
	Elem. Type:	Hillslope	Slope Category:	No Data
	Slope:	5.6 % 	Aspect:	No Data
	Surface Soil Condition (dry):	Hardsetting
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Bleached Eutrophic Brown Chromosol     	Principal Profile Form:	Dy2.42
	ASC Confidence:	Great Soil Group:	Yellow podzolic soil
	All necessary analytical data are available.
	Site Disturbance:	No effective disturbance other than grazing by hoofed animals
	Vegetation:	Low Strata - Tussock grass, , . *Species includes - Aristida species
	Tall Strata - Tree, 6.01-12m, Sparse. *Species includes - Eucalyptus crebra, Eucalyptus polycarpa
	Surface Coarse Fragments:	No surface coarse fragments
	Profile Morphology
	A1	0 - 0.05 m	Very dark greyish brown (10YR3/2-Moist); ; Coarse sandy loam (Light); Massive grade of 
	structure; Dry; Weak consistence; 10-20%, fine gravelly, 2-6mm, Quartz, coarse fragments; Field
	 pH 6.5 (pH meter); Common, fine (1-2mm) roots; Clear change to - 
	A21	0.05 - 0.1 m	Brown (10YR4/3-Moist); ; Loamy coarse sand; Massive grade of structure; Dry; Weak 
	consistence; 20-50%, fine gravelly, 2-6mm, Quartz, coarse fragments; Field pH 6 (pH meter); 
	Common, fine (1-2mm) roots; Clear change to - 
	A21	0.1 - 0.2 m	Brown (10YR4/3-Moist); ; Clayey coarse sand; Massive grade of structure; Dry; Weak 
	consistence; 20-50%, medium gravelly, 6-20mm, Quartz, coarse fragments; Field pH 6 (pH 
	meter); Common, fine (1-2mm) roots; Gradual change to - 
	A22	0.2 - 0.3 m	Light yellowish brown (10YR6/4-Moist); ; Clayey coarse sand; Massive grade of structure; Dry; 
	Very weak consistence; 20-50%, medium gravelly, 6-20mm, Substrate material, coarse 
	fragments; Field pH 6 (pH meter); Few, fine (1-2mm) roots; Gradual change to - 
	A22	0.3 - 0.38 m	Light yellowish brown (10YR6/4-Moist); ; Clayey coarse sand; Massive grade of structure; Dry; 
	Very weak consistence; 20-50%, medium gravelly, 6-20mm, Substrate material, coarse 
	fragments; Field pH 7 (pH meter); Few, fine (1-2mm) roots; Clear change to - 
	B1	0.38 - 0.4 m	Yellowish brown (10YR5/8-Moist); ; Coarse sandy clay loam; Weak grade of structure, 10-20 
	mm, Angular blocky; Dry; Very firm consistence; 20-50%, medium gravelly, 6-20mm, Substrate 
	material, coarse fragments; Field pH 7 (pH meter); Few, fine (1-2mm) roots; Sharp change to - 
	B2	0.4 - 0.6 m	Yellowish brown (10YR5/8-Moist); ; Medium clay; Moderate grade of structure, 20-50 mm, 
	Angular blocky; Moderately moist; Strong consistence; 20-50%, medium gravelly, 6-20mm, 
	Substrate material, coarse fragments; Field pH 7 (pH meter); Few, fine (1-2mm) roots; Gradual 
	change to - 
	B3	0.6 - 0.7 m	Yellowish brown (10YR5/8-Moist); , 10YR52, 20-50% , 0-5mm, Prominent; , 7.5YR58, 20-50% , 
	0-5mm, Prominent; Medium clay; Weak grade of structure, 20-50 mm; Moderately moist; Strong 
	consistence; 20-50%, medium gravelly, 6-20mm, Substrate material, coarse fragments; Field 
	pH 7 (pH meter); Few, fine (1-2mm) roots; Gradual change to - 

	Project Name:	NAR
	Project Code:	NAR	Site ID:	B579	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	C	0.7 - 0.9 m	Strong brown (7.5YR5/8-Moist); , 10YR52, 20-50% , 0-5mm, Prominent; , 20-50% , 0-5mm, 
	Prominent; Coarse sandy medium clay; Massive grade of structure; Moderately moist; Strong 
	consistence; 20-50%, medium gravelly, 6-20mm, Substrate material, coarse fragments; Field 
	pH 7 (pH meter); 
	Morphological Notes
	Observation Notes
	2-6MM QUARTZ GRIT PRESENT THROUGHOUT:TEXTURES OF 20-40CM HORIZONS ARE GRAVELLY DOMINANT 
	FELDSPAR TO 25MM:ALL OTHER      TEXTURES ARE GRITTY, DOMINANTLY 2-6MM QUARTZ:
	Site Notes
	MUNDUBERRA

	Project Name:	NAR
	Project Code:	NAR	Site ID:	B579	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.05	6.2H	 0.02B	 3.9K	 1.8	 0.54	 0.09	 3.6D
	0.05 - 0.1	5.7H	 0.008B	 0.95K	 0.86	 0.24	 0.07	 2.5D
	0.1 - 0.2	5.3H	 0.008B
	0.2 - 0.3	5.5H	 0.009B	 0.61K	 0.76	 0.11	 0.05	 1.7D
	0.3 - 0.38	6.2H	 0.01B
	0.38 - 0.4	6.4H	 0.014B	 3K	 4.1	 0.18	 0.17	 2D
	0.4 - 0.6	6.7H	 0.014B	 4.7K	 7.1	 0.25	 0.5	 2.8D
	0.6 - 0.7	6.7H	 0.014B	 5K	 9.2	 0.3	 0.56	 2.6D
	0.7 - 0.9	7.1H	 0.02B
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.05	 1.93E	 23B	 0.022F	 0.111B	 3.2B	 17	 51C	 31	 7	 7
	0.05 - 0.1	 0.53E	 4B	 0.013F	 0.04B	 3.2B	 23	 51C	 33	 7	 7
	0.1 - 0.2	 0.36E	 0.01F	 0.03B	 3.2B	 31	 51C	 36	 6	 7
	0.2 - 0.3	 0.21E	 2B	 0.007F	 0.021B	 3.5B	 40	 59C	 29	 5	 6
	0.3 - 0.38	 0.19E	 0.011F	 0.025B	 3.6B	 44	 55C	 28	 8	 8
	0.38 - 0.4	 0.35E	 0.017F	 0.044B	 3.2B	 37	 43C	 24	 8	 25
	0.4 - 0.6	 0.39E	 5B	 0.02F	 0.045B	 2.4B	 28	 33C	 20	 9	 40
	0.6 - 0.7	 0.43E	 0.017F	 0.049B	 1.95B	 28	 35C	 17	 10	 37
	0.7 - 0.9	 0.2E	 0.014F	 0.025B	 2.05B	 44	 53C	 18	 7	 25
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.05
	0.05 - 0.1
	0.1 - 0.2
	0.2 - 0.3
	0.3 - 0.38
	0.38 - 0.4
	0.4 - 0.6
	0.6 - 0.7
	0.7 - 0.9

	Project Name:	NAR
	Project Code:	NAR	Site ID:	B579	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Analyses Completed for this profile
	10A_NR	Total element - S(%) - Not recorded
	15_NR_CA	Exch. basic cations (Ca++) - meq per 100g of soil - Not recorded
	15_NR_H	Hydrogen Cation - meq per 100g of soil - Not recorded
	15_NR_K	Exch. basic cations (K++) - meq per 100g of soil - Not recorded
	15_NR_MG	Exch. basic cations (Mg++) - meq per 100g of soil - Not recorded
	15_NR_NA	Exch. basic cations (Na++) - meq per 100g of soil - Not recorded
	17A_NR	Total element - K(%) - Not recorded
	3_NR	Electrical conductivity or soluble salts - Not recorded
	4_NR	pH of soil - Not recorded
	5_NR	Water soluble Chloride - Cl(%) - Not recordede
	6Z	Organic carbon (%) - Not recorded
	7_NR	Total nitrogen (%) - Not recorded
	9A_NR	Total element - P(%) - Not recorded
	9G_BSES	Available P (mg/kg) - Acid P - 0.005M H2SO4 (BSES)
	P10_GRAV	Gravel (%)
	P10_NR_C	Clay (%) - Not recorded
	P10_NR_CS	Coarse sand (%) - Not recorded
	P10_NR_FS	Fine sand (%) - Not recorded
	P10_NR_Z	Silt (%) - Not recorded