Project Name:	NAR
	Project Code:	NAR	Site ID:	B725	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Site Information
	Desc. By:	G.D. Hubble	Locality:
	Date Desc.:	10/05/71	Elevation:	 240 metres
	Map Ref.:	Sheet No. : 9046   1:100000	Rainfall:	716
	Northing/Long.:	150.902777777778	Runoff:	No Data
	Easting/Lat.:	-25.7041666666667	Drainage:	No Data
	Geology
	ExposureType:	Auger boring	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	 PRt	Substrate Material:	Auger boring, 1 m deep,Adamellite 
	Land Form
	Rel/Slope Class: 	Undulating rises 9-30m 3-10%	Pattern Type:	No Data
	Morph. Type:	Upper-slope	Relief:	No Data
	Elem. Type:	Hillslope	Slope Category:	No Data
	Slope:	4.4 % 	Aspect:	No Data
	Surface Soil Condition (dry):	Hardsetting
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Eutrophic Mottled-Mesonatric Brown Sodosol     	Principal Profile Form:	Dy3.42
	ASC Confidence:	Great Soil Group:	Solodic soil
	All necessary analytical data are available.
	Site Disturbance:	No effective disturbance other than grazing by hoofed animals
	Vegetation:	Low Strata - Tussock grass, , . *Species includes - Heteropogon contortus
	Tall Strata - Tree, 6.01-12m, Sparse. *Species includes - None Recorded
	Surface Coarse Fragments:
	Profile Morphology
	A1	0 - 0.1 m	Very dark greyish brown (10YR3/2-Moist); ; Sandy loam; Massive grade of structure; Dry; Firm 
	consistence; 10-20%, medium gravelly, 6-20mm, angular, Gravel, coarse fragments; Field pH 6 
	(pH meter); Many, very fine (0-1mm) roots; Gradual change to - 
	A2	0.1 - 0.34 m	Pale brown (10YR6/3-Moist); ; Coarse sand; Massive grade of structure; Dry; Weak consistence;
	 10-20%, medium gravelly, 6-20mm, angular, Gravel, coarse fragments; Field pH 6.5 (pH meter); 
	Common, very fine (0-1mm) roots; Abrupt change to - 
	B21	0.34 - 0.7 m	Strong brown (7.5YR5/6-Moist); , 10YR52, 10-20% , 0-5mm, Distinct; , 10YR63, 10-20% , 0-
	5mm, Distinct; Sandy medium clay; Weak grade of structure, 20-50 mm, Prismatic; , Angular 
	blocky; Dry; Very firm consistence; 10-20%, medium gravelly, 6-20mm, angular, Gravel, coarse 
	fragments; Field pH 6.5 (pH meter); Few, very fine (0-1mm) roots; Gradual change to - 
	B22	0.7 - 1 m	Strong brown (7.5YR5/8-Moist); , 7.5YR66, 20-50% , 5-15mm, Distinct; , 10YR62, 20-50% , 5-
	15mm, Distinct; Light clay; Weak grade of structure, 20-50 mm, Polyhedral; Dry; Strong 
	consistence; 10-20%, medium gravelly, 6-20mm, angular, Gravel, coarse fragments; Field pH 8 
	(pH meter); Few, very fine (0-1mm) roots; Gradual change to - 
	D	1 - 1.2 m	Pale yellow (2.5Y7/3-Moist); , 10YR62, 20-50% , 5-15mm, Distinct; , 10YR66, 20-50% , 5-15mm,
	 Distinct; Medium clay; Weak grade of structure, 20-50 mm, Polyhedral; Dry; Very firm 
	consistence; 10-20%, medium gravelly, 6-20mm, angular, Gravel, coarse fragments; Field pH 
	7.5 (pH meter); Few, very fine (0-1mm) roots; Gradual change to - 
	D	1.2 - 2 m	Strong brown (7.5YR5/6-Moist); , 10YR62, 20-50% , 15-30mm, Prominent; , 2.5Y83, 20-50% , 15-
	30mm, Prominent; Coarse sandy clay loam; Massive grade of structure; Moderately moist; Firm 
	consistence; 10-20%, medium gravelly, 6-20mm, angular, Gravel, coarse fragments; Field pH 
	6.5 (pH meter); 
	Morphological Notes
	Observation Notes
	ADAMELLITE FINE GRAINED DIFFERENTIATE. STRONG WEATHERING MINERAL SPECK LING BELOW 80CM. GRAVELS 
	VARYING FELDSPAR AND    QUARTZ DOMINANT.
	Site Notes
	NARAYEN

	Project Name:	NAR
	Project Code:	NAR	Site ID:	B725	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)

	Project Name:	NAR
	Project Code:	NAR	Site ID:	B725	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.1	5.8H	<0.01B	 1.9K	 0.7	 0.021	 0.02	 2.6D
	0.1 - 0.34
	0.34 - 0.7	6.7H	 0.02B	 3.3K	 10.6	 0.26	 2.8	 2.5D
	0.7 - 1
	1 - 1.2
	1.2 - 2
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.1	 1.16A	 8B	 160F	 0.06B	 3.7B	 13	 65C	 24	 6	 4
	0.1 - 0.34
	0.34 - 0.7	 160F	 2.8B	 4	 41C	 15	 7	 39
	0.7 - 1
	1 - 1.2
	1.2 - 2
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.1
	0.1 - 0.34
	0.34 - 0.7
	0.7 - 1
	1 - 1.2
	1.2 - 2

	Project Name:	NAR
	Project Code:	NAR	Site ID:	B725	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Analyses Completed for this profile
	10A_NR	Total element - S(%) - Not recorded
	15_NR_CA	Exch. basic cations (Ca++) - meq per 100g of soil - Not recorded
	15_NR_H	Hydrogen Cation - meq per 100g of soil - Not recorded
	15_NR_K	Exch. basic cations (K++) - meq per 100g of soil - Not recorded
	15_NR_MG	Exch. basic cations (Mg++) - meq per 100g of soil - Not recorded
	15_NR_NA	Exch. basic cations (Na++) - meq per 100g of soil - Not recorded
	17A_NR	Total element - K(%) - Not recorded
	2A1	Air-dry moisture content
	3_NR	Electrical conductivity or soluble salts - Not recorded
	4_NR	pH of soil - Not recorded
	5_NR	Water soluble Chloride - Cl(%) - Not recordede
	6A1	Organic carbon - Walkley and Black
	7_NR	Total nitrogen (%) - Not recorded
	9A_NR	Total element - P(%) - Not recorded
	9G_BSES	Available P (mg/kg) - Acid P - 0.005M H2SO4 (BSES)
	P10_GRAV	Gravel (%)
	P10_NR_C	Clay (%) - Not recorded
	P10_NR_CS	Coarse sand (%) - Not recorded
	P10_NR_FS	Fine sand (%) - Not recorded
	P10_NR_Z	Silt (%) - Not recorded